Copyright (c) 2003-2013 The DragonFly Project.
Copyright (c) 1992-2003 The FreeBSD Project.
Copyright (c) 1979, 1980, 1983, 1986, 1988, 1989, 1991, 1992, 1993, 1994
	The Regents of the University of California. All rights reserved.
Slab ZoneSize set to 128KB
Leaving critical section, allowing interrupts
ACPI SDT: RSDP not in EBDA
ACPI SDT: RSDP in BIOS mem
ACPI FADT: SCI irq 9, conform/conform
DragonFly v3.6.1-RELEASE #9: Thu Feb 20 21:39:35 PST 2014
    root@pkgbox64.dragonflybsd.org:/usr/obj/build/home/justin/src/sys/X86_64_GENERIC
Calibrating clock(s) ...
TSC clock: 2255422572 Hz, i8254 clock: 1193228 Hz
CLK_USE_I8254_CALIBRATION not specified - using default frequency
CLK_USE_TSC_CALIBRATION not specified - using old calibration method
CPU: Intel(R) Core(TM)2 Duo CPU     P7550  @ 2.26GHz (2255.36-MHz K8-class CPU)
  Origin = "GenuineIntel"  Id = 0x1067a  Stepping = 10
  Features=0xbfebfbff<FPU,VME,DE,PSE,TSC,MSR,PAE,MCE,CX8,APIC,SEP,MTRR,PGE,MCA,CMOV,PAT,PSE36,CLFLUSH,DTS,ACPI,MMX,FXSR,SSE,SSE2,SS,HTT,TM,PBE>
  Features2=0x408e3bd<SSE3,DTES64,MON,DS_CPL,VMX,EST,TM2,SSSE3,CX16,xTPR,PDCM,SSE4.1,XSAVE>
  AMD Features=0x20100800<SYSCALL,NX,LM>
  AMD Features2=0x1<LAHF>
real memory  = 8295066624 (7910 MB)
Physical memory chunk(s):
0x00020000 - 0x0007ffff, 393216 bytes (96 pages)
0x00100000 - 0x001fffff, 1048576 bytes (256 pages)
0x01ce0000 - 0xae71ffff, 2896429056 bytes (707136 pages)
0x100000000 - 0x23ffdffff, 5368578048 bytes (1310688 pages)
avail memory = 7719841792 (7362 MB)
ACPI MADT: LAPIC address 0xfee00000, flags 0x1
ACPI MADT: BSP apic id 0
ACPI MADT: cpu id 0, apic id 0
ACPI MADT: cpu id 1, apic id 1
lapic: divisor index 0, frequency 132667347 Hz
SMP: CPU0 apic_initialize():
     lint0: 0x00010700 lint1: 0x00000400 TPR: 0x00000000 SVR: 0x000001ff
SMP: Waiting APs LAPIC initialization
SMP: CPU1 apic_initialize():
     lint0: 0x00010000 lint1: 0x00010400 TPR: 0x00000000 SVR: 0x000001ff
ACPI MADT: warning invalid intsrc irq 9 trig, level
ACPI MADT: IOAPIC addr 0xfec00000, apic id 1, gsi base 0
ACPI MADT: INTSRC irq 0 -> gsi 2 edge/high
ACPI MADT: SCI irq 9, first test level/high
IOAPIC: idx 0, apic id 2, gsi base 0, npin 24
IOAPIC: irq 1, gsi 1 -> cpu0 (fixed)
IOAPIC: irq 1 -> gsi 1 edge/high
IOAPIC: irq 0, gsi 2 -> cpu0 (0)
IOAPIC: irq 0 -> gsi 2 edge/high
IOAPIC: irq 3, gsi 3 -> cpu0 (fixed)
IOAPIC: irq 3 -> gsi 3 edge/high
IOAPIC: irq 4, gsi 4 -> cpu0 (fixed)
IOAPIC: irq 4 -> gsi 4 edge/high
IOAPIC: irq 5, gsi 5 -> cpu0 (fixed)
IOAPIC: irq 5 -> gsi 5 edge/high
IOAPIC: irq 6, gsi 6 -> cpu0 (fixed)
IOAPIC: irq 6 -> gsi 6 edge/high
IOAPIC: irq 7, gsi 7 -> cpu0 (fixed)
IOAPIC: irq 7 -> gsi 7 edge/high
IOAPIC: irq 8, gsi 8 -> cpu0 (fixed)
IOAPIC: irq 8 -> gsi 8 edge/high
IOAPIC: irq 9, gsi 9 -> cpu0 (sci)
IOAPIC: irq 9 -> gsi 9 edge/high
IOAPIC: irq 10, gsi 10 -> cpu0 (fixed)
IOAPIC: irq 10 -> gsi 10 edge/high
IOAPIC: irq 11, gsi 11 -> cpu0 (fixed)
IOAPIC: irq 11 -> gsi 11 edge/high
IOAPIC: irq 12, gsi 12 -> cpu0 (fixed)
IOAPIC: irq 12 -> gsi 12 edge/high
IOAPIC: irq 13, gsi 13 -> cpu0 (fixed)
IOAPIC: irq 13 -> gsi 13 edge/high
IOAPIC: irq 14, gsi 14 -> cpu0 (fixed)
IOAPIC: irq 14 -> gsi 14 edge/high
IOAPIC: irq 15, gsi 15 -> cpu0 (fixed)
IOAPIC: irq 15 -> gsi 15 edge/high
IOAPIC: irq 16, gsi 16 -> cpu0 (fixed)
IOAPIC: irq 16 -> gsi 16 level/low
IOAPIC: irq 17, gsi 17 -> cpu0 (fixed)
IOAPIC: irq 17 -> gsi 17 level/low
IOAPIC: irq 18, gsi 18 -> cpu0 (fixed)
IOAPIC: irq 18 -> gsi 18 level/low
IOAPIC: irq 19, gsi 19 -> cpu0 (fixed)
IOAPIC: irq 19 -> gsi 19 level/low
IOAPIC: irq 20, gsi 20 -> cpu0 (fixed)
IOAPIC: irq 20 -> gsi 20 level/low
IOAPIC: irq 21, gsi 21 -> cpu0 (fixed)
IOAPIC: irq 21 -> gsi 21 level/low
IOAPIC: irq 22, gsi 22 -> cpu0 (fixed)
IOAPIC: irq 22 -> gsi 22 level/low
IOAPIC: irq 23, gsi 23 -> cpu0 (fixed)
IOAPIC: irq 23 -> gsi 23 level/low
IOAPIC: cpu0 irq 2 reserved
IOAPIC: cpu1 irq 0 reserved
IOAPIC: cpu1 irq 1 reserved
IOAPIC: cpu1 irq 2 reserved
IOAPIC: cpu1 irq 3 reserved
IOAPIC: cpu1 irq 4 reserved
IOAPIC: cpu1 irq 5 reserved
IOAPIC: cpu1 irq 6 reserved
IOAPIC: cpu1 irq 7 reserved
IOAPIC: cpu1 irq 8 reserved
IOAPIC: cpu1 irq 9 reserved
IOAPIC: cpu1 irq 10 reserved
IOAPIC: cpu1 irq 11 reserved
IOAPIC: cpu1 irq 12 reserved
IOAPIC: cpu1 irq 13 reserved
IOAPIC: cpu1 irq 14 reserved
IOAPIC: cpu1 irq 15 reserved
IOAPIC: legacy irq max 24
ELCR Found.  ISA IRQs programmed as:
  0  1  2  3  4  5  6  7  8  9 10 11 12 13 14 15
  E  E  E  E  E  L  E  L  E  E  L  L  E  E  L  L
Initialize MI interrupts
objcache: magazine cap [6, 134]
Finish MP startup
Active CPU Mask: 0000000000000003
Preloaded elf kernel "/kernel/kernel" at 0xffffffff81698000.
Bits within APICID: logical_CPU_bits: 0; core_bits: 1
CPU Topology: cores_per_chip: 2; threads_per_core: 1; chips_per_package: 1;
VMM: VMENTRY_LOAD_IA32_EFER not supported by this CPU
Start scheduler helpers on cpus:
	cpu0 - No HT available, multi-core/physical cpu. Physical siblings: cpu0 cpu1 
	cpu1 - No HT available, multi-core/physical cpu. Physical siblings: cpu0 cpu1 
start dummy scheduler helpers on cpus: 0 1
Start scheduler helpers on cpus:
	cpu0 - No HT available, multi-core/physical cpu. Physical siblings: cpu0 cpu1 
	cpu1 - No HT available, multi-core/physical cpu. Physical siblings: cpu0 cpu1 
FQ scheduler policy version 1.1 loaded
wdog: In-kernel automatic watchdog reset enabled
wlan: <802.11 Link Layer>
ath_rate: <SampleRate bit-rate selection algorithm>
No policy for md0 specified, or policy not found
disk scheduler: set policy of md0 to noop
md0: Malloc disk
kbd0 at kbdmux0
crypto: <crypto core>
md0: invalid primary partition table: no magic
hptrr: RocketRAID 17xx/2xxx SATA controller driver v1.2
hpt27xx: RocketRAID 27xx controller driver v1.0 (Feb 20 2014 21:39:07)
IOAPIC: rman cpu0 0 - 1
IOAPIC: rman cpu0 3 - 95
IOAPIC: rman cpu0 97 - 191
IOAPIC: rman cpu1 16 - 95
IOAPIC: rman cpu1 97 - 191
cryptosoft0.nexus0.root0
cryptosoft0: <software crypto> [tentative] on motherboard
crypto: assign cryptosoft0 driver id 0, flags 234881024
crypto: cryptosoft0 registers alg 1 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 2 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 3 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 4 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 5 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 16 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 6 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 7 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 18 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 19 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 20 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 8 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 15 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 9 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 10 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 13 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 14 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 11 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 22 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 23 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 24 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 28 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 25 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 26 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 27 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 21 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 29 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 30 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 31 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 32 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 17 flags 0 maxoplen 0
cryptosoft0: <software crypto> [attached!] on motherboard
pcib0.legacy0.nexus0.root0
pcib0: <MPTABLE Host-PCI bridge> [tentative] pcibus 0 on motherboard
pci0.pcib0.legacy0.nexus0.root0
pci0: <PCI bus> [tentative] on pcib0
pci0: domain=0, physical bus=0
found->	vendor=0x10de, dev=0x0a82, revid=0xb1
	domain=0, bus=0, slot=0, func=0
	class=06-00-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0006, statreg=0x00a0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
found->	vendor=0x10de, dev=0x0a88, revid=0xb1
	domain=0, bus=0, slot=0, func=1
	class=05-00-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0004, statreg=0x00a0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
found->	vendor=0x10de, dev=0x0aae, revid=0xb3
	domain=0, bus=0, slot=3, func=0
	class=06-01-00, hdrtype=0x00, mfdev=1
	cmdreg=0x000f, statreg=0x00a0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	map[10]: type I/O Port, range 32, base 0x2000, size  8, enabled
found->	vendor=0x10de, dev=0x0aa4, revid=0xb1
	domain=0, bus=0, slot=3, func=1
	class=05-00-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0400, statreg=0x00a0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
found->	vendor=0x10de, dev=0x0aa2, revid=0xb1
	domain=0, bus=0, slot=3, func=2
	class=0c-05-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0001, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=15
	powerspec 2  supports D0 D3  current D0
	map[10]: type I/O Port, range 32, base 0x2180, size  6, enabled
	map[20]: type I/O Port, range 32, base 0x2140, size  6, enabled
	map[24]: type I/O Port, range 32, base 0x2100, size  6, enabled
MPTABLE: fixed interrupt routing for 0:3 INTA
MPTABLE: 0:3 INTA routed to irq 15
IOAPIC: irq 15, gsi 15 edge/high -> level/low
found->	vendor=0x10de, dev=0x0a89, revid=0xb1
	domain=0, bus=0, slot=3, func=3
	class=05-00-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0000, statreg=0x0020, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
found->	vendor=0x10de, dev=0x0a98, revid=0xb1
	domain=0, bus=0, slot=3, func=4
	class=05-00-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0400, statreg=0x00a0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
found->	vendor=0x10de, dev=0x0aa3, revid=0xb1
	domain=0, bus=0, slot=3, func=5
	class=0b-40-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0006, statreg=0x00a0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x03 (750 ns), maxlat=0x01 (250 ns)
	intpin=b, irq=14
	map[10]: type Memory, range 32, base 0xd3400000, size 19, enabled
MPTABLE: fixed interrupt routing for 0:3 INTB
MPTABLE: 0:3 INTB routed to irq 14
IOAPIC: irq 14, gsi 14 edge/high -> level/low
found->	vendor=0x10de, dev=0x0aa5, revid=0xb1
	domain=0, bus=0, slot=4, func=0
	class=0c-03-10, hdrtype=0x00, mfdev=1
	cmdreg=0x0007, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x03 (750 ns), maxlat=0x01 (250 ns)
	intpin=a, irq=11
	powerspec 2  supports D0 D1 D2 D3  current D0
	map[10]: type Memory, range 32, base 0xd3488000, size 12, enabled
MPTABLE: fixed interrupt routing for 0:4 INTA
MPTABLE: 0:4 INTA routed to irq 11
IOAPIC: irq 11, gsi 11 edge/high -> level/low
found->	vendor=0x10de, dev=0x0aa6, revid=0xb1
	domain=0, bus=0, slot=4, func=1
	class=0c-03-20, hdrtype=0x00, mfdev=1
	cmdreg=0x0006, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x03 (750 ns), maxlat=0x01 (250 ns)
	intpin=b, irq=10
	powerspec 2  supports D0 D1 D2 D3  current D0
	map[10]: type Memory, range 32, base 0xd3489200, size  8, enabled
MPTABLE: fixed interrupt routing for 0:4 INTB
MPTABLE: 0:4 INTB routed to irq 10
IOAPIC: irq 10, gsi 10 edge/high -> level/low
found->	vendor=0x10de, dev=0x0aa7, revid=0xb1
	domain=0, bus=0, slot=6, func=0
	class=0c-03-10, hdrtype=0x00, mfdev=1
	cmdreg=0x0007, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x03 (750 ns), maxlat=0x01 (250 ns)
	intpin=a, irq=7
	powerspec 2  supports D0 D1 D2 D3  current D0
	map[10]: type Memory, range 32, base 0xd3487000, size 12, enabled
MPTABLE: fixed interrupt routing for 0:6 INTA
MPTABLE: 0:6 INTA routed to irq 7
IOAPIC: irq 7, gsi 7 edge/high -> level/low
found->	vendor=0x10de, dev=0x0aa9, revid=0xb1
	domain=0, bus=0, slot=6, func=1
	class=0c-03-20, hdrtype=0x00, mfdev=1
	cmdreg=0x0006, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x03 (750 ns), maxlat=0x01 (250 ns)
	intpin=b, irq=5
	powerspec 2  supports D0 D1 D2 D3  current D0
	map[10]: type Memory, range 32, base 0xd3489100, size  8, enabled
MPTABLE: fixed interrupt routing for 0:6 INTB
MPTABLE: 0:6 INTB routed to irq 5
IOAPIC: irq 5, gsi 5 edge/high -> level/low
found->	vendor=0x10de, dev=0x0ac0, revid=0xb1
	domain=0, bus=0, slot=8, func=0
	class=04-03-00, hdrtype=0x00, mfdev=0
	cmdreg=0x0006, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x02 (500 ns), maxlat=0x05 (1250 ns)
	intpin=a, irq=15
	powerspec 2  supports D0 D3  current D0
	map[10]: type Memory, range 32, base 0xd3480000, size 14, enabled
MPTABLE: fixed interrupt routing for 0:8 INTA
MPTABLE: 0:8 INTA routed to irq 15
found->	vendor=0x10de, dev=0x0aab, revid=0xb1
	domain=0, bus=0, slot=9, func=0
	class=06-04-01, hdrtype=0x01, mfdev=0
	cmdreg=0x0000, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x02 (500 ns)
found->	vendor=0x10de, dev=0x0ab0, revid=0xb1
	domain=0, bus=0, slot=10, func=0
	class=02-00-00, hdrtype=0x00, mfdev=0
	cmdreg=0x0007, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x01 (250 ns), maxlat=0x14 (5000 ns)
	intpin=a, irq=14
	powerspec 2  supports D0 D1 D2 D3  current D0
	MSI supports 16 messages, 64 bit, vector masks
	map[10]: type Memory, range 32, base 0xd3486000, size 12, enabled
	map[14]: type I/O Port, range 32, base 0x21e0, size  3, enabled
	map[18]: type Memory, range 32, base 0xd3489000, size  8, enabled
	map[1c]: type Memory, range 32, base 0xd3489300, size  4, enabled
MPTABLE: fixed interrupt routing for 0:10 INTA
MPTABLE: 0:10 INTA routed to irq 14
found->	vendor=0x10de, dev=0x0ab5, revid=0xb1
	domain=0, bus=0, slot=11, func=0
	class=01-01-85, hdrtype=0x00, mfdev=0
	cmdreg=0x0007, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x03 (750 ns), maxlat=0x01 (250 ns)
	intpin=a, irq=11
	powerspec 2  supports D0 D3  current D0
	MSI supports 8 messages, 64 bit
	map[10]: type I/O Port, range 32, base 0x21d8, size  3, enabled
	map[14]: type I/O Port, range 32, base 0x21ec, size  2, enabled
	map[18]: type I/O Port, range 32, base 0x21d0, size  3, enabled
	map[1c]: type I/O Port, range 32, base 0x21e8, size  2, enabled
	map[20]: type I/O Port, range 32, base 0x21c0, size  4, enabled
	map[24]: type Memory, range 32, base 0xd3484000, size 13, enabled
MPTABLE: fixed interrupt routing for 0:11 INTA
MPTABLE: 0:11 INTA routed to irq 11
found->	vendor=0x10de, dev=0x0aa0, revid=0xb1
	domain=0, bus=0, slot=16, func=0
	class=06-04-00, hdrtype=0x01, mfdev=0
	cmdreg=0x0007, statreg=0x0010, cachelnsz=64 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x08 (2000 ns), maxlat=0x00 (0 ns)
	powerspec 2  supports D0 D3  current D0
	MSI supports 2 messages, 64 bit
found->	vendor=0x10de, dev=0x0ac6, revid=0xb1
	domain=0, bus=0, slot=21, func=0
	class=06-04-00, hdrtype=0x01, mfdev=0
	cmdreg=0x0007, statreg=0x0010, cachelnsz=64 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=255
	powerspec 3  supports D0 D3  current D0
	MSI supports 2 messages, 64 bit
	PCI Express ver.2 cap=0x0142[ROOT], slotcap=0x00000000
found->	vendor=0x10de, dev=0x0ac7, revid=0xb1
	domain=0, bus=0, slot=22, func=0
	class=06-04-00, hdrtype=0x01, mfdev=0
	cmdreg=0x0007, statreg=0x0010, cachelnsz=64 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=255
	powerspec 3  supports D0 D3  current D0
	MSI supports 2 messages, 64 bit
	PCI Express ver.2 cap=0x0142[ROOT], slotcap=0x00000000
pci0: <memory, RAM> (vendor 0x10de, dev 0x0a88) at device 0.1
isab0.pci0.pcib0.legacy0.nexus0.root0
isab0: <PCI-ISA bridge> [tentative] port 0x2000-0x20ff at device 3.0 on pci0
isa0.isab0.pci0.pcib0.legacy0.nexus0.root0
isa0: <ISA bus> [tentative] on isab0
isa0: <ISA bus> [attached!] on isab0
isab0: <PCI-ISA bridge> [attached!] port 0x2000-0x20ff at device 3.0 on pci0
pci0: <memory, RAM> (vendor 0x10de, dev 0x0aa4) at device 3.1
pci0: <serial bus, SMBus> (vendor 0x10de, dev 0x0aa2) at device 3.2 irq 15
pci0: <memory, RAM> (vendor 0x10de, dev 0x0a89) at device 3.3
pci0: <memory, RAM> (vendor 0x10de, dev 0x0a98) at device 3.4
pci0: <processor> (vendor 0x10de, dev 0x0aa3) at device 3.5 irq 14
ohci0.pci0.pcib0.legacy0.nexus0.root0
ohci0: <OHCI (generic) USB controller> [tentative] mem 0xd3488000-0xd3488fff irq 11 at device 4.0 on pci0
ohci0: Reserved 0x1000 bytes for rid 0x10 type 3 at 0xd3488000
usb0: OHCI version 1.0, legacy support
usb0.ohci0.pci0.pcib0.legacy0.nexus0.root0
usb0: <OHCI (generic) USB controller> [tentative] on ohci0
usb0: USB revision 1.0
uhub0.usb0.ohci0.pci0.pcib0.legacy0.nexus0.root0
uhub0: <nVidia OHCI root hub, class 9/0, rev 1.00/1.00, addr 1> [tentative] on usb0
uhub0: 7 ports with 7 removable, self powered
uhub0: <nVidia OHCI root hub, class 9/0, rev 1.00/1.00, addr 1> [attached!] on usb0
usb0: <OHCI (generic) USB controller> [attached!] on ohci0
ohci0: <OHCI (generic) USB controller> [attached!] mem 0xd3488000-0xd3488fff irq 11 at device 4.0 on pci0
pci0: <serial bus, USB> (vendor 0x10de, dev 0x0aa6) at device 4.1 irq 10
ohci1.pci0.pcib0.legacy0.nexus0.root0
ohci1: <OHCI (generic) USB controller> [tentative] mem 0xd3487000-0xd3487fff irq 7 at device 6.0 on pci0
ohci1: Reserved 0x1000 bytes for rid 0x10 type 3 at 0xd3487000
usb1: OHCI version 1.0, legacy support
usb1.ohci1.pci0.pcib0.legacy0.nexus0.root0
usb1: <OHCI (generic) USB controller> [tentative] on ohci1
usb1: USB revision 1.0
uhub1.usb1.ohci1.pci0.pcib0.legacy0.nexus0.root0
uhub1: <nVidia OHCI root hub, class 9/0, rev 1.00/1.00, addr 1> [tentative] on usb1
uhub1: 5 ports with 5 removable, self powered
uhub1: <nVidia OHCI root hub, class 9/0, rev 1.00/1.00, addr 1> [attached!] on usb1
usb1: <OHCI (generic) USB controller> [attached!] on ohci1
ohci1: <OHCI (generic) USB controller> [attached!] mem 0xd3487000-0xd3487fff irq 7 at device 6.0 on pci0
pci0: <serial bus, USB> (vendor 0x10de, dev 0x0aa9) at device 6.1 irq 5
pci0: <multimedia, HDA> (vendor 0x10de, dev 0x0ac0) at device 8.0 irq 15
pcib1.pci0.pcib0.legacy0.nexus0.root0
pcib1: <MPTABLE PCI-PCI bridge> [tentative] at device 9.0 on pci0
pcib1:   domain            0
pcib1:   secondary bus     1
pcib1:   subordinate bus   1
pcib1:   I/O decode        0x0-0x0
pcib1:   no prefetched decode
pcib1:   Subtractively decoded bridge.
pci1.pcib1.pci0.pcib0.legacy0.nexus0.root0
pci1: <PCI bus> [tentative] on pcib1
pci1: domain=0, physical bus=1
pci1: <PCI bus> [attached!] on pcib1
pcib1: <MPTABLE PCI-PCI bridge> [attached!] at device 9.0 on pci0
nfe0.pci0.pcib0.legacy0.nexus0.root0
nfe0: <NVIDIA MCP79 Gigabit Ethernet> [tentative] port 0x21e0-0x21e7 mem 0xd3489300-0xd348930f,0xd3489000-0xd34890ff,0xd3486000-0xd3486fff irq 14 at device 10.0 on pci0
nfe0: Reserved 0x1000 bytes for rid 0x10 type 3 at 0xd3486000
miibus0.nfe0.pci0.pcib0.legacy0.nexus0.root0
miibus0: <MII bus> [tentative] on nfe0
rgephy0: rev: 2
rgephy0.miibus0.nfe0.pci0.pcib0.legacy0.nexus0.root0
rgephy0: <8211B/RTL8169S/8110S media interface> [tentative] on miibus0
rgephy0:  10baseT, 10baseT-FDX, 100baseTX, 100baseTX-FDX, 1000baseT, 1000baseT-FDX, auto
rgephy0: <8211B/RTL8169S/8110S media interface> [attached!] on miibus0
miibus0: <MII bus> [attached!] on nfe0
nfe0: bpf attached
nfe0: MAC address: 00:25:bc:e1:70:fe
nfe0: <NVIDIA MCP79 Gigabit Ethernet> [attached!] port 0x21e0-0x21e7 mem 0xd3489300-0xd348930f,0xd3489000-0xd34890ff,0xd3486000-0xd3486fff irq 14 at device 10.0 on pci0
atapci0.pci0.pcib0.legacy0.nexus0.root0
atapci0: <nVidia ATA controller> [tentative] port 0x21c0-0x21cf,0x21e8-0x21eb,0x21d0-0x21d7,0x21ec-0x21ef,0x21d8-0x21df mem 0xd3484000-0xd3485fff irq 11 at device 11.0 on pci0
atapci0: Reserved 0x10 bytes for rid 0x20 type 4 at 0x21c0
ata2.atapci0.pci0.pcib0.legacy0.nexus0.root0
ata2: <ATA channel 0> [tentative] on atapci0
atapci0: Reserved 0x8 bytes for rid 0x10 type 4 at 0x21d8
atapci0: Reserved 0x4 bytes for rid 0x14 type 4 at 0x21ec
ata2: reset tp1 mask=03 ostat0=50 ostat1=7f
ata2: stat0=0x50 err=0x01 lsb=0x00 msb=0x00
ata2: stat1=0xff err=0xff lsb=0xff msb=0xff
ata2: stat1=0xff err=0xff lsb=0xff msb=0xff
ata2: stat1=0xff err=0xff lsb=0xff msb=0xff
ata2: stat1=0xff err=0xff lsb=0xff msb=0xff
ata2: stat1=0xff err=0xff lsb=0xff msb=0xff
ata2: stat1=0xff err=0xff lsb=0xff msb=0xff
ata2: stat1=0xff err=0xff lsb=0xff msb=0xff
ata2: stat1=0xff err=0xff lsb=0xff msb=0xff
ata2: stat1=0xff err=0xff lsb=0xff msb=0xff
ata2: stat1=0xff err=0xff lsb=0xff msb=0xff
ata2: stat1=0xff err=0xff lsb=0xff msb=0xff
ata2: stat1=0xff err=0xff lsb=0xff msb=0xff
ata2: stat1=0xff err=0xff lsb=0xff msb=0xff
ata2: stat1=0xff err=0xff lsb=0xff msb=0xff
ata2: stat1=0xff err=0xff lsb=0xff msb=0xff
ata2: stat1=0xff err=0xff lsb=0xff msb=0xff
ata2: stat1=0xff err=0xff lsb=0xff msb=0xff
ata2: stat1=0xff err=0xff lsb=0xff msb=0xff
ata2: stat1=0xff err=0xff lsb=0xff msb=0xff
ata2: stat1=0xff err=0xff lsb=0xff msb=0xff
ata2: stat1=0xff err=0xff lsb=0xff msb=0xff
ata2: stat1=0xff err=0xff lsb=0xff msb=0xff
ata2: reset tp2 stat0=50 stat1=ff devices=0x1<ATA_MASTER>
ata2-master: pio=PIO4 wdma=WDMA2 udma=UDMA133 cable=40 wire
No policy for ad4 specified, or policy not found
disk scheduler: set policy of ad4 to noop
uhub2.uhub1.usb1.ohci1.pci0.pcib0.legacy0.nexus0.root0
uhub2: <Apple Inc. BRCM2046 Hub, class 9/0, rev 2.00/1.00, addr 2> [tentative] on uhub1
uhub2: 3 ports with 0 removable, self powered
uhub2: <Apple Inc. BRCM2046 Hub, class 9/0, rev 2.00/1.00, addr 2> [attached!] on uhub1
ad4: nVidia check1 failed
ad4: Adaptec check1 failed
ad4: LSI (v3) check1 failed
ad4: LSI (v2) check1 failed
ad4: FreeBSD check1 failed
ad4: 238475MB <Hitachi HTS545025B9SA02 PB2AC60Q> at ata2-master UDMA33
ad4: 488397168 sectors [484521C/16H/63S] 16 sectors/interrupt 1 depth queue
ata2: <ATA channel 0> [attached!] on atapci0
ata3.atapci0.pci0.pcib0.legacy0.nexus0.root0
ata3: <ATA channel 1> [tentative] on atapci0
atapci0: Reserved 0x8 bytes for rid 0x18 type 4 at 0x21d0
atapci0: Reserved 0x4 bytes for rid 0x1c type 4 at 0x21e8
ata3: reset tp1 mask=03 ostat0=50 ostat1=7f
ata3: stat0=0x00 err=0x01 lsb=0x14 msb=0xeb
ata3: stat1=0xff err=0xff lsb=0xff msb=0xff
ata3: stat1=0xff err=0xff lsb=0xff msb=0xff
ata3: stat1=0xff err=0xff lsb=0xff msb=0xff
ata3: stat1=0xff err=0xff lsb=0xff msb=0xff
ata3: stat1=0xff err=0xff lsb=0xff msb=0xff
ata3: stat1=0xff err=0xff lsb=0xff msb=0xff
ata3: stat1=0xff err=0xff lsb=0xff msb=0xff
ata3: stat1=0xff err=0xff lsb=0xff msb=0xff
ata3: stat1=0xff err=0xff lsb=0xff msb=0xff
ata3: stat1=0xff err=0xff lsb=0xff msb=0xff
ata3: stat1=0xff err=0xff lsb=0xff msb=0xff
ata3: stat1=0xff err=0xff lsb=0xff msb=0xff
ata3: stat1=0xff err=0xff lsb=0xff msb=0xff
ata3: stat1=0xff err=0xff lsb=0xff msb=0xff
ata3: stat1=0xff err=0xff lsb=0xff msb=0xff
ata3: stat1=0xff err=0xff lsb=0xff msb=0xff
ata3: stat1=0xff err=0xff lsb=0xff msb=0xff
ata3: stat1=0xff err=0xff lsb=0xff msb=0xff
ata3: stat1=0xff err=0xff lsb=0xff msb=0xff
ata3: stat1=0xff err=0xff lsb=0xff msb=0xff
ata3: stat1=0xff err=0xff lsb=0xff msb=0xff
ata3: stat1=0xff err=0xff lsb=0xff msb=0xff
ata3: reset tp2 stat0=00 stat1=ff devices=0x4<ATAPI_MASTER>
ata3-master: pio=PIO4 wdma=WDMA2 udma=UDMA133 cable=40 wire
ugen0.uhub0.usb0.ohci0.pci0.pcib0.legacy0.nexus0.root0
ugen0: <Apple Inc. Built-in iSight, class 239/2, rev 2.00/4.19, addr 2> [tentative] on uhub0
ad4: type 0xa5, start 63, end = 167763455, size 167763393 : OK
ad4: type 0x5, start 167763966, end = 335544319, size 167780354 
ad4: C/H/S start 1023/254/63 (16515008) != start 167763966: invalid
ad4: C/H/S end 1023/254/63 (16515008) != end 335544319: invalid
ad4: type 0xa5, start 335544363, end = 488397104, size 152852742 : OK
ad4: type 0x83, start 167763968, end = 321871871, size 154107904 
ad4: C/H/S start 1023/254/63 (16515008) != start 167763968: invalid
ad4: C/H/S end 1023/254/63 (16515008) != end 321871871: invalid
ad4<extended>: type 0x5, start 321871872, end = 335544319, size 13672448 
ad4<extended>: C/H/S start 1023/254/63 (16515008) != start 321871872: invalid
ad4<extended>: C/H/S end 1023/254/63 (16515008) != end 335544319: invalid
ugen0: <Apple Inc. Built-in iSight, class 239/2, rev 2.00/4.19, addr 2> [attached!] on uhub0
ad4: type 0x82, start 321873920, end = 335544319, size 13670400 
ad4: C/H/S start 1023/254/63 (16515008) != start 321873920: invalid
ad4: C/H/S end 1023/254/63 (16515008) != end 335544319: invalid
No policy for acd0 specified, or policy not found
disk scheduler: set policy of acd0 to noop
acd0: <HL-DT-ST DVDRW GS23N/SB00> DVDR drive at ata3 as master
acd0: read 10820KB/s (10820KB/s) write 10820KB/s (10820KB/s), 2048KB buffer, UDMA33
acd0: Reads: CDR, CDRW, CDDA stream, DVDROM, DVDR, DVDRAM, packet
acd0: Writes: CDR, CDRW, DVDR, test write, burnproof
acd0: Audio: play, 256 volume levels
acd0: Mechanism: ejectable caddy, unlocked
acd0: Medium: DVD 120mm data disc
ata3: <ATA channel 1> [attached!] on atapci0
atapci0: <nVidia ATA controller> [attached!] port 0x21c0-0x21cf,0x21e8-0x21eb,0x21d0-0x21d7,0x21ec-0x21ef,0x21d8-0x21df mem 0xd3484000-0xd3485fff irq 11 at device 11.0 on pci0
pcib2.pci0.pcib0.legacy0.nexus0.root0
pcib2: <MPTABLE PCI-PCI bridge> [tentative] at device 16.0 on pci0
pcib2:   domain            0
pcib2:   secondary bus     2
pcib2:   subordinate bus   2
pcib2:   I/O decode        0x1000-0x1fff
pcib2:   memory decode     0xd2000000-0xd30fffff
pcib2:   prefetched decode 0xc0000000-0xd1ffffff
pci2.pcib2.pci0.pcib0.legacy0.nexus0.root0
pci2: <PCI bus> [tentative] on pcib2
pci2: domain=0, physical bus=2
found->	vendor=0x10de, dev=0x0863, revid=0xb1
	domain=0, bus=2, slot=0, func=0
	class=03-00-00, hdrtype=0x00, mfdev=0
	cmdreg=0x0007, statreg=0x0010, cachelnsz=64 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=11
	powerspec 2  supports D0 D3  current D0
	MSI supports 1 message, 64 bit
	map[10]: type Memory, range 32, base 0xd2000000, size 24, enabled
pcib2: requested memory range 0xd2000000-0xd2ffffff: good
	map[14]: type Prefetchable Memory, range 64, base 0xc0000000, size 28, enabled
pcib2: requested memory range 0xc0000000-0xcfffffff: good
	map[1c]: type Prefetchable Memory, range 64, base 0xd0000000, size 25, enabled
pcib2: requested memory range 0xd0000000-0xd1ffffff: good
	map[24]: type I/O Port, range 32, base 0x1000, size  7, enabled
pcib2: requested I/O range 0x1000-0x107f: in range
MPTABLE: fixed interrupt routing for 0:16 INTA
MPTABLE: Unable to route for bus 0 slot 16 INTA
MPTABLE: fixed interrupt routing for 2:0 INTA
MPTABLE: 2:0 INTA routed to irq 11
vgapci0.pci2.pcib2.pci0.pcib0.legacy0.nexus0.root0
vgapci0: <VGA-compatible display> [tentative] port 0x1000-0x107f mem 0xd0000000-0xd1ffffff,0xc0000000-0xcfffffff,0xd2000000-0xd2ffffff irq 11 at device 0.0 on pci2
vgapci0: <VGA-compatible display> [attached!] port 0x1000-0x107f mem 0xd0000000-0xd1ffffff,0xc0000000-0xcfffffff,0xd2000000-0xd2ffffff irq 11 at device 0.0 on pci2
pci2: <PCI bus> [attached!] on pcib2
pcib2: <MPTABLE PCI-PCI bridge> [attached!] at device 16.0 on pci0
pcib3.pci0.pcib0.legacy0.nexus0.root0
pcib3: <MPTABLE PCI-PCI bridge> [tentative] at device 21.0 on pci0
pcib3:   domain            0
pcib3:   secondary bus     3
pcib3:   subordinate bus   3
pcib3:   I/O decode        0xfffff000-0xfff
pcib3:   memory decode     0xd3200000-0xd32fffff
pcib3:   no prefetched decode
pcib3: Disable PCI Express hot-plug interrupts(0x0020)
pci3.pcib3.pci0.pcib0.legacy0.nexus0.root0
pci3: <PCI bus> [tentative] on pcib3
pci3: domain=0, physical bus=3
found->	vendor=0x14e4, dev=0x432b, revid=0x01
	domain=0, bus=3, slot=0, func=0
	class=02-80-00, hdrtype=0x00, mfdev=0
	cmdreg=0x0006, statreg=0x0010, cachelnsz=64 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=10
	powerspec 3  supports D0 D1 D2 D3  current D0
	MSI supports 1 message, 64 bit
	PCI Express ver.1 cap=0x0001[DEVICE]
	map[10]: type Memory, range 64, base 0xd3200000, size 14, enabled
pcib3: requested memory range 0xd3200000-0xd3203fff: good
MPTABLE: fixed interrupt routing for 0:21 INTA
MPTABLE: Unable to route for bus 0 slot 21 INTA
MPTABLE: fixed interrupt routing for 3:0 INTA
MPTABLE: 3:0 INTA routed to irq 10
pci3: <network> (vendor 0x14e4, dev 0x432b) at device 0.0 irq 10
pci3: <PCI bus> [attached!] on pcib3
pcib3: <MPTABLE PCI-PCI bridge> [attached!] at device 21.0 on pci0
pcib4.pci0.pcib0.legacy0.nexus0.root0
pcib4: <MPTABLE PCI-PCI bridge> [tentative] at device 22.0 on pci0
pcib4:   domain            0
pcib4:   secondary bus     4
pcib4:   subordinate bus   4
pcib4:   I/O decode        0xfffff000-0xfff
pcib4:   memory decode     0xd3100000-0xd31fffff
pcib4:   no prefetched decode
pcib4: Disable PCI Express hot-plug interrupts(0x0020)
pci4.pcib4.pci0.pcib0.legacy0.nexus0.root0
pci4: <PCI bus> [tentative] on pcib4
pci4: domain=0, physical bus=4
found->	vendor=0x11c1, dev=0x5901, revid=0x07
	domain=0, bus=4, slot=0, func=0
	class=0c-00-10, hdrtype=0x00, mfdev=0
	cmdreg=0x0007, statreg=0x0010, cachelnsz=64 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=7
	powerspec 3  supports D0 D1 D2 D3  current D0
	MSI supports 1 message, 64 bit
	PCI Express ver.1 cap=0x0001[DEVICE]
	map[10]: type Memory, range 64, base 0xd3100000, size 12, enabled
pcib4: requested memory range 0xd3100000-0xd3100fff: good
MPTABLE: fixed interrupt routing for 0:22 INTA
MPTABLE: Unable to route for bus 0 slot 22 INTA
MPTABLE: fixed interrupt routing for 4:0 INTA
MPTABLE: 4:0 INTA routed to irq 7
fwohci0: vendor=11c1, dev=5901
fwohci0.pci4.pcib4.pci0.pcib0.legacy0.nexus0.root0
fwohci0: <1394 Open Host Controller Interface> [tentative] mem 0xd3100000-0xd3100fff irq 7 at device 0.0 on pci4
fwohci0: latency timer 0 -> 32.
fwohci0: cache size 64 -> 64.
fwohci0: Reserved 0x1000 bytes for rid 0x10 type 3 at 0xd3100000
fwohci0: OHCI version 1.10 (ROM=0)
fwohci0: No. of Isochronous channel is 8.
fwohci0: EUI64 00:25:bc:ff:fe:e1:70:fe
fwohci0: resetting OHCI...done (loop=0)
fwohci0: fwphy_rddata: 0x2 loop=1, retry=0
fwohci0: fwphy_rddata: 0x3 loop=1, retry=0
fwohci0: invalid speed 7 (fixed to 3).
fwohci0: Phy 1394a available S800, 3 ports.
fwohci0: fwphy_rddata: 0x5 loop=1, retry=0
fwohci0: Enable 1394a Enhancements
fwohci0: fwphy_rddata: 0x5 loop=1, retry=0
fwohci0: fwphy_rddata: 0x2 loop=1, retry=0
fwohci0: fwphy_rddata: 0x4 loop=1, retry=0
fwohci0: fwphy_rddata: 0x4 loop=1, retry=0
fwohci0: fwphy_rddata: 0x4 loop=1, retry=0
fwohci0: Link S800, max_rec 4096 bytes.
fwohci0: BUS_OPT 0xb083 -> 0xf800b083
fwohci0: fwohci_set_intr: 1
firewire0.fwohci0.pci4.pcib4.pci0.pcib0.legacy0.nexus0.root0
firewire0: <IEEE1394(FireWire) bus> [tentative] on fwohci0
fwe0.firewire0.fwohci0.pci4.pcib4.pci0.pcib0.legacy0.nexus0.root0
fwe0: <Ethernet over FireWire> [tentative] on firewire0
fwe0: bpf attached
fwe0: MAC address: 02:25:bc:e1:70:fe
fwe0: <Ethernet over FireWire> [attached!] on firewire0
sbp0.firewire0.fwohci0.pci4.pcib4.pci0.pcib0.legacy0.nexus0.root0
sbp0: <SBP-2/SCSI over FireWire> [tentative] on firewire0
sbp_attach (cold=1)
sbp0: <SBP-2/SCSI over FireWire> [attached!] on firewire0
sbp_post_busreset
fwohci0: Initiate bus reset
fwohci0: fwphy_rddata: 0x1 loop=1, retry=0
fwohci0: fwphy_rddata: 0x1 loop=1, retry=0
firewire0: <IEEE1394(FireWire) bus> [attached!] on fwohci0
Unknown tcode 14
fwohci0: node_id=0xc800ffc0, gen=2, CYCLEMASTER mode
firewire0: 1 nodes, maxhop <= 0, cable IRM = 0 (me)
fwohci0: fw_set_bus_manager: 0->0 (loop=0)
firewire0: bus manager 0 (me)
send phy_config root_node=-1 gap_count=5
fwohci0: maxdesc: 2
fwohci0: start AT DMA status=0
fwohci0: <1394 Open Host Controller Interface> [attached!] mem 0xd3100000-0xd3100fff irq 7 at device 0.0 on pci4
pci4: <PCI bus> [attached!] on pcib4
pcib4: <MPTABLE PCI-PCI bridge> [attached!] at device 22.0 on pci0
pci0: <PCI bus> [attached!] on pcib0
pcib0: <MPTABLE Host-PCI bridge> [attached!] pcibus 0 on motherboard
Trying Read_Port at 203
Trying Read_Port at 243
Trying Read_Port at 283
Trying Read_Port at 2c3
Trying Read_Port at 303
Trying Read_Port at 343
Trying Read_Port at 383
Trying Read_Port at 3c3
ex_isa_identify()
isa_probe_children: disabling PnP devices
isa_probe_children: probing non-PnP devices
orm0.isa0.isab0.pci0.pcib0.legacy0.nexus0.root0
orm0: <Option ROM> [tentative] at iomem 0xc0000-0xce7ff on isa0
orm0: <Option ROM> [attached!] at iomem 0xc0000-0xce7ff on isa0
adv0 [tentative] failed to probe on isa0
atkbdc0: <Keyboard controller (i8042)> [tentative] failed to probe at port 0x60,0x64 on isa0
vga0.isa0.isab0.pci0.pcib0.legacy0.nexus0.root0
vga0: <Generic ISA VGA> [tentative] at port 0x3c0-0x3df iomem 0xa0000-0xbffff on isa0
fb0: vga0, vga, type:VGA (5), flags:0x7007f
fb0: port:0x3c0-0x3df, mem:0xa0000 0x20000
fb0: init mode:24, bios mode:3, current mode:24
fb0: window:0xffffffff800b8000 size:32k gran:32k, buf:0 size:32k
VGA parameters upon power-up
 50 18 10 00 00 00 03 00 02 67 5f 4f 50 82 55 81
 bf 1f 00 4f 0d 0e 00 00 07 80 9c 8e 8f 28 1f 96
 b9 a3 ff 00 01 02 03 04 05 14 07 38 39 3a 3b 3c
 3d 3e 3f 0c 00 0f 08 00 00 00 00 00 10 0e 00 ff
VGA parameters in BIOS for mode 24
 50 18 10 00 10 00 03 00 02 67 5f 4f 50 82 54 80
 bf 1f 00 4f 0d 0e 00 00 00 00 9c 8e 8f 28 1f 96
 b9 a3 ff 00 01 02 03 04 05 14 07 38 39 3a 3b 3c
 3d 3e 3f 0c 00 0f 08 00 00 00 00 00 10 0e 00 ff
VGA parameters to be used for mode 24
 50 18 10 00 10 00 03 00 02 67 5f 4f 50 82 54 80
 bf 1f 00 4f 0d 0e 00 00 00 00 9c 8e 8f 28 1f 96
 b9 a3 ff 00 01 02 03 04 05 14 07 38 39 3a 3b 3c
 3d 3e 3f 0c 00 0f 08 00 00 00 00 00 10 0e 00 ff
vga0: <Generic ISA VGA> [attached!] at port 0x3c0-0x3df iomem 0xa0000-0xbffff on isa0
sc0.isa0.isab0.pci0.pcib0.legacy0.nexus0.root0
sc0: <System console> [tentative] at flags 0x100 on isa0
sc0: VGA <16 virtual consoles, flags=0x300>
sc0: fb0, kbd0, terminal emulator: sc (syscons terminal)
sc0: <System console> [attached!] at flags 0x100 on isa0
lm0 [tentative] failed to probe at port 0x290-0x297 on isa0
it0 [tentative] failed to probe at port 0x290-0x297 on isa0
it1 [tentative] failed to probe at port 0xc00-0xc07 on isa0
it2 [tentative] failed to probe at port 0xd00-0xd07 on isa0
it3 [tentative] failed to probe at port 0x228-0x22f on isa0
wbsio0 [tentative] failed to probe at port 0x2e-0x2f on isa0
wbsio1 [tentative] failed to probe at port 0x4e-0x4f on isa0
sio0: can't drain, serial port might not exist, disabling
sio0 [tentative] failed to probe at port 0x3f8-0x3ff irq 4 flags 0x10 on isa0
sio1: can't drain, serial port might not exist, disabling
sio1 [tentative] failed to probe at port 0x2f8-0x2ff irq 3 on isa0
sio2: not probed (disabled)
sio3: not probed (disabled)
ppc0: cannot reserve I/O port range
ppc0: <Parallel port> [tentative] failed to probe at irq 7 on isa0
ed0: not probed (disabled)
lnc0: not probed (disabled)
cs0: not probed (disabled)
sn0: not probed (disabled)
isa_probe_children: probing PnP devices
uhid0.uhub0.usb0.ohci0.pci0.pcib0.legacy0.nexus0.root0
uhid0: <Apple Computer, Inc. IR Receiver, class 0/0, rev 2.00/0.16, addr 3> [tentative] on uhub0
uhid0: <Apple Computer, Inc. IR Receiver, class 0/0, rev 2.00/0.16, addr 3> [attached!] on uhub0
ukbd0.uhub0.usb0.ohci0.pci0.pcib0.legacy0.nexus0.root0
ukbd0: <Apple Inc. Apple Internal Keyboard / Trackpad, class 0/0, rev 2.00/0.81, addr 4> [tentative] on uhub0
kbd: new array size 4
kbd1 at ukbd0
kbd1: ukbd0, generic (0), config:0x0, flags:0x350000
ukbd0: <Apple Inc. Apple Internal Keyboard / Trackpad, class 0/0, rev 2.00/0.81, addr 4> [attached!] on uhub0
uhid1.uhub0.usb0.ohci0.pci0.pcib0.legacy0.nexus0.root0
uhid1: <Apple Inc. Apple Internal Keyboard / Trackpad, class 0/0, rev 2.00/0.81, addr 4> [tentative] on uhub0
uhid1: <Apple Inc. Apple Internal Keyboard / Trackpad, class 0/0, rev 2.00/0.81, addr 4> [attached!] on uhub0
ums0.uhub0.usb0.ohci0.pci0.pcib0.legacy0.nexus0.root0
ums0: <Apple Inc. Apple Internal Keyboard / Trackpad, class 0/0, rev 2.00/0.81, addr 4> [tentative] on uhub0
ums0: 3 buttons
ums0: <Apple Inc. Apple Internal Keyboard / Trackpad, class 0/0, rev 2.00/0.81, addr 4> [attached!] on uhub0
ukbd1.uhub2.uhub1.usb1.ohci1.pci0.pcib0.legacy0.nexus0.root0
ukbd1: <vendor 0x05ac product 0x820a, class 0/0, rev 2.00/1.00, addr 4> [tentative] on uhub2
kbd2 at ukbd1
kbd2: ukbd1, generic (0), config:0x0, flags:0x350000
ukbd1: <vendor 0x05ac product 0x820a, class 0/0, rev 2.00/1.00, addr 4> [attached!] on uhub2
ums1.uhub2.uhub1.usb1.ohci1.pci0.pcib0.legacy0.nexus0.root0
ums1: <vendor 0x05ac product 0x820b, class 0/0, rev 2.00/1.00, addr 5> [tentative] on uhub2
ums1: 3 buttons
ums1: <vendor 0x05ac product 0x820b, class 0/0, rev 2.00/1.00, addr 5> [attached!] on uhub2
umass0.uhub1.usb1.ohci1.pci0.pcib0.legacy0.nexus0.root0
umass0: <Apple Card Reader, class 0/0, rev 2.00/98.33, addr 6> [tentative] on uhub1
umass0:3:0:-1: Attached to scbus3
umass0: <Apple Card Reader, class 0/0, rev 2.00/98.33, addr 6> [attached!] on uhub1
Current DB 0
ch = 0
 Current OP   KEY INT BR   len     Addr   Depend Stat: Cnt
01d52000 OUTL ST2 ALL ALL    12 00000000 01d52080 8411:57ff RUN,ACTIVE, ack complete(11)
0x000000e0 0x00450000 0xffbaffff 0x00000000
bus_explore done
sbp_post_explore
faith0: bpf attached
lo0: bpf attached
ppp0: bpf attached
sl0: bpf attached
hptrr: no controller detected.
hpt27xx: no controller detected.
CAM: Configuring bus: ata0
CAM: Configuring bus: ata1
CAM: Configuring bus: sbp0
CAM: Configuring bus: umass-sim0
CAM: Configuring 4 busses
CAM: Finished configuring bus: ata0
(probe1:sbp0:0:0:0): error 22
(probe1:sbp0:0:0:0): Unretryable Error
(probe2:sbp0:0:1:0): error 22
(probe2:sbp0:0:1:0): Unretryable Error
(probe3:sbp0:0:2:0): error 22
(probe3:sbp0:0:2:0): Unretryable Error
(probe4:sbp0:0:3:0): error 22
(probe4:sbp0:0:3:0): Unretryable Error
(probe5:sbp0:0:4:0): error 22
(probe5:sbp0:0:4:0): Unretryable Error
(probe6:sbp0:0:5:0): error 22
(probe6:sbp0:0:5:0): Unretryable Error
(probe7:sbp0:0:6:0): error 22
(probe7:sbp0:0:6:0): Unretryable Error
CAM: Finished configuring bus: sbp0
(probe0:ata1:0:0:0): error 22
(probe0:ata1:0:0:0): Unretryable Error
(probe0:ata1:0:0:0): Down reving Protocol Version from 2 to 0?
(probe0:ata1:0:0:0): error 22
(probe0:ata1:0:0:0): Unretryable Error
CAM: Finished configuring bus: ata1
(probe8:umass-sim0:0:0:0): Down reving Protocol Version from 2 to 0?
(probe8:umass-sim0:0:0:0): Uninitialized Transport 5:ffffffe0?
CAM: Finished configuring bus: umass-sim0
CAM: finished configuring all busses
no B_DEVMAGIC (bootdev=0)
ATA PseudoRAID loaded
sg0 at ata1 bus 0 target 0 lun 0
sg0: <HL-DT-ST DVDRW  GS23N SB00> Removable CD-ROM SCSI-0 device 
sg0: 33.000MB/s transfers
sg8 at umass-sim0 bus 0 target 0 lun 0
sg8: <APPLE SD Card Reader 1.00> Removable Direct Access SCSI-0 device 
sg8: 1.000MB/s transfers
No policy for da8 specified, or policy not found
disk scheduler: set policy of da8 to noop
da8: si_iosize_max:131072
No policy for cd0 specified, or policy not found
disk scheduler: set policy of cd0 to noop
pass0 at ata1 bus 0 target 0 lun 0
pass0: <HL-DT-ST DVDRW  GS23N SB00> Removable CD-ROM SCSI-0 device 
pass0: 33.000MB/s transfers
pass8 at umass-sim0 bus 0 target 0 lun 0
pass8: <APPLE SD Card Reader 1.00> Removable Direct Access SCSI-0 device 
pass8: 1.000MB/s transfers
cd0 at ata1 bus 0 target 0 lun 0
cd0: <HL-DT-ST DVDRW  GS23N SB00> Removable CD-ROM SCSI-0 device 
cd0: 33.000MB/s transfers
cd0: cd present [376832 x 2048 byte records]
ugen1.uhub2.uhub1.usb1.ohci1.pci0.pcib0.legacy0.nexus0.root0
ugen1: <Apple Inc. Bluetooth USB Host Controller, class 255/1, rev 2.00/2.07, addr 3> [tentative] on uhub2
(da8:umass-sim0:0:0:0): error 6
(da8:umass-sim0:0:0:0): Unretryable Error
da8 at umass-sim0 bus 0 target 0 lun 0
da8: <APPLE SD Card Reader 1.00> Removable Direct Access SCSI-0 device 
da8: 1.000MB/s transfers
da8: Attempt to query device size failed: NOT READY, Medium not present
ugen1: <Apple Inc. Bluetooth USB Host Controller, class 255/1, rev 2.00/2.07, addr 3> [attached!] on uhub2
Mounting root from hammer:serno/090621PBC200QSH43EMH_.s1d
HAMMER(ROOT) recovery check seqno=004409b9
HAMMER(ROOT) recovery range 300000001d7941e8-300000001d7941e8
HAMMER(ROOT) recovery nexto 300000001d7941e8 endseqno=004409ba
HAMMER(ROOT) mounted clean, no recovery needed
DMA space used: 3680k, remaining available: 16384k
Mounting devfs
start_init: trying /sbin/init
cd0: invalid primary partition table: no magic
cd0: invalid primary partition table: no magic
cd0: invalid primary partition table: no magic
kthread 0xffffffe1264cc100 syncer6 has exited
kthread 0xffffffe1264cd700 syncer7 has exited
kthread 0xffffffe1264cd700 syncer8 has exited
kthread 0xffffffe1264cd180 syncer9 has exited
kthread 0xffffffe1264cd180 syncer10 has exited
kthread 0xffffffe1264ccc00 syncer11 has exited
kthread 0xffffffe1264ccc00 syncer12 has exited
nfe0: use non-jumbo frames
pflog0: bpf attached
pflog0: promiscuous mode enabled
splash: image decoder found: blank_saver
umass1.uhub1.usb1.ohci1.pci0.pcib0.legacy0.nexus0.root0
umass1: <Kingston DataTraveler 3.0, class 0/0, rev 2.10/1.10, addr 7> [tentative] on uhub1
umass1:4:1:-1: Attached to scbus4
umass1: <Kingston DataTraveler 3.0, class 0/0, rev 2.10/1.10, addr 7> [attached!] on uhub1
(probe8:umass-sim1:1:0:0): Uninitialized Transport 5:ffffffe1?
pass9 at umass-sim1 bus 1 target 0 lun 0
pass9: <Kingston DataTraveler 3.0 PMAP> Removable Direct Access SCSI-6 device 
pass9: Serial Number 6E0DAC4043C9
pass9: 1.000MB/s transfers
No policy for da9 specified, or policy not found
disk scheduler: set policy of da9 to noop
da9: si_iosize_max:131072
sg9 at umass-sim1 bus 1 target 0 lun 0
sg9: <Kingston DataTraveler 3.0 PMAP> Removable Direct Access SCSI-6 device 
sg9: Serial Number 6E0DAC4043C9
sg9: 1.000MB/s transfers
da9 at umass-sim1 bus 1 target 0 lun 0
da9: <Kingston DataTraveler 3.0 PMAP> Removable Direct Access SCSI-6 device 
da9: Serial Number 6E0DAC4043C9
da9: 1.000MB/s transfers
da9: 121195MB (248208384 512 byte sectors: 255H 63S/T 15450C)
da9: type 0xc, start 8064, end = 248208383, size 248200320 
da9: C/H/S start 1/0/1 (4160) != start 8064: invalid
da9: C/H/S end 58/103/40 (245439) != end 248208383: invalid
