Table 'FACP' at 0xbfeec000
Table 'HPET' at 0xbfeeb000
Table 'APIC' at 0xbfeea000
APIC: Found table at 0xbfeea000
APIC: Using the MADT enumerator.
MADT: Found CPU APIC ID 0 ACPI ID 0: enabled
SMP: Added CPU 0 (AP)
MADT: Found CPU APIC ID 1 ACPI ID 1: enabled
SMP: Added CPU 1 (AP)
Copyright (c) 1992-2014 The FreeBSD Project.
Copyright (c) 1979, 1980, 1983, 1986, 1988, 1989, 1991, 1992, 1993, 1994
	The Regents of the University of California. All rights reserved.
FreeBSD is a registered trademark of The FreeBSD Foundation.
FreeBSD 10.0-RELEASE #0 r260789: Thu Jan 16 22:34:59 UTC 2014
    root@snap.freebsd.org:/usr/obj/usr/src/sys/GENERIC amd64
FreeBSD clang version 3.3 (tags/RELEASE_33/final 183502) 20130610
Preloaded elf kernel "/boot/kernel/kernel" at 0xffffffff82682000.
Preloaded elf obj module "/boot/modules/nvidia.ko" at 0xffffffff82682db0.
Preloaded elf obj module "/boot/kernel/linux.ko" at 0xffffffff82683398.
Calibrating TSC clock ... TSC clock: 2255389235 Hz
CPU: Intel(R) Core(TM)2 Duo CPU     P7550  @ 2.26GHz (2255.39-MHz K8-class CPU)
  Origin = "GenuineIntel"  Id = 0x1067a  Family = 0x6  Model = 0x17  Stepping = 10
  Features=0xbfebfbff<FPU,VME,DE,PSE,TSC,MSR,PAE,MCE,CX8,APIC,SEP,MTRR,PGE,MCA,CMOV,PAT,PSE36,CLFLUSH,DTS,ACPI,MMX,FXSR,SSE,SSE2,SS,HTT,TM,PBE>
  Features2=0xc08e3bd<SSE3,DTES64,MON,DS_CPL,VMX,EST,TM2,SSSE3,CX16,xTPR,PDCM,SSE4.1,XSAVE,OSXSAVE>
  AMD Features=0x20100800<SYSCALL,NX,LM>
  AMD Features2=0x1<LAHF>
  TSC: P-state invariant, performance statistics
real memory  = 8589934592 (8192 MB)
Physical memory chunk(s):
0x0000000000010000 - 0x000000000009bfff, 573440 bytes (140 pages)
0x0000000000100000 - 0x00000000001fffff, 1048576 bytes (256 pages)
0x00000000026b7000 - 0x00000000ae72afff, 2886156288 bytes (704628 pages)
0x0000000100000000 - 0x0000000231518fff, 5122396160 bytes (1250585 pages)
avail memory = 7957954560 (7589 MB)
Event timer "LAPIC" quality 400
ACPI APIC Table: <APPLE  Apple00>
INTR: Adding local APIC 1 as a target
FreeBSD/SMP: Multiprocessor System Detected: 2 CPUs
FreeBSD/SMP: 1 package(s) x 2 core(s)
 cpu0 (BSP): APIC ID:  0
 cpu1 (AP): APIC ID:  1
APIC: CPU 0 has ACPI ID 0
APIC: CPU 1 has ACPI ID 1
x86bios:  IVT 0x000000-0x0004ff at 0xfffff80000000000
x86bios: SSEG 0x098000-0x098fff at 0xfffffe021b7f0000
x86bios: EBDA 0x09f000-0x09ffff at 0xfffff8000009f000
x86bios:  ROM 0x0a0000-0x0fefff at 0xfffff800000a0000
XEN: CPU 0 has VCPU ID 0
XEN: CPU 1 has VCPU ID 1
ULE: setup cpu 0
ULE: setup cpu 1
ACPI: RSDP 0xfe020 00024 (v02 APPLE )
ACPI: XSDT 0xbfeee1c0 0007C (v01 APPLE   Apple00 000000AC      01000013)
ACPI: FACP 0xbfeec000 000F4 (v04 APPLE   Apple00 000000AC Loki 0000005F)
ACPI: DSDT 0xbfedf000 05B9E (v01 APPLE  MacBookP 00050005 INTL 20061109)
ACPI: FACS 0xbfecd000 00040
ACPI: HPET 0xbfeeb000 00038 (v01 APPLE   Apple00 00000001 Loki 0000005F)
ACPI: APIC 0xbfeea000 00068 (v01 APPLE   Apple00 00000001 Loki 0000005F)
ACPI: APIC 0xbfee9000 00068 (v02 APPLE   Apple00 00000001 Loki 0000005F)
ACPI: MCFG 0xbfee8000 0003C (v01 APPLE   Apple00 00000001 Loki 0000005F)
ACPI: ASF! 0xbfee7000 000A5 (v32 APPLE   Apple00 00000001 Loki 0000005F)
ACPI: SBST 0xbfee6000 00030 (v01 APPLE   Apple00 00000001 Loki 0000005F)
ACPI: ECDT 0xbfee5000 00053 (v01 APPLE   Apple00 00000001 Loki 0000005F)
ACPI: SSDT 0xbfec7000 004DC (v01  APPLE    CpuPm 00003000 INTL 20061109)
ACPI: SSDT 0xbfecc000 000A5 (v01 SataRe  SataPri 00001000 INTL 20061109)
ACPI: SSDT 0xbfecb000 0009F (v01 SataRe  SataSec 00001000 INTL 20061109)
MADT: Found IO APIC ID 1, Interrupt 0 at 0xfec00000
ioapic0: Changing APIC ID to 1
ioapic0: Routing external 8259A's -> intpin 0
MADT: Interrupt override: source 0, irq 2
ioapic0: Routing IRQ 0 -> intpin 2
MADT: Interrupt override: source 9, irq 9
ioapic0: intpin 9 trigger: level
lapic0: Routing NMI -> LINT1
lapic0: LINT1 trigger: edge
lapic0: LINT1 polarity: high
lapic1: Routing NMI -> LINT1
lapic1: LINT1 trigger: edge
lapic1: LINT1 polarity: high
ioapic0 <Version 1.1> irqs 0-23 on motherboard
cpu0 BSP:
     ID: 0x00000000   VER: 0x00050014 LDR: 0x00000000 DFR: 0xffffffff
  lint0: 0x00010700 lint1: 0x00000400 TPR: 0x00000000 SVR: 0x000001ff
  timer: 0x000100ef therm: 0x00010000 err: 0x000000f0 pmc: 0x00010400
wlan: <802.11 Link Layer>
snd_unit_init() u=0x00ff8000 [512] d=0x00007c00 [32] c=0x000003ff [1024]
feeder_register: snd_unit=-1 snd_maxautovchans=16 latency=5 feeder_rate_min=1 feeder_rate_max=2016000 feeder_rate_round=25
Hardware, Intel IvyBridge+ RNG: RDRAND is not present
Hardware, VIA Nehemiah Padlock RNG: VIA Padlock RNG not present
kbd0 at kbdmux0
mem: <memory>
null: <null device, zero device>
nfslock: pseudo-device
Falling back to <Software, Yarrow> random adaptor
random: <Software, Yarrow> initialized
VESA: INT 0x10 vector 0xc000:0x1b50
VESA: information block
0000   56 45 53 41 00 03 00 01 00 99 01 00 00 00 22 00
0010   00 99 e0 00 79 62 07 01 00 99 1a 01 00 99 3c 01
0020   00 99 00 01 01 01 02 01 03 01 04 01 05 01 0e 01
0030   0f 01 11 01 12 01 14 01 15 01 17 01 18 01 30 01
0040   31 01 32 01 33 01 34 01 35 01 36 01 3d 01 3e 01
0050   60 01 61 01 62 01 7b 01 ff ff 00 00 00 00 00 00
0060   00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
0070   00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
0080   00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
0090   00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
00a0   00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
00b0   00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
00c0   00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
00d0   00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
00e0   00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
00f0   00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
0100   4e 56 49 44 49 41 00 4e 56 49 44 49 41 20 43 6f
0110   72 70 6f 72 61 74 69 6f 6e 00 4e 56 49 44 49 41
0120   20 47 65 46 6f 72 63 65 20 39 34 30 30 4d 0d 0a
0130   20 2d 20 6d 63 70 37 39 6b 32 34 00 43 68 69 70
0140   20 52 65 76 20 20 20 00 00 00 00 00 00 00 00 00
0150   00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
0160   00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
0170   00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
0180   00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
0190   00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
01a0   00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
01b0   00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
01c0   00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
01d0   00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
01e0   00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
01f0   00 00 00 00 00 00 00 00 00 00 00 00 00 00 00 00
VESA: 27 mode(s) found
VESA: v3.0, 14336k memory, flags:0x1, mode table:0xfffffe01df98f022 (99000022)
VESA: NVIDIA
VESA: NVIDIA Corporation NVIDIA GeForce 9400M
 - mcp79k24 Chip Rev   
io: <I/O>
VMBUS: load
hpt27xx: RocketRAID 27xx controller driver v1.1
hptrr: RocketRAID 17xx/2xxx SATA controller driver v1.2
hptnr: R750/DC7280 controller driver v1.0
acpi0: <APPLE Apple00> on motherboard
ACPI: All ACPI Tables successfully acquired
PCIe: Memory Mapped configuration base @ 0xf0000000
ioapic0: routing intpin 9 (ISA IRQ 9) to lapic 0 vector 48
acpi_ec0: <Embedded Controller: GPE 0x3f, ECDT> port 0x62,0x66 on acpi0
acpi0: Power Button (fixed)
unknown: I/O range not supported
hpet0: <High Precision Event Timer> iomem 0xfed00000-0xfed003ff irq 0,8 on acpi0
hpet0: vendor 0x10de, rev 0x1, 25000000Hz 64bit, 4 timers, legacy route
hpet0:  t0: irqs 0x00ff3efa (31), 64bit, periodic
hpet0:  t1: irqs 0x00ff3efa (31)
hpet0:  t2: irqs 0x00ff3efa (31)
hpet0:  t3: irqs 0x00ff3efa (31)
Timecounter "HPET" frequency 25000000 Hz quality 950
cpu0: Processor \134_PR_.CPU0 (ACPI ID 0) -> APIC ID 0
cpu0: <ACPI CPU> on acpi0
ACPI: SSDT 0xbfec9c18 0027A (v01  APPLE  Cpu0Ist 00003000 INTL 20061109)
ACPI: Dynamic OEM Table Load:
ACPI: SSDT 0 0027A (v01  APPLE  Cpu0Ist 00003000 INTL 20061109)
ACPI: SSDT 0xbfec9918 002AD (v01  APPLE  Cpu0Cst 00003001 INTL 20061109)
ACPI: Dynamic OEM Table Load:
ACPI: SSDT 0 002AD (v01  APPLE  Cpu0Cst 00003001 INTL 20061109)
cpu1: Processor \134_PR_.CPU1 (ACPI ID 1) -> APIC ID 1
cpu1: <ACPI CPU> on acpi0
ACPI: SSDT 0xbfec9f18 000C8 (v01  APPLE  Cpu1Ist 00003000 INTL 20061109)
ACPI: Dynamic OEM Table Load:
ACPI: SSDT 0 000C8 (v01  APPLE  Cpu1Ist 00003000 INTL 20061109)
ACPI: SSDT 0xbfec8f18 00085 (v01  APPLE  Cpu1Cst 00003000 INTL 20061109)
ACPI: Dynamic OEM Table Load:
ACPI: SSDT 0 00085 (v01  APPLE  Cpu1Cst 00003000 INTL 20061109)
atrtc0: <AT realtime clock> port 0x70-0x77 on acpi0
atrtc0: registered as a time-of-day clock (resolution 1000000us, adjustment 0.500000000s)
ioapic0: routing intpin 8 (ISA IRQ 8) to lapic 0 vector 49
Event timer "RTC" frequency 32768 Hz quality 0
attimer0: <AT timer> port 0x40-0x43 on acpi0
Timecounter "i8254" frequency 1193182 Hz quality 0
ioapic0: routing intpin 2 (ISA IRQ 0) to lapic 0 vector 50
Event timer "i8254" frequency 1193182 Hz quality 100
ACPI timer: 1/1 1/1 0/1 1/1 1/1 1/1 1/1 1/1 1/1 1/1 -> 9
Timecounter "ACPI-safe" frequency 3579545 Hz quality 850
acpi_timer0: <24-bit timer at 3.579545MHz> port 0x408-0x40b on acpi0
pci_link0:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  5 7 10 11 14 15
  Validation          0  255   N     0  5 7 10 11 14 15
  After Disable       0  255   N     0  5 7 10 11 14 15
pci_link1:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  5 7 10 11 14 15
  Validation          0  255   N     0  5 7 10 11 14 15
  After Disable       0  255   N     0  5 7 10 11 14 15
pci_link2:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  5 7 10 11 14 15
  Validation          0  255   N     0  5 7 10 11 14 15
  After Disable       0  255   N     0  5 7 10 11 14 15
pci_link3:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  5 7 10 11 14 15
  Validation          0  255   N     0  5 7 10 11 14 15
  After Disable       0  255   N     0  5 7 10 11 14 15
pci_link4:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link5:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link6:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link7:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link8:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link9:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link10:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link11:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link12:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link13:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link14:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link15:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link16:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   10   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link17:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link18:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link19:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link20:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0    7   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link21:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link22:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link23:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link24:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link25:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link26:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link27:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link28:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link29:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link30:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link31:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link32:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   15   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link33:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   11   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link34:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   10   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link35:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   14   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link36:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   15   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link37:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   11   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link38:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link39:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   11   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link40:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link41:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0    7   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link42:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0    5   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
pci_link43:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   14   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
acpi_acad0: <AC Adapter> on acpi0
acpi_lid0: <Control Method Lid Switch> on acpi0
acpi_button0: <Power Button> on acpi0
acpi_button1: <Sleep Button> on acpi0
pcib0: <ACPI Host-PCI bridge> on acpi0
pcib0: decoding 4 range 0-0xcf7
pcib0: decoding 4 range 0xd00-0xffff
pcib0: decoding 3 range 0xa0000-0xbffff
pcib0: decoding 3 range 0xc0000-0xc3fff
pcib0: decoding 3 range 0xc4000-0xc7fff
pcib0: decoding 3 range 0xc8000-0xcbfff
pcib0: decoding 3 range 0xcc000-0xcffff
pcib0: decoding 3 range 0xd0000-0xd3fff
pcib0: decoding 3 range 0xd4000-0xd7fff
pcib0: decoding 3 range 0xd8000-0xdbfff
pcib0: decoding 3 range 0xdc000-0xdffff
pcib0: decoding 3 range 0xe0000-0xe3fff
pcib0: decoding 3 range 0xe4000-0xe7fff
pcib0: decoding 3 range 0xe8000-0xebfff
pcib0: decoding 3 range 0xec000-0xeffff
pcib0: decoding 3 range 0xf0000-0xfffff
pcib0: decoding 3 range 0xc0000000-0xfebfffff
pci0: <ACPI PCI bus> on pcib0
pci0: domain=0, physical bus=0
found->	vendor=0x10de, dev=0x0a82, revid=0xb1
	domain=0, bus=0, slot=0, func=0
	class=06-00-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0006, statreg=0x00a0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
found->	vendor=0x10de, dev=0x0a88, revid=0xb1
	domain=0, bus=0, slot=0, func=1
	class=05-00-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0004, statreg=0x00a0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
found->	vendor=0x10de, dev=0x0aae, revid=0xb3
	domain=0, bus=0, slot=3, func=0
	class=06-01-00, hdrtype=0x00, mfdev=1
	cmdreg=0x000f, statreg=0x00a0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	map[10]: type I/O Port, range 32, base 0x2000, size  8, enabled
pcib0: allocated type 4 (0x2000-0x20ff) for rid 10 of pci0:0:3:0
found->	vendor=0x10de, dev=0x0aa4, revid=0xb1
	domain=0, bus=0, slot=3, func=1
	class=05-00-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0400, statreg=0x00a0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
found->	vendor=0x10de, dev=0x0aa2, revid=0xb1
	domain=0, bus=0, slot=3, func=2
	class=0c-05-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0001, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=15
	powerspec 2  supports D0 D3  current D0
	map[10]: type I/O Port, range 32, base 0x2180, size  6, enabled
pcib0: allocated type 4 (0x2180-0x21bf) for rid 10 of pci0:0:3:2
	map[20]: type I/O Port, range 32, base 0x2140, size  6, enabled
pcib0: allocated type 4 (0x2140-0x217f) for rid 20 of pci0:0:3:2
	map[24]: type I/O Port, range 32, base 0x2100, size  6, enabled
pcib0: allocated type 4 (0x2100-0x213f) for rid 24 of pci0:0:3:2
pcib0: matched entry for 0.3.INTA (src \134_SB_.PCI0.LSMB:0)
pci_link32: Picked IRQ 16 with weight 0
pcib0: slot 3 INTA routed to irq 16 via \134_SB_.PCI0.LSMB
found->	vendor=0x10de, dev=0x0a89, revid=0xb1
	domain=0, bus=0, slot=3, func=3
	class=05-00-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0000, statreg=0x0020, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
found->	vendor=0x10de, dev=0x0a98, revid=0xb1
	domain=0, bus=0, slot=3, func=4
	class=05-00-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0400, statreg=0x00a0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
found->	vendor=0x10de, dev=0x0aa3, revid=0xb1
	domain=0, bus=0, slot=3, func=5
	class=0b-40-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0006, statreg=0x00a0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x03 (750 ns), maxlat=0x01 (250 ns)
	intpin=b, irq=14
	map[10]: type Memory, range 32, base 0xd3400000, size 19, enabled
pcib0: allocated type 3 (0xd3400000-0xd347ffff) for rid 10 of pci0:0:3:5
pcib0: matched entry for 0.3.INTB (src \134_SB_.PCI0.LPMU:0)
pci_link43: Picked IRQ 17 with weight 0
pcib0: slot 3 INTB routed to irq 17 via \134_SB_.PCI0.LPMU
found->	vendor=0x10de, dev=0x0aa5, revid=0xb1
	domain=0, bus=0, slot=4, func=0
	class=0c-03-10, hdrtype=0x00, mfdev=1
	cmdreg=0x0007, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x03 (750 ns), maxlat=0x01 (250 ns)
	intpin=a, irq=11
	powerspec 2  supports D0 D1 D2 D3  current D0
	map[10]: type Memory, range 32, base 0xd3488000, size 12, enabled
pcib0: allocated type 3 (0xd3488000-0xd3488fff) for rid 10 of pci0:0:4:0
pcib0: matched entry for 0.4.INTA (src \134_SB_.PCI0.LUS0:0)
pci_link33: Picked IRQ 18 with weight 0
pcib0: slot 4 INTA routed to irq 18 via \134_SB_.PCI0.LUS0
ohci early: SMM active, request owner change
found->	vendor=0x10de, dev=0x0aa6, revid=0xb1
	domain=0, bus=0, slot=4, func=1
	class=0c-03-20, hdrtype=0x00, mfdev=1
	cmdreg=0x0006, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x03 (750 ns), maxlat=0x01 (250 ns)
	intpin=b, irq=10
	powerspec 2  supports D0 D1 D2 D3  current D0
	map[10]: type Memory, range 32, base 0xd3489200, size  8, enabled
pcib0: allocated type 3 (0xd3489200-0xd34892ff) for rid 10 of pci0:0:4:1
pcib0: matched entry for 0.4.INTB (src \134_SB_.PCI0.LUS2:0)
pci_link34: Picked IRQ 19 with weight 0
pcib0: slot 4 INTB routed to irq 19 via \134_SB_.PCI0.LUS2
found->	vendor=0x10de, dev=0x0aa7, revid=0xb1
	domain=0, bus=0, slot=6, func=0
	class=0c-03-10, hdrtype=0x00, mfdev=1
	cmdreg=0x0007, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x03 (750 ns), maxlat=0x01 (250 ns)
	intpin=a, irq=7
	powerspec 2  supports D0 D1 D2 D3  current D0
	map[10]: type Memory, range 32, base 0xd3487000, size 12, enabled
pcib0: allocated type 3 (0xd3487000-0xd3487fff) for rid 10 of pci0:0:6:0
pcib0: matched entry for 0.6.INTA (src \134_SB_.PCI0.Z000:0)
pci_link41: Picked IRQ 20 with weight 0
pcib0: slot 6 INTA routed to irq 20 via \134_SB_.PCI0.Z000
found->	vendor=0x10de, dev=0x0aa9, revid=0xb1
	domain=0, bus=0, slot=6, func=1
	class=0c-03-20, hdrtype=0x00, mfdev=1
	cmdreg=0x0006, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x03 (750 ns), maxlat=0x01 (250 ns)
	intpin=b, irq=5
	powerspec 2  supports D0 D1 D2 D3  current D0
	map[10]: type Memory, range 32, base 0xd3489100, size  8, enabled
pcib0: allocated type 3 (0xd3489100-0xd34891ff) for rid 10 of pci0:0:6:1
pcib0: matched entry for 0.6.INTB (src \134_SB_.PCI0.Z001:0)
pci_link42: Picked IRQ 21 with weight 0
pcib0: slot 6 INTB routed to irq 21 via \134_SB_.PCI0.Z001
found->	vendor=0x10de, dev=0x0ac0, revid=0xb1
	domain=0, bus=0, slot=8, func=0
	class=04-03-00, hdrtype=0x00, mfdev=0
	cmdreg=0x0006, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x02 (500 ns), maxlat=0x05 (1250 ns)
	intpin=a, irq=15
	powerspec 2  supports D0 D3  current D0
	map[10]: type Memory, range 32, base 0xd3480000, size 14, enabled
pcib0: allocated type 3 (0xd3480000-0xd3483fff) for rid 10 of pci0:0:8:0
pcib0: matched entry for 0.8.INTA (src \134_SB_.PCI0.LAZA:0)
pci_link36: Picked IRQ 22 with weight 0
pcib0: slot 8 INTA routed to irq 22 via \134_SB_.PCI0.LAZA
found->	vendor=0x10de, dev=0x0aab, revid=0xb1
	domain=0, bus=0, slot=9, func=0
	class=06-04-01, hdrtype=0x01, mfdev=0
	cmdreg=0x0000, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x02 (500 ns)
found->	vendor=0x10de, dev=0x0ab0, revid=0xb1
	domain=0, bus=0, slot=10, func=0
	class=02-00-00, hdrtype=0x00, mfdev=0
	cmdreg=0x0007, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x01 (250 ns), maxlat=0x14 (5000 ns)
	intpin=a, irq=14
	powerspec 2  supports D0 D1 D2 D3  current D0
	MSI supports 16 messages, 64 bit, vector masks
	map[10]: type Memory, range 32, base 0xd3486000, size 12, enabled
pcib0: allocated type 3 (0xd3486000-0xd3486fff) for rid 10 of pci0:0:10:0
	map[14]: type I/O Port, range 32, base 0x21e0, size  3, enabled
pcib0: allocated type 4 (0x21e0-0x21e7) for rid 14 of pci0:0:10:0
	map[18]: type Memory, range 32, base 0xd3489000, size  8, enabled
pcib0: allocated type 3 (0xd3489000-0xd34890ff) for rid 18 of pci0:0:10:0
	map[1c]: type Memory, range 32, base 0xd3489300, size  4, enabled
pcib0: allocated type 3 (0xd3489300-0xd348930f) for rid 1c of pci0:0:10:0
pcib0: matched entry for 0.10.INTA (src \134_SB_.PCI0.LMAC:0)
pci_link35: Picked IRQ 23 with weight 0
pcib0: slot 10 INTA routed to irq 23 via \134_SB_.PCI0.LMAC
found->	vendor=0x10de, dev=0x0ab5, revid=0xb1
	domain=0, bus=0, slot=11, func=0
	class=01-01-85, hdrtype=0x00, mfdev=0
	cmdreg=0x0007, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x03 (750 ns), maxlat=0x01 (250 ns)
	intpin=a, irq=11
	powerspec 2  supports D0 D3  current D0
	MSI supports 8 messages, 64 bit
	map[10]: type I/O Port, range 32, base 0x21d8, size  3, enabled
pcib0: allocated type 4 (0x21d8-0x21df) for rid 10 of pci0:0:11:0
	map[14]: type I/O Port, range 32, base 0x21ec, size  2, enabled
pcib0: allocated type 4 (0x21ec-0x21ef) for rid 14 of pci0:0:11:0
	map[18]: type I/O Port, range 32, base 0x21d0, size  3, enabled
pcib0: allocated type 4 (0x21d0-0x21d7) for rid 18 of pci0:0:11:0
	map[1c]: type I/O Port, range 32, base 0x21e8, size  2, enabled
pcib0: allocated type 4 (0x21e8-0x21eb) for rid 1c of pci0:0:11:0
	map[20]: type I/O Port, range 32, base 0x21c0, size  4, enabled
pcib0: allocated type 4 (0x21c0-0x21cf) for rid 20 of pci0:0:11:0
	map[24]: type Memory, range 32, base 0xd3484000, size 13, enabled
pcib0: allocated type 3 (0xd3484000-0xd3485fff) for rid 24 of pci0:0:11:0
pcib0: matched entry for 0.11.INTA (src \134_SB_.PCI0.LSI0:0)
pci_link39: Picked IRQ 16 with weight 1
pcib0: slot 11 INTA routed to irq 16 via \134_SB_.PCI0.LSI0
found->	vendor=0x10de, dev=0x0aa0, revid=0xb1
	domain=0, bus=0, slot=16, func=0
	class=06-04-00, hdrtype=0x01, mfdev=0
	cmdreg=0x0007, statreg=0x0010, cachelnsz=64 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x08 (2000 ns), maxlat=0x00 (0 ns)
	powerspec 2  supports D0 D3  current D0
	MSI supports 2 messages, 64 bit
found->	vendor=0x10de, dev=0x0ac6, revid=0xb1
	domain=0, bus=0, slot=21, func=0
	class=06-04-00, hdrtype=0x01, mfdev=0
	cmdreg=0x0007, statreg=0x0010, cachelnsz=64 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=255
	powerspec 3  supports D0 D3  current D0
	MSI supports 2 messages, 64 bit
found->	vendor=0x10de, dev=0x0ac7, revid=0xb1
	domain=0, bus=0, slot=22, func=0
	class=06-04-00, hdrtype=0x01, mfdev=0
	cmdreg=0x0007, statreg=0x0010, cachelnsz=64 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=255
	powerspec 3  supports D0 D3  current D0
	MSI supports 2 messages, 64 bit
CPU0: local APIC error 0x80
CPU0: local APIC error 0x80
CPU0: local APIC error 0x80
CPU0: local APIC error 0x80
CPU0: local APIC error 0x80
CPU0: local APIC error 0x80
pci0: <memory, RAM> at device 0.1 (no driver attached)
isab0: <PCI-ISA bridge> port 0x2000-0x20ff at device 3.0 on pci0
isa0: <ISA bus> on isab0
pci0: <memory, RAM> at device 3.1 (no driver attached)
pci0: <serial bus, SMBus> at device 3.2 (no driver attached)
pci0: <memory, RAM> at device 3.3 (no driver attached)
pci0: <memory, RAM> at device 3.4 (no driver attached)
pci0: <processor> at device 3.5 (no driver attached)
ohci0: <nVidia nForce MCP79 USB Controller> mem 0xd3488000-0xd3488fff irq 18 at device 4.0 on pci0
ioapic0: routing intpin 18 (PCI IRQ 18) to lapic 0 vector 51
usbus0 on ohci0
ohci0: usbpf: Attached
ehci0: <NVIDIA nForce MCP79 USB 2.0 controller> mem 0xd3489200-0xd34892ff irq 19 at device 4.1 on pci0
ioapic0: routing intpin 19 (PCI IRQ 19) to lapic 0 vector 52
ehci0: Doorbell workaround enabled
usbus1: EHCI version 1.0
usbus1 on ehci0
ehci0: usbpf: Attached
ohci1: <nVidia nForce MCP79 USB Controller> mem 0xd3487000-0xd3487fff irq 20 at device 6.0 on pci0
ioapic0: routing intpin 20 (PCI IRQ 20) to lapic 0 vector 53
usbus2 on ohci1
ohci1: usbpf: Attached
ehci1: <NVIDIA nForce MCP79 USB 2.0 controller> mem 0xd3489100-0xd34891ff irq 21 at device 6.1 on pci0
ioapic0: routing intpin 21 (PCI IRQ 21) to lapic 0 vector 54
ehci1: Doorbell workaround enabled
usbus3: EHCI version 1.0
usbus3 on ehci1
ehci1: usbpf: Attached
hdac0: <NVIDIA MCP79 HDA Controller> mem 0xd3480000-0xd3483fff irq 22 at device 8.0 on pci0
hdac0: PCI card vendor: 0x10de, device: 0xcb79
hdac0: HDA Driver Revision: 20120126_0002
hdac0: Config options: on=0x00000000 off=0x00000000
ioapic0: routing intpin 22 (PCI IRQ 22) to lapic 0 vector 55
hdac0: Caps: OSS 4, ISS 4, BSS 0, NSDO 1, 64bit, CORB 256, RIRB 256
pcib1: <PCI-PCI bridge> at device 9.0 on pci0
pcib0: allocated type 3 (0xd3300000-0xd33fffff) for rid 20 of pcib1
pcib1:   domain            0
pcib1:   secondary bus     1
pcib1:   subordinate bus   1
pcib1:   memory decode     0xd3300000-0xd33fffff
pcib1:   special decode    subtractive
pci1: <PCI bus> on pcib1
pci1: domain=0, physical bus=1
nfe0: <NVIDIA nForce MCP79 Networking Adapter> port 0x21e0-0x21e7 mem 0xd3486000-0xd3486fff,0xd3489000-0xd34890ff,0xd3489300-0xd348930f irq 23 at device 10.0 on pci0
miibus0: <MII bus> on nfe0
rgephy0: <RTL8169S/8110S/8211 1000BASE-T media interface> PHY 1 on miibus0
rgephy0: OUI 0x00e04c, model 0x0011, rev. 2
rgephy0:  none, 10baseT, 10baseT-FDX, 10baseT-FDX-flow, 100baseTX, 100baseTX-FDX, 100baseTX-FDX-flow, 1000baseT, 1000baseT-master, 1000baseT-FDX, 1000baseT-FDX-master, 1000baseT-FDX-flow, 1000baseT-FDX-flow-master, auto, auto-flow
nfe0: bpf attached
nfe0: Ethernet address: 00:25:bc:e1:70:fe
ioapic0: routing intpin 23 (PCI IRQ 23) to lapic 0 vector 56
ahci0: <NVIDIA MCP79 AHCI SATA controller> port 0x21d8-0x21df,0x21ec-0x21ef,0x21d0-0x21d7,0x21e8-0x21eb,0x21c0-0x21cf mem 0xd3484000-0xd3485fff irq 16 at device 11.0 on pci0
ahci0: attempting to allocate 1 MSI vectors (8 supported)
msi: routing MSI IRQ 256 to local APIC 0 vector 57
ahci0: using IRQ 256 for MSI
ahci0: AHCI v1.20 with 6 3Gbps ports, Port Multiplier supported
ahci0: quirks=0x200<NOAA>
ahci0: Caps: 64bit NCQ SNTF ALP AL 3Gbps PM PMD SSC PSC 32cmd 6ports
ahci0: Caps2: BOH
ahcich0: <AHCI channel> at channel 0 on ahci0
ahcich0: Caps:
ahcich1: <AHCI channel> at channel 1 on ahci0
ahcich1: Caps:
ahcich2: not probed (disabled)
ahcich3: not probed (disabled)
ahcich4: not probed (disabled)
ahcich5: not probed (disabled)
pcib2: <ACPI PCI-PCI bridge> at device 16.0 on pci0
pcib0: allocated type 4 (0x1000-0x1fff) for rid 1c of pcib2
pcib0: allocated type 3 (0xd2000000-0xd30fffff) for rid 20 of pcib2
pcib0: allocated type 3 (0xc0000000-0xd1ffffff) for rid 24 of pcib2
pcib2:   domain            0
pcib2:   secondary bus     2
pcib2:   subordinate bus   2
pcib2:   I/O decode        0x1000-0x1fff
pcib2:   memory decode     0xd2000000-0xd30fffff
pcib2:   prefetched decode 0xc0000000-0xd1ffffff
pcib2:   special decode    VGA
pci2: <ACPI PCI bus> on pcib2
pci2: domain=0, physical bus=2
found->	vendor=0x10de, dev=0x0863, revid=0xb1
	domain=0, bus=2, slot=0, func=0
	class=03-00-00, hdrtype=0x00, mfdev=0
	cmdreg=0x0007, statreg=0x0010, cachelnsz=64 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=11
	powerspec 2  supports D0 D3  current D0
	MSI supports 1 message, 64 bit
	map[10]: type Memory, range 32, base 0xd2000000, size 24, enabled
pcib2: allocated memory range (0xd2000000-0xd2ffffff) for rid 10 of pci0:2:0:0
	map[14]: type Prefetchable Memory, range 64, base 0xc0000000, size 28, enabled
pcib2: allocated prefetch range (0xc0000000-0xcfffffff) for rid 14 of pci0:2:0:0
	map[1c]: type Prefetchable Memory, range 64, base 0xd0000000, size 25, enabled
pcib2: allocated prefetch range (0xd0000000-0xd1ffffff) for rid 1c of pci0:2:0:0
	map[24]: type I/O Port, range 32, base 0x1000, size  7, enabled
pcib2: allocated I/O port range (0x1000-0x107f) for rid 24 of pci0:2:0:0
pcib2: matched entry for 2.0.INTA (src \134_SB_.PCI0.LGPU:0)
pci_link37: Picked IRQ 17 with weight 1
pcib2: slot 0 INTA routed to irq 17 via \134_SB_.PCI0.LGPU
vgapci0: <VGA-compatible display> port 0x1000-0x107f mem 0xd2000000-0xd2ffffff,0xc0000000-0xcfffffff,0xd0000000-0xd1ffffff irq 17 at device 0.0 on pci2
nvidia0: <GeForce 9400M> on vgapci0
vgapci0: child nvidia0 requested pci_enable_io
vgapci0: attempting to allocate 1 MSI vectors (1 supported)
msi: routing MSI IRQ 257 to local APIC 0 vector 58
vgapci0: using IRQ 257 for MSI
vgapci0: child nvidia0 requested pci_enable_io
vgapci0: Boot video device
pcib3: <ACPI PCI-PCI bridge> at device 21.0 on pci0
pcib0: allocated type 3 (0xd3200000-0xd32fffff) for rid 20 of pcib3
pcib3:   domain            0
pcib3:   secondary bus     3
pcib3:   subordinate bus   3
pcib3:   memory decode     0xd3200000-0xd32fffff
pcib3: could not get PCI interrupt routing table for \134_SB_.PCI0.RP04 - AE_NOT_FOUND
pci3: <ACPI PCI bus> on pcib3
pci3: domain=0, physical bus=3
found->	vendor=0x14e4, dev=0x432b, revid=0x01
	domain=0, bus=3, slot=0, func=0
	class=02-80-00, hdrtype=0x00, mfdev=0
	cmdreg=0x0006, statreg=0x0010, cachelnsz=64 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=10
	powerspec 3  supports D0 D1 D2 D3  current D0
	MSI supports 1 message, 64 bit
	map[10]: type Memory, range 64, base 0xd3200000, size 14, enabled
pcib3: allocated memory range (0xd3200000-0xd3203fff) for rid 10 of pci0:3:0:0
pcib0: matched entry for 0.21.INTA (src \134_SB_.PCI0.Z00F:0)
pci_link16: Picked IRQ 18 with weight 1
pcib0: slot 21 INTA routed to irq 18 via \134_SB_.PCI0.Z00F
pcib3: slot 0 INTA is routed to irq 18
pci3: <network> at device 0.0 (no driver attached)
pcib4: <ACPI PCI-PCI bridge> at device 22.0 on pci0
pcib0: allocated type 3 (0xd3100000-0xd31fffff) for rid 20 of pcib4
pcib4:   domain            0
pcib4:   secondary bus     4
pcib4:   subordinate bus   4
pcib4:   memory decode     0xd3100000-0xd31fffff
pcib4: could not get PCI interrupt routing table for \134_SB_.PCI0.RP05 - AE_NOT_FOUND
pci4: <ACPI PCI bus> on pcib4
pci4: domain=0, physical bus=4
found->	vendor=0x11c1, dev=0x5901, revid=0x07
	domain=0, bus=4, slot=0, func=0
	class=0c-00-10, hdrtype=0x00, mfdev=0
	cmdreg=0x0007, statreg=0x0010, cachelnsz=64 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=7
	powerspec 3  supports D0 D1 D2 D3  current D0
	MSI supports 1 message, 64 bit
	map[10]: type Memory, range 64, base 0xd3100000, size 12, enabled
pcib4: allocated memory range (0xd3100000-0xd3100fff) for rid 10 of pci0:4:0:0
pcib0: matched entry for 0.22.INTA (src \134_SB_.PCI0.Z00J:0)
pci_link20: Picked IRQ 19 with weight 1
pcib0: slot 22 INTA routed to irq 19 via \134_SB_.PCI0.Z00J
pcib4: slot 0 INTA is routed to irq 19
pci4: <serial bus, FireWire> at device 0.0 (no driver attached)
battery0: <ACPI Control Method Battery> on acpi0
ACPI: Enabled 3 GPEs in block 00 to 1F
ACPI: Enabled 3 GPEs in block 20 to 5F
acpi0: wakeup code va 0xfffffe0225934000 pa 0x90000
ahc_isa_identify 0: ioport 0xc00 alloc failed
ahc_isa_identify 1: ioport 0x1c00 alloc failed
ahc_isa_identify 2: ioport 0x2c00 alloc failed
ahc_isa_identify 3: ioport 0x3c00 alloc failed
ahc_isa_identify 4: ioport 0x4c00 alloc failed
ahc_isa_identify 5: ioport 0x5c00 alloc failed
ahc_isa_identify 6: ioport 0x6c00 alloc failed
ahc_isa_identify 7: ioport 0x7c00 alloc failed
ahc_isa_identify 8: ioport 0x8c00 alloc failed
ahc_isa_identify 9: ioport 0x9c00 alloc failed
ahc_isa_identify 10: ioport 0xac00 alloc failed
ahc_isa_identify 11: ioport 0xbc00 alloc failed
ahc_isa_identify 12: ioport 0xcc00 alloc failed
ahc_isa_identify 13: ioport 0xdc00 alloc failed
ahc_isa_identify 14: ioport 0xec00 alloc failed
ex_isa_identify()
pcib0: allocated type 3 (0xa0000-0xa07ff) for rid 0 of orm0
pcib0: allocated type 3 (0xa0800-0xa0fff) for rid 0 of orm0
pcib0: allocated type 3 (0xa1000-0xa17ff) for rid 0 of orm0
pcib0: allocated type 3 (0xa1800-0xa1fff) for rid 0 of orm0
pcib0: allocated type 3 (0xa2000-0xa27ff) for rid 0 of orm0
pcib0: allocated type 3 (0xa2800-0xa2fff) for rid 0 of orm0
pcib0: allocated type 3 (0xa3000-0xa37ff) for rid 0 of orm0
pcib0: allocated type 3 (0xa3800-0xa3fff) for rid 0 of orm0
pcib0: allocated type 3 (0xa4000-0xa47ff) for rid 0 of orm0
pcib0: allocated type 3 (0xa4800-0xa4fff) for rid 0 of orm0
pcib0: allocated type 3 (0xa5000-0xa57ff) for rid 0 of orm0
pcib0: allocated type 3 (0xa5800-0xa5fff) for rid 0 of orm0
pcib0: allocated type 3 (0xa6000-0xa67ff) for rid 0 of orm0
pcib0: allocated type 3 (0xa6800-0xa6fff) for rid 0 of orm0
pcib0: allocated type 3 (0xa7000-0xa77ff) for rid 0 of orm0
pcib0: allocated type 3 (0xa7800-0xa7fff) for rid 0 of orm0
pcib0: allocated type 3 (0xa8000-0xa87ff) for rid 0 of orm0
pcib0: allocated type 3 (0xa8800-0xa8fff) for rid 0 of orm0
pcib0: allocated type 3 (0xa9000-0xa97ff) for rid 0 of orm0
pcib0: allocated type 3 (0xa9800-0xa9fff) for rid 0 of orm0
pcib0: allocated type 3 (0xaa000-0xaa7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xaa800-0xaafff) for rid 0 of orm0
pcib0: allocated type 3 (0xab000-0xab7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xab800-0xabfff) for rid 0 of orm0
pcib0: allocated type 3 (0xac000-0xac7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xac800-0xacfff) for rid 0 of orm0
pcib0: allocated type 3 (0xad000-0xad7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xad800-0xadfff) for rid 0 of orm0
pcib0: allocated type 3 (0xae000-0xae7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xae800-0xaefff) for rid 0 of orm0
pcib0: allocated type 3 (0xaf000-0xaf7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xaf800-0xaffff) for rid 0 of orm0
pcib0: allocated type 3 (0xb0000-0xb07ff) for rid 0 of orm0
pcib0: allocated type 3 (0xb0800-0xb0fff) for rid 0 of orm0
pcib0: allocated type 3 (0xb1000-0xb17ff) for rid 0 of orm0
pcib0: allocated type 3 (0xb1800-0xb1fff) for rid 0 of orm0
pcib0: allocated type 3 (0xb2000-0xb27ff) for rid 0 of orm0
pcib0: allocated type 3 (0xb2800-0xb2fff) for rid 0 of orm0
pcib0: allocated type 3 (0xb3000-0xb37ff) for rid 0 of orm0
pcib0: allocated type 3 (0xb3800-0xb3fff) for rid 0 of orm0
pcib0: allocated type 3 (0xb4000-0xb47ff) for rid 0 of orm0
pcib0: allocated type 3 (0xb4800-0xb4fff) for rid 0 of orm0
pcib0: allocated type 3 (0xb5000-0xb57ff) for rid 0 of orm0
pcib0: allocated type 3 (0xb5800-0xb5fff) for rid 0 of orm0
pcib0: allocated type 3 (0xb6000-0xb67ff) for rid 0 of orm0
pcib0: allocated type 3 (0xb6800-0xb6fff) for rid 0 of orm0
pcib0: allocated type 3 (0xb7000-0xb77ff) for rid 0 of orm0
pcib0: allocated type 3 (0xb7800-0xb7fff) for rid 0 of orm0
pcib0: allocated type 3 (0xb8000-0xb87ff) for rid 0 of orm0
pcib0: allocated type 3 (0xb8800-0xb8fff) for rid 0 of orm0
pcib0: allocated type 3 (0xb9000-0xb97ff) for rid 0 of orm0
pcib0: allocated type 3 (0xb9800-0xb9fff) for rid 0 of orm0
pcib0: allocated type 3 (0xba000-0xba7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xba800-0xbafff) for rid 0 of orm0
pcib0: allocated type 3 (0xbb000-0xbb7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xbb800-0xbbfff) for rid 0 of orm0
pcib0: allocated type 3 (0xbc000-0xbc7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xbc800-0xbcfff) for rid 0 of orm0
pcib0: allocated type 3 (0xbd000-0xbd7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xbd800-0xbdfff) for rid 0 of orm0
pcib0: allocated type 3 (0xbe000-0xbe7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xbe800-0xbefff) for rid 0 of orm0
pcib0: allocated type 3 (0xbf000-0xbf7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xbf800-0xbffff) for rid 0 of orm0
pcib0: allocated type 3 (0xc0000-0xc07ff) for rid 0 of orm0
pcib0: allocated type 3 (0xce800-0xcefff) for rid 1 of orm0
pcib0: allocated type 3 (0xcf000-0xcf7ff) for rid 1 of orm0
pcib0: allocated type 3 (0xcf800-0xcffff) for rid 1 of orm0
pcib0: allocated type 3 (0xd0000-0xd07ff) for rid 1 of orm0
pcib0: allocated type 3 (0xd0800-0xd0fff) for rid 1 of orm0
pcib0: allocated type 3 (0xd1000-0xd17ff) for rid 1 of orm0
pcib0: allocated type 3 (0xd1800-0xd1fff) for rid 1 of orm0
pcib0: allocated type 3 (0xd2000-0xd27ff) for rid 1 of orm0
pcib0: allocated type 3 (0xd2800-0xd2fff) for rid 1 of orm0
pcib0: allocated type 3 (0xd3000-0xd37ff) for rid 1 of orm0
pcib0: allocated type 3 (0xd3800-0xd3fff) for rid 1 of orm0
pcib0: allocated type 3 (0xd4000-0xd47ff) for rid 1 of orm0
pcib0: allocated type 3 (0xd4800-0xd4fff) for rid 1 of orm0
pcib0: allocated type 3 (0xd5000-0xd57ff) for rid 1 of orm0
pcib0: allocated type 3 (0xd5800-0xd5fff) for rid 1 of orm0
pcib0: allocated type 3 (0xd6000-0xd67ff) for rid 1 of orm0
pcib0: allocated type 3 (0xd6800-0xd6fff) for rid 1 of orm0
pcib0: allocated type 3 (0xd7000-0xd77ff) for rid 1 of orm0
pcib0: allocated type 3 (0xd7800-0xd7fff) for rid 1 of orm0
pcib0: allocated type 3 (0xd8000-0xd87ff) for rid 1 of orm0
pcib0: allocated type 3 (0xd8800-0xd8fff) for rid 1 of orm0
pcib0: allocated type 3 (0xd9000-0xd97ff) for rid 1 of orm0
pcib0: allocated type 3 (0xd9800-0xd9fff) for rid 1 of orm0
pcib0: allocated type 3 (0xda000-0xda7ff) for rid 1 of orm0
pcib0: allocated type 3 (0xda800-0xdafff) for rid 1 of orm0
pcib0: allocated type 3 (0xdb000-0xdb7ff) for rid 1 of orm0
pcib0: allocated type 3 (0xdb800-0xdbfff) for rid 1 of orm0
pcib0: allocated type 3 (0xdc000-0xdc7ff) for rid 1 of orm0
pcib0: allocated type 3 (0xdc800-0xdcfff) for rid 1 of orm0
pcib0: allocated type 3 (0xdd000-0xdd7ff) for rid 1 of orm0
pcib0: allocated type 3 (0xdd800-0xddfff) for rid 1 of orm0
pcib0: allocated type 3 (0xde000-0xde7ff) for rid 1 of orm0
pcib0: allocated type 3 (0xde800-0xdefff) for rid 1 of orm0
pcib0: allocated type 3 (0xdf000-0xdf7ff) for rid 1 of orm0
pcib0: allocated type 3 (0xdf800-0xdffff) for rid 1 of orm0
pcib0: allocated type 3 (0xe0000-0xe07ff) for rid 1 of orm0
pcib0: allocated type 3 (0xe0800-0xe0fff) for rid 1 of orm0
pcib0: allocated type 3 (0xe1000-0xe17ff) for rid 1 of orm0
pcib0: allocated type 3 (0xe1800-0xe1fff) for rid 1 of orm0
pcib0: allocated type 3 (0xe2000-0xe27ff) for rid 1 of orm0
pcib0: allocated type 3 (0xe2800-0xe2fff) for rid 1 of orm0
pcib0: allocated type 3 (0xe3000-0xe37ff) for rid 1 of orm0
pcib0: allocated type 3 (0xe3800-0xe3fff) for rid 1 of orm0
pcib0: allocated type 3 (0xe4000-0xe47ff) for rid 1 of orm0
pcib0: allocated type 3 (0xe4800-0xe4fff) for rid 1 of orm0
pcib0: allocated type 3 (0xe5000-0xe57ff) for rid 1 of orm0
pcib0: allocated type 3 (0xe5800-0xe5fff) for rid 1 of orm0
pcib0: allocated type 3 (0xe6000-0xe67ff) for rid 1 of orm0
pcib0: allocated type 3 (0xe6800-0xe6fff) for rid 1 of orm0
pcib0: allocated type 3 (0xe7000-0xe77ff) for rid 1 of orm0
pcib0: allocated type 3 (0xe7800-0xe7fff) for rid 1 of orm0
pcib0: allocated type 3 (0xe8000-0xe87ff) for rid 1 of orm0
pcib0: allocated type 3 (0xe8800-0xe8fff) for rid 1 of orm0
pcib0: allocated type 3 (0xe9000-0xe97ff) for rid 1 of orm0
pcib0: allocated type 3 (0xe9800-0xe9fff) for rid 1 of orm0
pcib0: allocated type 3 (0xea000-0xea7ff) for rid 1 of orm0
pcib0: allocated type 3 (0xea800-0xeafff) for rid 1 of orm0
pcib0: allocated type 3 (0xeb000-0xeb7ff) for rid 1 of orm0
pcib0: allocated type 3 (0xeb800-0xebfff) for rid 1 of orm0
pcib0: allocated type 3 (0xec000-0xec7ff) for rid 1 of orm0
pcib0: allocated type 3 (0xec800-0xecfff) for rid 1 of orm0
pcib0: allocated type 3 (0xed000-0xed7ff) for rid 1 of orm0
pcib0: allocated type 3 (0xed800-0xedfff) for rid 1 of orm0
pcib0: allocated type 3 (0xee000-0xee7ff) for rid 1 of orm0
pcib0: allocated type 3 (0xee800-0xeefff) for rid 1 of orm0
pcib0: allocated type 3 (0xef000-0xef7ff) for rid 1 of orm0
pcib0: allocated type 3 (0xef800-0xeffff) for rid 1 of orm0
pcib0: allocated type 3 (0xf0000-0xf07ff) for rid 1 of orm0
pcib0: allocated type 3 (0xf0800-0xf0fff) for rid 1 of orm0
pcib0: allocated type 3 (0xf1000-0xf17ff) for rid 1 of orm0
pcib0: allocated type 3 (0xf1800-0xf1fff) for rid 1 of orm0
pcib0: allocated type 3 (0xf2000-0xf27ff) for rid 1 of orm0
pcib0: allocated type 3 (0xf2800-0xf2fff) for rid 1 of orm0
pcib0: allocated type 3 (0xf3000-0xf37ff) for rid 1 of orm0
pcib0: allocated type 3 (0xf3800-0xf3fff) for rid 1 of orm0
pcib0: allocated type 3 (0xf4000-0xf47ff) for rid 1 of orm0
pcib0: allocated type 3 (0xf4800-0xf4fff) for rid 1 of orm0
pcib0: allocated type 3 (0xf5000-0xf57ff) for rid 1 of orm0
pcib0: allocated type 3 (0xf5800-0xf5fff) for rid 1 of orm0
pcib0: allocated type 3 (0xf6000-0xf67ff) for rid 1 of orm0
pcib0: allocated type 3 (0xf6800-0xf6fff) for rid 1 of orm0
pcib0: allocated type 3 (0xf7000-0xf77ff) for rid 1 of orm0
pcib0: allocated type 3 (0xf7800-0xf7fff) for rid 1 of orm0
pcib0: allocated type 3 (0xf8000-0xf87ff) for rid 1 of orm0
pcib0: allocated type 3 (0xf8800-0xf8fff) for rid 1 of orm0
pcib0: allocated type 3 (0xf9000-0xf97ff) for rid 1 of orm0
pcib0: allocated type 3 (0xf9800-0xf9fff) for rid 1 of orm0
pcib0: allocated type 3 (0xfa000-0xfa7ff) for rid 1 of orm0
pcib0: allocated type 3 (0xfa800-0xfafff) for rid 1 of orm0
pcib0: allocated type 3 (0xfb000-0xfb7ff) for rid 1 of orm0
pcib0: allocated type 3 (0xfb800-0xfbfff) for rid 1 of orm0
pcib0: allocated type 3 (0xfc000-0xfc7ff) for rid 1 of orm0
pcib0: allocated type 3 (0xfc800-0xfcfff) for rid 1 of orm0
pcib0: allocated type 3 (0xfd000-0xfd7ff) for rid 1 of orm0
pcib0: allocated type 3 (0xfd800-0xfdfff) for rid 1 of orm0
pcib0: allocated type 3 (0xfe000-0xfe7ff) for rid 1 of orm0
pcib0: allocated type 3 (0xfe800-0xfefff) for rid 1 of orm0
pcib0: allocated type 3 (0xff000-0xff7ff) for rid 1 of orm0
pcib0: allocated type 3 (0xff800-0xfffff) for rid 1 of orm0
isa_probe_children: disabling PnP devices
atrtc: atrtc0 already exists; skipping it
attimer: attimer0 already exists; skipping it
sc: sc0 already exists; skipping it
isa_probe_children: probing non-PnP devices
orm0: <ISA Option ROM> at iomem 0xc0000-0xce7ff on isa0
sc0: <System console> at flags 0x100 on isa0
sc0: VGA <16 virtual consoles, flags=0x300>
sc0: fb0, kbd0, terminal emulator: scteken (teken terminal)
vga0: <Generic ISA VGA> at port 0x3c0-0x3df iomem 0xa0000-0xbffff on isa0
pcib0: allocated type 4 (0x3c0-0x3df) for rid 0 of vga0
pcib0: allocated type 3 (0xa0000-0xbffff) for rid 0 of vga0
pcib0: allocated type 4 (0x60-0x60) for rid 0 of atkbdc0
pcib0: allocated type 4 (0x64-0x64) for rid 1 of atkbdc0
atkbdc0: AT keyboard controller not found
atkbdc0 failed to probe at port 0x60,0x64 on isa0
pcib0: allocated type 4 (0x3f0-0x3f5) for rid 0 of fdc0
pcib0: allocated type 4 (0x3f7-0x3f7) for rid 1 of fdc0
fdc0 failed to probe at port 0x3f0-0x3f5,0x3f7 irq 6 drq 2 on isa0
ppc0: cannot reserve I/O port range
ppc0 failed to probe at irq 7 on isa0
pcib0: allocated type 4 (0x3f8-0x3ff) for rid 0 of uart0
uart0 failed to probe at port 0x3f8-0x3ff irq 4 on isa0
pcib0: allocated type 4 (0x2f8-0x2ff) for rid 0 of uart1
uart1 failed to probe at port 0x2f8-0x2ff irq 3 on isa0
wbwd0 failed to probe on isa0
isa_probe_children: probing PnP devices
est0: <Enhanced SpeedStep Frequency Control> on cpu0
p4tcc0: <CPU Frequency Thermal Control> on cpu0
est1: <Enhanced SpeedStep Frequency Control> on cpu1
p4tcc1: <CPU Frequency Thermal Control> on cpu1
Device configuration finished.
procfs registered
lapic: Divisor 2, Frequency 132670014 Hz
Timecounters tick every 1.000 msec
vlan: initialized, using hash tables with chaining
Linux ELF exec handler installed
tcp_init: net.inet.tcp.tcbhashsize auto tuned to 65536
lo0: bpf attached
hpt27xx: no controller detected.
hptrr: no controller detected.
hptnr: no controller detected.
hdacc0: <Cirrus Logic CS4206 HDA CODEC> at cad 0 on hdac0
hdaa0: <Cirrus Logic CS4206 Audio Function Group> at nid 1 on hdacc0
hdaa0: Subsystem ID: 0x106b4d00
hdaa0: NumGPIO=4 NumGPO=0 NumGPI=0 GPIWake=0 GPIUnsol=0
hdaa0:  GPIO0: disabled
hdaa0:  GPIO1: disabled
hdaa0:  GPIO2: disabled
hdaa0:  GPIO3: output state=0
hdaa0: Original pins configuration:
hdaa0: nid   0x    as seq device       conn  jack    loc        color   misc
hdaa0:  9 012b4030 3  0  Headphones    Jack  Combo   Rear       Green   0
hdaa0: 10 90100121 2  1  Speaker       Fixed Unknown Internal   Unknown 1
hdaa0: 11 90100120 2  0  Speaker       Fixed Unknown Internal   Unknown 1
hdaa0: 12 400000f0 15 0  Line-out      None  Unknown 0x00       Unknown 0
hdaa0: 13 90a00110 1  0  Mic           Fixed Unknown Internal   Unknown 1
hdaa0: 14 400000f0 15 0  Line-out      None  Unknown 0x00       Unknown 0
hdaa0: 15 400000f0 15 0  Line-out      None  Unknown 0x00       Unknown 0
hdaa0: 16 014be040 4  0  SPDIF-out     Jack  Combo   Rear       White   0
hdaa0: 18 400000f0 15 0  Line-out      None  Unknown 0x00       Unknown 0
hdaa0: 21 400000f0 15 0  Line-out      None  Unknown 0x00       Unknown 0
hdaa0: Patched pins configuration:
hdaa0: nid   0x    as seq device       conn  jack    loc        color   misc
hdaa0:  9 012b4030 3  0  Headphones    Jack  Combo   Rear       Green   0
hdaa0: 10 90100121 2  1  Speaker       Fixed Unknown Internal   Unknown 1
hdaa0: 11 90100120 2  0  Speaker       Fixed Unknown Internal   Unknown 1
hdaa0: 12 400000f0 15 0  Line-out      None  Unknown 0x00       Unknown 0 DISA
hdaa0: 13 90a00110 1  0  Mic           Fixed Unknown Internal   Unknown 1
hdaa0: 14 400000f0 15 0  Line-out      None  Unknown 0x00       Unknown 0 DISA
hdaa0: 15 400000f0 15 0  Line-out      None  Unknown 0x00       Unknown 0 DISA
hdaa0: 16 014be040 4  0  SPDIF-out     Jack  Combo   Rear       White   0
hdaa0: 18 400000f0 15 0  Line-out      None  Unknown 0x00       Unknown 0 DISA
hdaa0: 21 400000f0 15 0  Line-out      None  Unknown 0x00       Unknown 0 DISA
hdaa0: 4 associations found:
hdaa0: Association 0 (1) in:
hdaa0:  Pin nid=13 seq=0
hdaa0: Association 1 (2) out:
hdaa0:  Pin nid=11 seq=0
hdaa0:  Pin nid=10 seq=1
hdaa0: Association 2 (3) out:
hdaa0:  Pin nid=9 seq=0
hdaa0: Association 3 (4) out:
hdaa0:  Pin nid=16 seq=0
hdaa0: Tracing association 0 (1)
hdaa0:  Unable to trace pin 13 to ADC 5, undo traces
hdaa0:  Pin 13 traced to ADC 6
hdaa0: Association 0 (1) trace succeeded
hdaa0: Tracing association 1 (2)
hdaa0:  Pin 11 traced to DAC 4
hdaa0:  Pin 10 traced to DAC 3
hdaa0: Association 1 (2) trace succeeded
hdaa0: Tracing association 2 (3)
hdaa0:  Pin 9 traced to DAC 2
hdaa0: Association 2 (3) trace succeeded
hdaa0: Tracing association 3 (4)
hdaa0:  Pin 16 traced to DAC 8
hdaa0: Association 3 (4) trace succeeded
hdaa0: Looking for additional ADC for association 0 (1)
hdaa0: Looking for additional DAC for association 1 (2)
hdaa0: Looking for additional DAC for association 2 (3)
hdaa0: Looking for additional DAC for association 3 (4)
hdaa0: Tracing input monitor
hdaa0: Tracing other input monitors
hdaa0:  Tracing nid 13 to out
hdaa0: Tracing beeper
hdaa0: GPIO commit
hdaa0:  GPIO0: disabled
hdaa0:  GPIO1: output state=1
hdaa0:  GPIO2: disabled
hdaa0:  GPIO3: output state=1
hdaa0: FG config/quirks: forcestereo ivref50 ivref80 ivref100 ivref
pcm0: <Cirrus Logic CS4206 (Internal Analog 3.1/2.0)> at nid 11,10 and 13 on hdaa0
pcm0: Playback:
pcm0:      Stream cap: 0x00000003 FLOAT32 PCM
pcm0:         PCM cap: 0x001e07f0 16 20 24 32 bits, 32 44 48 88 96 176 192 KHz
pcm0:             DAC: 4 3
pcm0: 
pcm0:     nid=11 [pin: Speaker (Fixed)]
pcm0:       + <- nid=4 [audio output] [src: pcm]
pcm0: 
pcm0:     nid=10 [pin: Speaker (Fixed)]
pcm0:       + <- nid=3 [audio output] [src: pcm]
pcm0: 
pcm0: Record:
pcm0:      Stream cap: 0x00000003 FLOAT32 PCM
pcm0:         PCM cap: 0x001e01f5 16 20 24 32 bits, 8 16 32 44 48 88 96 KHz
pcm0:             ADC: 6
pcm0: 
pcm0:     nid=6 [audio input]
pcm0:       + <- nid=13 [pin: Mic (Fixed)] [src: monitor]
pcm0: 
pcm0: Master Volume (OSS: vol): -57/6dB
pcm0:    +- ctl  2 (nid   3 out):    -57/6dB (128 steps) + mute
pcm0:    +- ctl  3 (nid   4 out):    -57/6dB (128 steps) + mute
pcm0: 
pcm0: PCM Volume (OSS: pcm): -57/6dB
pcm0:    +- ctl  2 (nid   3 out):    -57/6dB (128 steps) + mute
pcm0:    +- ctl  3 (nid   4 out):    -57/6dB (128 steps) + mute
pcm0: 
pcm0: Microphone2 Volume (OSS: monitor): 0/30dB
pcm0:    +- ctl  5 (nid   6 in   0): -51/12dB (64 steps) + mute
pcm0:    +- ctl  7 (nid  13 out):    0/30dB (4 steps)
pcm0: 
pcm0: Recording Level (OSS: rec): -51/12dB
pcm0:    +- ctl  5 (nid   6 in   0): -51/12dB (64 steps) + mute
pcm0:    +- ctl  7 (nid  13 out):    0/30dB (4 steps)
pcm0: 
pcm0: Mixer "vol":
pcm0: Mixer "pcm":
pcm0: Mixer "rec":
pcm0: Mixer "monitor":
pcm0: Playback channel set is: Front Left, Front Right, Front Center, Low Frequency Effects, 
pcm0: Playback channel matrix is: 2.0 (unknown)
pcm0: Automatically set rec source to: monitor
pcm0: Recording channel set is: Front Left, Front Right, 
pcm0: Recording channel matrix is: 2.0 (unknown)
pcm1: <Cirrus Logic CS4206 (Rear Analog Headphones)> at nid 9 on hdaa0
pcm1: Playback:
pcm1:      Stream cap: 0x00000003 FLOAT32 PCM
pcm1:         PCM cap: 0x001e07f0 16 20 24 32 bits, 32 44 48 88 96 176 192 KHz
pcm1:             DAC: 2
pcm1: 
pcm1:     nid=9 [pin: Headphones (Green Jack)]
pcm1:       + <- nid=2 [audio output] [src: pcm]
pcm1: 
pcm1: Master Volume (OSS: vol): -57/6dB
pcm1:    +- ctl  1 (nid   2 out):    -57/6dB (128 steps) + mute
pcm1: 
pcm1: PCM Volume (OSS: pcm): -57/6dB
pcm1:    +- ctl  1 (nid   2 out):    -57/6dB (128 steps) + mute
pcm1: 
pcm1: Mixer "vol":
pcm1: Mixer "pcm":
pcm1: Playback channel set is: Front Left, Front Right, 
pcm1: Playback channel matrix is: 2.0 (disconnected)
pcm2: <Cirrus Logic CS4206 (Rear Digital)> at nid 16 on hdaa0
pcm2: Playback:
pcm2:      Stream cap: 0x00000007 AC3 FLOAT32 PCM
pcm2:         PCM cap: 0x001e07f0 16 20 24 32 bits, 32 44 48 88 96 176 192 KHz
pcm2:             DAC: 8
pcm2: 
pcm2:     nid=16 [pin: SPDIF-out (White Jack)]
pcm2:       + <- nid=8 [audio output] [src: pcm]
pcm2: 
pcm2: Mixer "vol" -> "none": child=0x00000010
pcm2: Mixer "pcm": parent="vol"
pcm2: Soft PCM mixer ENABLED
pcm2: Playback channel set is: Front Left, Front Right, 
pcm2: Playback channel matrix is: 2.0 (unknown)
random: unblocking device.
usbus0: 12Mbps Full Speed USB v1.0
usbus1: 480Mbps High Speed USB v2.0
usbus2: 12Mbps Full Speed USB v1.0
usbus3: 480Mbps High Speed USB v2.0
ahcich0: AHCI reset...
ahcich0: SATA connect time=0us status=00000113
ahcich0: AHCI reset: device found
ahcich1: AHCI reset...
ahcich1: SATA connect time=0us status=00000113
ahcich1: AHCI reset: device found
ahcich1: AHCI reset: device ready after 0ms
ugen1.1: <nVidia> at usbus1
uhub0: <nVidia EHCI root HUB, class 9/0, rev 2.00/1.00, addr 1> on usbus1
ugen0.1: <nVidia> at usbus0
uhub1: <nVidia OHCI root HUB, class 9/0, rev 1.00/1.00, addr 1> on usbus0
ugen3.1: <nVidia> at usbus3
uhub2: <nVidia EHCI root HUB, class 9/0, rev 2.00/1.00, addr 1> on usbus3
ugen2.1: <nVidia> at usbus2
uhub3: <nVidia OHCI root HUB, class 9/0, rev 1.00/1.00, addr 1> on usbus2
acpi_acad0: acline initialization start
acpi_acad0: On Line
acpi_acad0: acline initialization done, tried 1 times
battery0: battery initialization start
ahcich0: AHCI reset: device ready after 100ms
pass0 at ahcich0 bus 0 scbus0 target 0 lun 0
pass0: <Hitachi HTS545025B9SA02 PB2AC60Q> ATA-8 SATA 1.x device
pass0: Serial Number 090621PBC200QSH43EMH
pass0: 150.000MB/s transfers (SATA 1.x, UDMA6, PIO 8192bytes)
pass0: Command Queueing enabled
pass1 at ahcich1 bus 0 scbus1 target 0 lun 0
pass1: <HL-DT-ST DVDRW  GS23N SB00> Removable CD-ROM SCSI-0 device 
pass1: Serial Number KZZ96KG1812
pass1: 150.000MB/s transfers (SATA 1.x, UDMA6, ATAPI 12bytes, PIO 8192bytes)
ada0 at ahcich0 bus 0 scbus0 target 0 lun 0
ada0: <Hitachi HTS545025B9SA02 PB2AC60Q> ATA-8 SATA 1.x device
ada0: Serial Number 090621PBC200QSH43EMH
ada0: 150.000MB/s transfers (SATA 1.x, UDMA6, PIO 8192bytes)
ada0: Command Queueing enabled
ada0: 238475MB (488397168 512 byte sectors: 16H 63S/T 16383C)
ada0: Previously was known as ad4
GEOM: new disk ada0
GEOM: new disk cd0
cd0 at ahcich1 bus 0 scbus1 target 0 lun 0
cd0: <HL-DT-ST DVDRW  GS23N SB00> Removable CD-ROM SCSI-0 device 
cd0: Serial Number KZZ96KG1812
cd0: 150.000MB/s transfers (SATA 1.x, UDMA6, ATAPI 12bytes, PIO 8192bytes)
cd0: Attempt to query device size failed: NOT READY, Medium not present
Netvsc initializing... SMP: AP CPU #1 Launched!
cpu1 AP:
     ID: 0x01000000   VER: 0x00050014 LDR: 0x00000000 DFR: 0xffffffff
  lint0: 0x00010700 lint1: 0x00000400 TPR: 0x00000000 SVR: 0x000001ff
  timer: 0x000100ef therm: 0x00010000 err: 0x000000f0 pmc: 0x00010400
ioapic0: routing intpin 9 (ISA IRQ 9) to lapic 1 vector 48
ioapic0: routing intpin 19 (PCI IRQ 19) to lapic 1 vector 49
ioapic0: routing intpin 21 (PCI IRQ 21) to lapic 1 vector 50
ioapic0: routing intpin 23 (PCI IRQ 23) to lapic 1 vector 51
msi: Assigning MSI IRQ 257 to local APIC 1 vector 52
TSC timecounter disabled: C3 enabled.
Timecounter "TSC" frequency 2255389235 Hz quality -1000
uhub3: 5 ports with 5 removable, self powered
uhub1: 7 ports with 7 removable, self powered
Root mount waiting for: usbus3 usbus1
battery0: battery initialization done, tried 1 times
Root mount waiting for: usbus3 usbus1
uhub2: 5 ports with 5 removable, self powered
Root mount waiting for: usbus3 usbus1
uhub0: 7 ports with 7 removable, self powered
Root mount waiting for: usbus3 usbus1
ugen2.2: <Apple Inc.> at usbus2
uhub4: <Apple Inc. BRCM2046 Hub, class 9/0, rev 2.00/1.00, addr 2> on usbus2
ugen3.2: <Apple> at usbus3
umass0: <Apple Card Reader, class 0/0, rev 2.00/98.33, addr 2> on usbus3
umass0:  SCSI over Bulk-Only; quirks = 0x4000
umass0:2:0:-1: Attached to scbus2
(probe0:umass-sim0:0:0:0): Down reving Protocol Version from 2 to 0?
pass2 at umass-sim0 bus 0 scbus2 target 0 lun 0
pass2: <APPLE SD Card Reader 1.00> Removable Direct Access SCSI-0 device 
pass2: Serial Number 000000009833
pass2: 40.000MB/s transfers
GEOM: new disk da0
da0 at umass-sim0 bus 0 scbus2 target 0 lun 0
da0: <APPLE SD Card Reader 1.00> Removable Direct Access SCSI-0 device 
da0: Serial Number 000000009833
da0: 40.000MB/s transfers
da0: Attempt to query device size failed: NOT READY, Medium not present
da0: quirks=0x2<NO_6_BYTE>
da0: Delete methods: <NONE(*)>
ugen1.2: <Apple Inc.> at usbus1
uhub4: 3 ports with 0 removable, self powered
ugen2.3: <Apple Inc.> at usbus2
Trying to mount root from ufs:/dev/ada0s3a [rw]...
start_init: trying /sbin/init
ugen0.2: <Apple Computer, Inc.> at usbus0
ugen2.4: <vendor 0x05ac> at usbus2
ukbd0: <vendor 0x05ac product 0x820a, class 0/0, rev 2.00/1.00, addr 4> on usbus2
kbd: new array size 4
kbd1 at ukbd0
kbd1: ukbd0, generic (0), config:0x0, flags:0x3d0000
ugen0.3: <Apple Inc.> at usbus0
ukbd1: <Apple Internal Keyboard> on usbus0
kbd2 at ukbd1
kbd2: ukbd1, generic (0), config:0x0, flags:0x3d0000
ugen2.5: <vendor 0x05ac> at usbus2
ubt0: <Apple Inc. Bluetooth USB Host Controller, rev 2.00/2.07, addr 3> on usbus2
uhid0: <Apple Computer, Inc. IR Receiver, class 0/0, rev 2.00/0.16, addr 2> on usbus0
uhid1: <Touchpad> on usbus0
ums0: <Touchpad> on usbus0
ums1: <vendor 0x05ac product 0x820b, class 0/0, rev 2.00/1.00, addr 5> on usbus2
ums0: 3 buttons and [XY] coordinates ID=2
ums1: 3 buttons and [XY] coordinates ID=2
WARNING: attempt to domain_add(bluetooth) after domainfinalize()
WARNING: attempt to domain_add(netgraph) after domainfinalize()
ugen2.4: <vendor 0x05ac> at usbus2 (disconnected)
ukbd0: at uhub4, port 2, addr 4 (disconnected)
ugen2.5: <vendor 0x05ac> at usbus2 (disconnected)
ums1: at uhub4, port 3, addr 5 (disconnected)
ugen3.3: <Kingston> at usbus3
umass1: <Kingston DataTraveler 3.0, class 0/0, rev 2.10/1.10, addr 3> on usbus3
umass1:  SCSI over Bulk-Only; quirks = 0x0100
umass1:3:1:-1: Attached to scbus3
pass3 at umass-sim1 bus 1 scbus3 target 0 lun 0
pass3: <Kingston DataTraveler 3.0 PMAP> Removable Direct Access SCSI-6 device 
pass3: Serial Number 60A44C4138CCEDC0396949C0
pass3: 40.000MB/s transfers
GEOM: new disk da1
da1 at umass-sim1 bus 1 scbus3 target 0 lun 0
da1: <Kingston DataTraveler 3.0 PMAP> Removable Direct Access SCSI-6 device 
da1: Serial Number 60A44C4138CCEDC0396949C0
da1: 40.000MB/s transfers
da1: 121195MB (248208384 512 byte sectors: 255H 63S/T 15450C)
da1: quirks=0x2<NO_6_BYTE>
da1: Delete methods: <NONE(*)>
(da1:umass-sim1:1:0:0): PREVENT ALLOW MEDIUM REMOVAL not supported.
