Table 'FACP' at 0xbfeec000
Table 'HPET' at 0xbfeeb000
Table 'APIC' at 0xbfeea000
APIC: Found table at 0xbfeea000
APIC: Using the MADT enumerator.
MADT: Found CPU APIC ID 0 ACPI ID 0: enabled
SMP: Added CPU 0 (AP)
MADT: Found CPU APIC ID 1 ACPI ID 1: enabled
SMP: Added CPU 1 (AP)
Copyright (c) 1992-2016 The FreeBSD Project.
Copyright (c) 1979, 1980, 1983, 1986, 1988, 1989, 1991, 1992, 1993, 1994
	The Regents of the University of California. All rights reserved.
FreeBSD is a registered trademark of The FreeBSD Foundation.
FreeBSD 11.0-RELEASE-p1 #0 r306420: Thu Sep 29 01:43:23 UTC 2016
    root@releng2.nyi.freebsd.org:/usr/obj/usr/src/sys/GENERIC amd64
FreeBSD clang version 3.8.0 (tags/RELEASE_380/final 262564) (based on LLVM 3.8.0)
Table 'FACP' at 0xbfeec000
Table 'HPET' at 0xbfeeb000
Table 'APIC' at 0xbfeea000
Table 'APIC' at 0xbfee9000
Table 'MCFG' at 0xbfee8000
Table 'ASF!' at 0xbfee7000
Table 'SBST' at 0xbfee6000
Table 'ECDT' at 0xbfee5000
Table 'SSDT' at 0xbfeca000
Table 'SSDT' at 0xbfec7000
ACPI: No SRAT table found
PPIM 0: PA=0xc0010000, VA=0xffffffff82210000, size=0x640000, mode=0x1
VT(efifb): resolution 1280x800
Preloaded elf kernel "/boot/kernel/kernel" at 0xffffffff821a9000.
Calibrating TSC clock ... TSC clock: 2255390314 Hz
CPU: Intel(R) Core(TM)2 Duo CPU     P7550  @ 2.26GHz (2255.39-MHz K8-class CPU)
  Origin="GenuineIntel"  Id=0x1067a  Family=0x6  Model=0x17  Stepping=10
  Features=0xbfebfbff<FPU,VME,DE,PSE,TSC,MSR,PAE,MCE,CX8,APIC,SEP,MTRR,PGE,MCA,CMOV,PAT,PSE36,CLFLUSH,DTS,ACPI,MMX,FXSR,SSE,SSE2,SS,HTT,TM,PBE>
  Features2=0xc08e3bd<SSE3,DTES64,MON,DS_CPL,VMX,EST,TM2,SSSE3,CX16,xTPR,PDCM,SSE4.1,XSAVE,OSXSAVE>
  AMD Features=0x20100800<SYSCALL,NX,LM>
  AMD Features2=0x1<LAHF>
  VT-x: Basic Features=0x5a0800<SMM,INS/OUTS>
        Pin-Based Controls=0x3f<ExtINT,NMI,VNMI>
        Primary Processor Controls=0xf7f9fffe<INTWIN,TSCOff,HLT,INVLPG,MWAIT,RDPMC,RDTSC,CR3-LD,CR3-ST,CR8-LD,CR8-ST,TPR,NMIWIN,MOV-DR,IO,IOmap,MSRmap,MONITOR,PAUSE>
        Secondary Processor Controls=0x41<APIC,WBINVD>
        Exit Controls=0x5a0800<PAT-LD,EFER-SV,PTMR-SV>
        Entry Controls=0x5a0800
  TSC: P-state invariant, performance statistics
Instruction TLB: 2M pages, 4-way, 8 entries or 4M pages, 4-way, 4 entries
Instruction TLB: 4 KB Pages, 4-way set associative, 128 entries
64-Byte prefetching
Data TLB0: 4 KByte pages, 4-way associative, 16 entries
Data TLB0: 4 MByte pages, 4-way set associative, 16 entries
2nd-level cache: 3MByte, 12-way set associative, 64 byte line size
1st-level instruction cache: 32 KB, 8-way set associative, 64 byte line size
Data TLB1: 4 KByte pages, 4-way associative, 256 entries
1st-level data cache: 32 KB, 8-way set associative, 64 byte line size
L2 cache: 3072 kbytes, 8-way associative, 64 bytes/line
real memory  = 8589934592 (8192 MB)
Physical memory chunk(s):
0x0000000000010000 - 0x000000000008afff, 503808 bytes (123 pages)
0x0000000000090000 - 0x000000000009ffff, 65536 bytes (16 pages)
0x0000000000100000 - 0x00000000001fffff, 1048576 bytes (256 pages)
0x00000000021f5000 - 0x00000000ad38ffff, 2870587392 bytes (700827 pages)
0x00000000ad391000 - 0x00000000ae6f6fff, 20340736 bytes (4966 pages)
0x00000000ae6fc000 - 0x00000000ae721fff, 155648 bytes (38 pages)
0x00000000ae723000 - 0x00000000ae727fff, 20480 bytes (5 pages)
0x00000000ae729000 - 0x00000000ae72afff, 8192 bytes (2 pages)
0x00000000ae92c000 - 0x00000000aefc4fff, 6918144 bytes (1689 pages)
0x00000000aefc6000 - 0x00000000aeffffff, 237568 bytes (58 pages)
0x00000000bf000000 - 0x00000000bf017fff, 98304 bytes (24 pages)
0x00000000bf019000 - 0x00000000bf0a9fff, 593920 bytes (145 pages)
0x00000000bf0ad000 - 0x00000000bf0aefff, 8192 bytes (2 pages)
0x00000000bf0b1000 - 0x00000000bf0b2fff, 8192 bytes (2 pages)
0x00000000bf0b8000 - 0x00000000bf0b9fff, 8192 bytes (2 pages)
0x00000000bf0bb000 - 0x00000000bf0c2fff, 32768 bytes (8 pages)
0x00000000bf0c5000 - 0x00000000bf0c6fff, 8192 bytes (2 pages)
0x00000000bf0c9000 - 0x00000000bf10dfff, 282624 bytes (69 pages)
0x00000000bf112000 - 0x00000000bf119fff, 32768 bytes (8 pages)
0x00000000bf11d000 - 0x00000000bf11efff, 8192 bytes (2 pages)
0x00000000bf120000 - 0x00000000bf224fff, 1069056 bytes (261 pages)
0x00000000bf226000 - 0x00000000bf226fff, 4096 bytes (1 pages)
0x00000000bf23d000 - 0x00000000bf241fff, 20480 bytes (5 pages)
0x00000000bf243000 - 0x00000000bf264fff, 139264 bytes (34 pages)
0x00000000bf268000 - 0x00000000bf26ffff, 32768 bytes (8 pages)
0x00000000bf275000 - 0x00000000bf276fff, 8192 bytes (2 pages)
0x00000000bf278000 - 0x00000000bf278fff, 4096 bytes (1 pages)
0x00000000bf27c000 - 0x00000000bf27ffff, 16384 bytes (4 pages)
0x00000000bf281000 - 0x00000000bf709fff, 4755456 bytes (1161 pages)
0x00000000bf70b000 - 0x00000000bf714fff, 40960 bytes (10 pages)
0x00000000bf717000 - 0x00000000bf718fff, 8192 bytes (2 pages)
0x00000000bf71a000 - 0x00000000bfe92fff, 7835648 bytes (1913 pages)
0x00000000bfe94000 - 0x00000000bfe9dfff, 40960 bytes (10 pages)
0x00000000bfe9f000 - 0x00000000bfec4fff, 155648 bytes (38 pages)
0x00000000bfeef000 - 0x00000000bfef8fff, 40960 bytes (10 pages)
0x0000000100000000 - 0x00000002314d0fff, 5122101248 bytes (1250513 pages)
avail memory = 7981740032 (7611 MB)
Event timer "LAPIC" quality 400
LAPIC: ipi_wait() us multiplier 55 (r 4100230 tsc 2255390314)
ACPI APIC Table: <APPLE  Apple00>
Package ID shift: 1
L2 cache ID shift: 1
L1 cache ID shift: 0
Core ID shift: 0
INTR: Adding local APIC 1 as a target
FreeBSD/SMP: Multiprocessor System Detected: 2 CPUs
FreeBSD/SMP: 1 package(s) x 2 core(s)
Package HW ID = 0 (0)
	Core HW ID = 0 (0)
		CPU0 (BSP): APIC ID: 0 (0)
	Core HW ID = 1 (0x1)
		CPU1 (AP): APIC ID: 1 (0x1)
APIC: CPU 0 has ACPI ID 0
APIC: CPU 1 has ACPI ID 1
x86bios:  IVT 0x000000-0x0004ff at 0xfffff80000000000
x86bios: SSEG 0x08a000-0x08afff at 0xfffffe01e11a7000
x86bios:  ROM 0x0a0000-0x0fefff at 0xfffff800000a0000
ULE: setup cpu 0
ULE: setup cpu 1
ACPI: RSDP 0x00000000BFEEE014 000024 (v02 APPLE )
ACPI: XSDT 0x00000000BFEEE1C0 000074 (v01 APPLE  Apple00  000000AC      01000013)
ACPI: FACP 0x00000000BFEEC000 0000F4 (v04 APPLE  Apple00  000000AC Loki 0000005F)
ACPI: DSDT 0x00000000BFEDF000 005B9E (v01 APPLE  MacBookP 00050005 INTL 20061109)
ACPI: FACS 0x00000000BFECD000 000040
ACPI: FACS 0x00000000BFECD000 000040
ACPI: HPET 0x00000000BFEEB000 000038 (v01 APPLE  Apple00  00000001 Loki 0000005F)
ACPI: APIC 0x00000000BFEEA000 000068 (v01 APPLE  Apple00  00000001 Loki 0000005F)
ACPI: APIC 0x00000000BFEE9000 000068 (v02 APPLE  Apple00  00000001 Loki 0000005F)
ACPI: MCFG 0x00000000BFEE8000 00003C (v01 APPLE  Apple00  00000001 Loki 0000005F)
ACPI: ASF! 0x00000000BFEE7000 0000A5 (v32 APPLE  Apple00  00000001 Loki 0000005F)
ACPI: SBST 0x00000000BFEE6000 000030 (v01 APPLE  Apple00  00000001 Loki 0000005F)
ACPI: ECDT 0x00000000BFEE5000 000053 (v01 APPLE  Apple00  00000001 Loki 0000005F)
ACPI: SSDT 0x00000000BFECA000 00023A (v00        SataAhci 00001000 INTL 20061109)
ACPI: SSDT 0x00000000BFEC7000 0004DC (v01 APPLE  CpuPm    00003000 INTL 20061109)
MADT: Found IO APIC ID 1, Interrupt 0 at 0xfec00000
ioapic0: Changing APIC ID to 1
ioapic0: ver 0x11 maxredir 0x17
ioapic0: Routing external 8259A's -> intpin 0
MADT: Interrupt override: source 0, irq 2
ioapic0: Routing IRQ 0 -> intpin 2
MADT: Interrupt override: source 9, irq 9
ioapic0: intpin 9 trigger: level
lapic0: Routing NMI -> LINT1
lapic0: LINT1 trigger: edge
lapic0: LINT1 polarity: high
lapic1: Routing NMI -> LINT1
lapic1: LINT1 trigger: edge
lapic1: LINT1 polarity: high
ioapic0 <Version 1.1> irqs 0-23 on motherboard
cpu0 BSP:
     ID: 0x00000000   VER: 0x00050014 LDR: 0x00000000 DFR: 0xffffffff
  lint0: 0x00010700 lint1: 0x00000400 TPR: 0x00000000 SVR: 0x000001ff
  timer: 0x000100ef therm: 0x00010000 err: 0x000000f0 pmc: 0x00010400
wlan: <802.11 Link Layer>
snd_unit_init() u=0x00ff8000 [512] d=0x00007c00 [32] c=0x000003ff [1024]
feeder_register: snd_unit=-1 snd_maxautovchans=16 latency=5 feeder_rate_min=1 feeder_rate_max=2016000 feeder_rate_round=25
random: entropy device external interface
kbd0 at kbdmux0
mem: <memory>
nfslock: pseudo-device
crypto: <crypto core>
netmap: loaded module
null: <full device, null device, zero device>
module_register_init: MOD_LOAD (vesa, 0xffffffff8101c950, 0) error 19
io: <I/O>
hpt27xx: RocketRAID 27xx controller driver v1.2.7
hptnr: R750/DC7280 controller driver v1.1.4
hptrr: RocketRAID 17xx/2xxx SATA controller driver v1.2
random: harvesting attach, 8 bytes (4 bits) from ram0
cryptosoft0: <software crypto> on motherboard
crypto: assign cryptosoft0 driver id 0, flags 100663296
crypto: cryptosoft0 registers alg 1 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 2 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 3 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 4 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 5 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 16 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 6 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 7 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 18 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 19 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 20 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 8 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 15 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 9 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 10 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 13 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 14 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 11 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 22 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 23 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 25 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 24 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 26 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 27 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 28 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 21 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 17 flags 0 maxoplen 0
random: harvesting attach, 8 bytes (4 bits) from cryptosoft0
acpi0: <APPLE Apple00> on motherboard
ACPI: 3 ACPI AML tables successfully acquired and loaded

PCIe: Memory Mapped configuration base @ 0xf0000000
ioapic0: routing intpin 9 (ISA IRQ 9) to lapic 0 vector 48
acpi_ec0: <Embedded Controller: GPE 0x3f, ECDT> port 0x62,0x66 on acpi0
random: harvesting attach, 8 bytes (4 bits) from acpi_ec0
acpi0: Power Button (fixed)
unknown: I/O range not supported
random: harvesting attach, 8 bytes (4 bits) from acpi_sysresource0
hpet0: <High Precision Event Timer> iomem 0xfed00000-0xfed003ff irq 0,8 on acpi0
hpet0: vendor 0x10de, rev 0x1, 25000000Hz 64bit, 4 timers, legacy route
hpet0:  t0: irqs 0x00ff3efa (31), 64bit, periodic
hpet0:  t1: irqs 0x00ff3efa (31)
hpet0:  t2: irqs 0x00ff3efa (31)
hpet0:  t3: irqs 0x00ff3efa (31)
Timecounter "HPET" frequency 25000000 Hz quality 950
random: harvesting attach, 8 bytes (4 bits) from hpet0
random: harvesting attach, 8 bytes (4 bits) from acpi_sysresource1
cpu0: Processor \134_PR_.CPU0 (ACPI ID 0) -> APIC ID 0
cpu0: <ACPI CPU> on acpi0
ACPI: Dynamic OEM Table Load:
ACPI: SSDT 0xFFFFF80004394C00 00027A (v01 APPLE  Cpu0Ist  00003000 INTL 20061109)
ACPI: Dynamic OEM Table Load:
ACPI: SSDT 0xFFFFF80004394800 0002AD (v01 APPLE  Cpu0Cst  00003001 INTL 20061109)
random: harvesting attach, 8 bytes (4 bits) from cpu0
cpu1: Processor \134_PR_.CPU1 (ACPI ID 1) -> APIC ID 1
cpu1: <ACPI CPU> on acpi0
ACPI: Dynamic OEM Table Load:
ACPI: SSDT 0xFFFFF8000438B200 0000C8 (v01 APPLE  Cpu1Ist  00003000 INTL 20061109)
ACPI: Dynamic OEM Table Load:
ACPI: SSDT 0xFFFFF8000438B100 000085 (v01 APPLE  Cpu1Cst  00003000 INTL 20061109)
random: harvesting attach, 8 bytes (4 bits) from cpu1
atrtc0: <AT realtime clock> port 0x70-0x77 on acpi0
atrtc0: registered as a time-of-day clock (resolution 1000000us, adjustment 0.500000000s)
ioapic0: routing intpin 8 (ISA IRQ 8) to lapic 0 vector 49
Event timer "RTC" frequency 32768 Hz quality 0
random: harvesting attach, 8 bytes (4 bits) from atrtc0
attimer0: <AT timer> port 0x40-0x43 on acpi0
Timecounter "i8254" frequency 1193182 Hz quality 0
ioapic0: routing intpin 2 (ISA IRQ 0) to lapic 0 vector 50
Event timer "i8254" frequency 1193182 Hz quality 100
random: harvesting attach, 8 bytes (4 bits) from attimer0
ACPI timer: 1/1 0/1 1/1 1/1 1/1 1/1 1/1 1/1 1/1 1/1 -> 9
Timecounter "ACPI-safe" frequency 3579545 Hz quality 850
acpi_timer0: <24-bit timer at 3.579545MHz> port 0x408-0x40b on acpi0
random: harvesting attach, 8 bytes (4 bits) from acpi_timer0
pci_link0:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   16   N     0  5 7 10 11 14 15
  Validation          0  255   N     0  5 7 10 11 14 15
  After Disable       0  255   N     0  5 7 10 11 14 15
random: harvesting attach, 8 bytes (4 bits) from pci_link0
pci_link1:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   16   N     0  5 7 10 11 14 15
  Validation          0  255   N     0  5 7 10 11 14 15
  After Disable       0  255   N     0  5 7 10 11 14 15
random: harvesting attach, 8 bytes (4 bits) from pci_link1
pci_link2:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   16   N     0  5 7 10 11 14 15
  Validation          0  255   N     0  5 7 10 11 14 15
  After Disable       0  255   N     0  5 7 10 11 14 15
random: harvesting attach, 8 bytes (4 bits) from pci_link2
pci_link3:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   16   N     0  5 7 10 11 14 15
  Validation          0  255   N     0  5 7 10 11 14 15
  After Disable       0  255   N     0  5 7 10 11 14 15
random: harvesting attach, 8 bytes (4 bits) from pci_link3
pci_link4:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   16   N     0  16 17 18 19 20 21 22 23
  Validation          0   16   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link4
pci_link5:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   16   N     0  16 17 18 19 20 21 22 23
  Validation          0   16   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link5
pci_link6:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   16   N     0  16 17 18 19 20 21 22 23
  Validation          0   16   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link6
pci_link7:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   16   N     0  16 17 18 19 20 21 22 23
  Validation          0   16   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link7
pci_link8:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link8
pci_link9:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link9
pci_link10:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link10
pci_link11:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link11
pci_link12:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link12
pci_link13:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link13
pci_link14:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link14
pci_link15:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link15
pci_link16:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   21   N     0  16 17 18 19 20 21 22 23
  Validation          0   21   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link16
pci_link17:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   21   N     0  16 17 18 19 20 21 22 23
  Validation          0   21   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link17
pci_link18:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   21   N     0  16 17 18 19 20 21 22 23
  Validation          0   21   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link18
pci_link19:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   21   N     0  16 17 18 19 20 21 22 23
  Validation          0   21   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link19
pci_link20:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   19   N     0  16 17 18 19 20 21 22 23
  Validation          0   19   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link20
pci_link21:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   19   N     0  16 17 18 19 20 21 22 23
  Validation          0   19   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link21
pci_link22:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   19   N     0  16 17 18 19 20 21 22 23
  Validation          0   19   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link22
pci_link23:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   19   N     0  16 17 18 19 20 21 22 23
  Validation          0   19   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link23
pci_link24:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   23   N     0  16 17 18 19 20 21 22 23
  Validation          0   23   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link24
pci_link25:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   23   N     0  16 17 18 19 20 21 22 23
  Validation          0   23   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link25
pci_link26:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   23   N     0  16 17 18 19 20 21 22 23
  Validation          0   23   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link26
pci_link27:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   23   N     0  16 17 18 19 20 21 22 23
  Validation          0   23   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link27
pci_link28:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   23   N     0  16 17 18 19 20 21 22 23
  Validation          0   23   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link28
pci_link29:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   23   N     0  16 17 18 19 20 21 22 23
  Validation          0   23   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link29
pci_link30:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   23   N     0  16 17 18 19 20 21 22 23
  Validation          0   23   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link30
pci_link31:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   23   N     0  16 17 18 19 20 21 22 23
  Validation          0   23   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link31
pci_link32:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   22   N     0  16 17 18 19 20 21 22 23
  Validation          0   22   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link32
pci_link33:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   17   N     0  16 17 18 19 20 21 22 23
  Validation          0   17   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link33
pci_link34:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   22   N     0  16 17 18 19 20 21 22 23
  Validation          0   22   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link34
pci_link35:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   17   N     0  16 17 18 19 20 21 22 23
  Validation          0   17   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link35
pci_link36:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   20   N     0  16 17 18 19 20 21 22 23
  Validation          0   20   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link36
pci_link37:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   16   N     0  16 17 18 19 20 21 22 23
  Validation          0   16   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link37
pci_link38:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link38
pci_link39:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   18   N     0  16 17 18 19 20 21 22 23
  Validation          0   18   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link39
pci_link40:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   18   N     0  16 17 18 19 20 21 22 23
  Validation          0   18   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link40
pci_link41:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   18   N     0  16 17 18 19 20 21 22 23
  Validation          0   18   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link41
pci_link42:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   23   N     0  16 17 18 19 20 21 22 23
  Validation          0   23   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link42
pci_link43:       Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  16 17 18 19 20 21 22 23
  Validation          0  255   N     0  16 17 18 19 20 21 22 23
  After Disable       0  255   N     0  16 17 18 19 20 21 22 23
random: harvesting attach, 8 bytes (4 bits) from pci_link43
acpi_acad0: <AC Adapter> on acpi0
random: harvesting attach, 8 bytes (4 bits) from acpi_acad0
acpi_lid0: <Control Method Lid Switch> on acpi0
random: harvesting attach, 8 bytes (4 bits) from acpi_lid0
acpi_button0: <Power Button> on acpi0
random: harvesting attach, 8 bytes (4 bits) from acpi_button0
acpi_button1: <Sleep Button> on acpi0
random: harvesting attach, 8 bytes (4 bits) from acpi_button1
pcib0: <ACPI Host-PCI bridge> on acpi0
pcib0: _OSC returned error 0x10
pcib0: decoding 5 range 0-0xff
pcib0: decoding 4 range 0-0xcf7
pcib0: decoding 4 range 0xd00-0xffff
pcib0: decoding 3 range 0xa0000-0xbffff
pcib0: decoding 3 range 0xc0000-0xc3fff
pcib0: decoding 3 range 0xc4000-0xc7fff
pcib0: decoding 3 range 0xc8000-0xcbfff
pcib0: decoding 3 range 0xcc000-0xcffff
pcib0: decoding 3 range 0xd0000-0xd3fff
pcib0: decoding 3 range 0xd4000-0xd7fff
pcib0: decoding 3 range 0xd8000-0xdbfff
pcib0: decoding 3 range 0xdc000-0xdffff
pcib0: decoding 3 range 0xe0000-0xe3fff
pcib0: decoding 3 range 0xe4000-0xe7fff
pcib0: decoding 3 range 0xe8000-0xebfff
pcib0: decoding 3 range 0xec000-0xeffff
pcib0: decoding 3 range 0xf0000-0xfffff
pcib0: decoding 3 range 0xc0000000-0xfebfffff
pci0: <ACPI PCI bus> on pcib0
pci0: domain=0, physical bus=0
found->	vendor=0x10de, dev=0x0a82, revid=0xb1
	domain=0, bus=0, slot=0, func=0
	class=06-00-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0006, statreg=0x00a0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
found->	vendor=0x10de, dev=0x0a88, revid=0xb1
	domain=0, bus=0, slot=0, func=1
	class=05-00-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0004, statreg=0x00a0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
found->	vendor=0x10de, dev=0x0aae, revid=0xb3
	domain=0, bus=0, slot=3, func=0
	class=06-01-00, hdrtype=0x00, mfdev=1
	cmdreg=0x000f, statreg=0x00a0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	map[10]: type I/O Port, range 32, base 0x2000, size  8, enabled
pcib0: allocated type 4 (0x2000-0x20ff) for rid 10 of pci0:0:3:0
found->	vendor=0x10de, dev=0x0aa4, revid=0xb1
	domain=0, bus=0, slot=3, func=1
	class=05-00-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0400, statreg=0x00a0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
found->	vendor=0x10de, dev=0x0aa2, revid=0xb1
	domain=0, bus=0, slot=3, func=2
	class=0c-05-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0000, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=255
	powerspec 2  supports D0 D3  current D0
	map[10]: type I/O Port, range 32, base 0x2180, size  6, port disabled
pcib0: allocated type 4 (0x2180-0x21bf) for rid 10 of pci0:0:3:2
	map[20]: type I/O Port, range 32, base 0x2140, size  6, enabled
pcib0: allocated type 4 (0x2140-0x217f) for rid 20 of pci0:0:3:2
	map[24]: type I/O Port, range 32, base 0x2100, size  6, enabled
pcib0: allocated type 4 (0x2100-0x213f) for rid 24 of pci0:0:3:2
found->	vendor=0x10de, dev=0x0a89, revid=0xb1
	domain=0, bus=0, slot=3, func=3
	class=05-00-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0000, statreg=0x0020, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
found->	vendor=0x10de, dev=0x0a98, revid=0xb1
	domain=0, bus=0, slot=3, func=4
	class=05-00-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0400, statreg=0x00a0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
found->	vendor=0x10de, dev=0x0aa3, revid=0xb1
	domain=0, bus=0, slot=3, func=5
	class=0b-40-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0006, statreg=0x00a0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x03 (750 ns), maxlat=0x01 (250 ns)
	intpin=b, irq=255
	map[10]: type Memory, range 32, base 0xd3400000, size 19, enabled
pcib0: allocated type 3 (0xd3400000-0xd347ffff) for rid 10 of pci0:0:3:5
found->	vendor=0x10de, dev=0x0aa5, revid=0xb1
	domain=0, bus=0, slot=4, func=0
	class=0c-03-10, hdrtype=0x00, mfdev=1
	cmdreg=0x0007, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x03 (750 ns), maxlat=0x01 (250 ns)
	intpin=a, irq=255
	powerspec 2  supports D0 D1 D2 D3  current D0
	map[10]: type Memory, range 32, base 0xd3488000, size 12, enabled
pcib0: allocated type 3 (0xd3488000-0xd3488fff) for rid 10 of pci0:0:4:0
found->	vendor=0x10de, dev=0x0aa6, revid=0xb1
	domain=0, bus=0, slot=4, func=1
	class=0c-03-20, hdrtype=0x00, mfdev=1
	cmdreg=0x0006, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x03 (750 ns), maxlat=0x01 (250 ns)
	intpin=b, irq=255
	powerspec 2  supports D0 D1 D2 D3  current D0
	map[10]: type Memory, range 32, base 0xd3489200, size  8, enabled
pcib0: allocated type 3 (0xd3489200-0xd34892ff) for rid 10 of pci0:0:4:1
found->	vendor=0x10de, dev=0x0aa7, revid=0xb1
	domain=0, bus=0, slot=6, func=0
	class=0c-03-10, hdrtype=0x00, mfdev=1
	cmdreg=0x0007, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x03 (750 ns), maxlat=0x01 (250 ns)
	intpin=a, irq=255
	powerspec 2  supports D0 D1 D2 D3  current D0
	map[10]: type Memory, range 32, base 0xd3487000, size 12, enabled
pcib0: allocated type 3 (0xd3487000-0xd3487fff) for rid 10 of pci0:0:6:0
found->	vendor=0x10de, dev=0x0aa9, revid=0xb1
	domain=0, bus=0, slot=6, func=1
	class=0c-03-20, hdrtype=0x00, mfdev=1
	cmdreg=0x0006, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x03 (750 ns), maxlat=0x01 (250 ns)
	intpin=b, irq=255
	powerspec 2  supports D0 D1 D2 D3  current D0
	map[10]: type Memory, range 32, base 0xd3489100, size  8, enabled
pcib0: allocated type 3 (0xd3489100-0xd34891ff) for rid 10 of pci0:0:6:1
found->	vendor=0x10de, dev=0x0ac0, revid=0xb1
	domain=0, bus=0, slot=8, func=0
	class=04-03-00, hdrtype=0x00, mfdev=0
	cmdreg=0x0000, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x02 (500 ns), maxlat=0x05 (1250 ns)
	intpin=a, irq=255
	powerspec 2  supports D0 D3  current D0
	map[10]: type Memory, range 32, base 0xd3480000, size 14, memory disabled
pcib0: allocated type 3 (0xd3480000-0xd3483fff) for rid 10 of pci0:0:8:0
found->	vendor=0x10de, dev=0x0aab, revid=0xb1
	domain=0, bus=0, slot=9, func=0
	class=06-04-01, hdrtype=0x01, mfdev=0
	cmdreg=0x0000, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	secbus=1, subbus=1
found->	vendor=0x10de, dev=0x0ab0, revid=0xb1
	domain=0, bus=0, slot=10, func=0
	class=02-00-00, hdrtype=0x00, mfdev=0
	cmdreg=0x0007, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x01 (250 ns), maxlat=0x14 (5000 ns)
	intpin=a, irq=255
	powerspec 2  supports D0 D1 D2 D3  current D0
	MSI supports 16 messages, 64 bit, vector masks
	map[10]: type Memory, range 32, base 0xd3486000, size 12, enabled
pcib0: allocated type 3 (0xd3486000-0xd3486fff) for rid 10 of pci0:0:10:0
	map[14]: type I/O Port, range 32, base 0x21e0, size  3, enabled
pcib0: allocated type 4 (0x21e0-0x21e7) for rid 14 of pci0:0:10:0
	map[18]: type Memory, range 32, base 0xd3489000, size  8, enabled
pcib0: allocated type 3 (0xd3489000-0xd34890ff) for rid 18 of pci0:0:10:0
	map[1c]: type Memory, range 32, base 0xd3489300, size  4, enabled
pcib0: allocated type 3 (0xd3489300-0xd348930f) for rid 1c of pci0:0:10:0
found->	vendor=0x10de, dev=0x0ab9, revid=0xb1
	domain=0, bus=0, slot=11, func=0
	class=01-06-01, hdrtype=0x00, mfdev=0
	cmdreg=0x0007, statreg=0x00b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x03 (750 ns), maxlat=0x01 (250 ns)
	intpin=a, irq=255
	powerspec 2  supports D0 D3  current D0
	MSI supports 8 messages, 64 bit
	map[10]: type I/O Port, range 32, base 0x21d8, size  3, enabled
pcib0: allocated type 4 (0x21d8-0x21df) for rid 10 of pci0:0:11:0
	map[14]: type I/O Port, range 32, base 0x21ec, size  2, enabled
pcib0: allocated type 4 (0x21ec-0x21ef) for rid 14 of pci0:0:11:0
	map[18]: type I/O Port, range 32, base 0x21d0, size  3, enabled
pcib0: allocated type 4 (0x21d0-0x21d7) for rid 18 of pci0:0:11:0
	map[1c]: type I/O Port, range 32, base 0x21e8, size  2, enabled
pcib0: allocated type 4 (0x21e8-0x21eb) for rid 1c of pci0:0:11:0
	map[20]: type I/O Port, range 32, base 0x21c0, size  4, enabled
pcib0: allocated type 4 (0x21c0-0x21cf) for rid 20 of pci0:0:11:0
	map[24]: type Memory, range 32, base 0xd3484000, size 13, enabled
pcib0: allocated type 3 (0xd3484000-0xd3485fff) for rid 24 of pci0:0:11:0
found->	vendor=0x10de, dev=0x0aa0, revid=0xb1
	domain=0, bus=0, slot=16, func=0
	class=06-04-00, hdrtype=0x01, mfdev=0
	cmdreg=0x0007, statreg=0x0010, cachelnsz=64 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	powerspec 2  supports D0 D3  current D0
	MSI supports 2 messages, 64 bit
	secbus=2, subbus=2
found->	vendor=0x10de, dev=0x0ac6, revid=0xb1
	domain=0, bus=0, slot=21, func=0
	class=06-04-00, hdrtype=0x01, mfdev=0
	cmdreg=0x0007, statreg=0x0010, cachelnsz=64 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=255
	powerspec 3  supports D0 D3  current D0
	MSI supports 2 messages, 64 bit
	secbus=3, subbus=3
found->	vendor=0x10de, dev=0x0ac7, revid=0xb1
	domain=0, bus=0, slot=22, func=0
	class=06-04-00, hdrtype=0x01, mfdev=0
	cmdreg=0x0007, statreg=0x0010, cachelnsz=64 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=255
	powerspec 3  supports D0 D3  current D0
	MSI supports 2 messages, 64 bit
	secbus=4, subbus=4
CPU0: local APIC error 0x80
CPU0: local APIC error 0x80
CPU0: local APIC error 0x80
CPU0: local APIC error 0x80
CPU0: local APIC error 0x80
CPU0: local APIC error 0x80
random: harvesting attach, 8 bytes (4 bits) from hostb0
pci0: <memory, RAM> at device 0.1 (no driver attached)
isab0: <PCI-ISA bridge> port 0x2000-0x20ff at device 3.0 on pci0
isa0: <ISA bus> on isab0
random: harvesting attach, 8 bytes (4 bits) from isa0
random: harvesting attach, 8 bytes (4 bits) from isab0
pci0: <memory, RAM> at device 3.1 (no driver attached)
pci0: <serial bus, SMBus> at device 3.2 (no driver attached)
pci0: <memory, RAM> at device 3.3 (no driver attached)
pci0: <memory, RAM> at device 3.4 (no driver attached)
pci0: <processor> at device 3.5 (no driver attached)
ohci0: <nVidia nForce MCP79 USB Controller> mem 0xd3488000-0xd3488fff at device 4.0 on pci0
pcib0: matched entry for 0.4.INTA (src \134_SB_.PCI0.LUS0:0)
pcib0: slot 4 INTA routed to irq 17 via \134_SB_.PCI0.LUS0
ioapic0: routing intpin 17 (PCI IRQ 17) to lapic 0 vector 51
usbus0 on ohci0
ohci0: usbpf: Attached
random: harvesting attach, 8 bytes (4 bits) from usbus0
random: harvesting attach, 8 bytes (4 bits) from ohci0
ehci0: <NVIDIA nForce MCP79 USB 2.0 controller> mem 0xd3489200-0xd34892ff at device 4.1 on pci0
pcib0: matched entry for 0.4.INTB (src \134_SB_.PCI0.LUS2:0)
pcib0: slot 4 INTB routed to irq 22 via \134_SB_.PCI0.LUS2
ioapic0: routing intpin 22 (PCI IRQ 22) to lapic 0 vector 52
ehci0: Doorbell workaround enabled
usbus1: EHCI version 1.0
usbus1 on ehci0
ehci0: usbpf: Attached
random: harvesting attach, 8 bytes (4 bits) from usbus1
random: harvesting attach, 8 bytes (4 bits) from ehci0
ohci1: <nVidia nForce MCP79 USB Controller> mem 0xd3487000-0xd3487fff at device 6.0 on pci0
pcib0: matched entry for 0.6.INTA (src \134_SB_.PCI0.Z000:0)
pcib0: slot 6 INTA routed to irq 18 via \134_SB_.PCI0.Z000
ioapic0: routing intpin 18 (PCI IRQ 18) to lapic 0 vector 53
usbus2 on ohci1
ohci1: usbpf: Attached
random: harvesting attach, 8 bytes (4 bits) from usbus2
random: harvesting attach, 8 bytes (4 bits) from ohci1
ehci1: <NVIDIA nForce MCP79 USB 2.0 controller> mem 0xd3489100-0xd34891ff at device 6.1 on pci0
pcib0: matched entry for 0.6.INTB (src \134_SB_.PCI0.Z001:0)
pcib0: slot 6 INTB routed to irq 23 via \134_SB_.PCI0.Z001
ioapic0: routing intpin 23 (PCI IRQ 23) to lapic 0 vector 54
ehci1: Doorbell workaround enabled
usbus3: EHCI version 1.0
usbus3 on ehci1
ehci1: usbpf: Attached
random: harvesting attach, 8 bytes (4 bits) from usbus3
random: harvesting attach, 8 bytes (4 bits) from ehci1
hdac0: <NVIDIA MCP79 HDA Controller> mem 0xd3480000-0xd3483fff at device 8.0 on pci0
hdac0: PCI card vendor: 0x10de, device: 0xcb79
hdac0: HDA Driver Revision: 20120126_0002
hdac0: Config options: on=0x00000000 off=0x00000000
pcib0: matched entry for 0.8.INTA (src \134_SB_.PCI0.LAZA:0)
pcib0: slot 8 INTA routed to irq 20 via \134_SB_.PCI0.LAZA
ioapic0: routing intpin 20 (PCI IRQ 20) to lapic 0 vector 55
hdac0: Caps: OSS 4, ISS 4, BSS 0, NSDO 1, 64bit, CORB 256, RIRB 256
random: harvesting attach, 8 bytes (4 bits) from hdac0
pcib1: <PCI-PCI bridge> at device 9.0 on pci0
pcib0: allocated type 3 (0xd3300000-0xd33fffff) for rid 20 of pcib1
pcib1:   domain            0
pcib1:   secondary bus     1
pcib1:   subordinate bus   1
pcib1:   memory decode     0xd3300000-0xd33fffff
pcib1:   special decode    subtractive
pci1: <PCI bus> on pcib1
pcib1: allocated bus range (1-1) for rid 0 of pci1
pci1: domain=0, physical bus=1
random: harvesting attach, 8 bytes (4 bits) from pci1
random: harvesting attach, 8 bytes (4 bits) from pcib1
nfe0: <NVIDIA nForce MCP79 Networking Adapter> port 0x21e0-0x21e7 mem 0xd3486000-0xd3486fff,0xd3489000-0xd34890ff,0xd3489300-0xd348930f at device 10.0 on pci0
pcib0: matched entry for 0.10.INTA (src \134_SB_.PCI0.LMAC:0)
pcib0: slot 10 INTA routed to irq 17 via \134_SB_.PCI0.LMAC
miibus0: <MII bus> on nfe0
rgephy0: <RTL8169S/8110S/8211 1000BASE-T media interface> PHY 1 on miibus0
rgephy0: OUI 0x00e04c, model 0x0011, rev. 2
rgephy0:  none, 10baseT, 10baseT-FDX, 10baseT-FDX-flow, 100baseTX, 100baseTX-FDX, 100baseTX-FDX-flow, 1000baseT, 1000baseT-master, 1000baseT-FDX, 1000baseT-FDX-master, 1000baseT-FDX-flow, 1000baseT-FDX-flow-master, auto, auto-flow
random: harvesting attach, 8 bytes (4 bits) from rgephy0
random: harvesting attach, 8 bytes (4 bits) from miibus0
nfe0: Using defaults for TSO: 65518/35/2048
nfe0: bpf attached
nfe0: Ethernet address: 00:25:bc:e1:70:fe
random: harvesting attach, 8 bytes (4 bits) from nfe0
ahci0: <NVIDIA MCP79 AHCI SATA controller> port 0x21d8-0x21df,0x21ec-0x21ef,0x21d0-0x21d7,0x21e8-0x21eb,0x21c0-0x21cf mem 0xd3484000-0xd3485fff at device 11.0 on pci0
ahci0: attempting to allocate 8 MSI vectors (8 supported)
msi: routing MSI IRQ 256 to local APIC 0 vector 56
msi: routing MSI IRQ 257 to local APIC 0 vector 57
msi: routing MSI IRQ 258 to local APIC 0 vector 58
msi: routing MSI IRQ 259 to local APIC 0 vector 59
msi: routing MSI IRQ 260 to local APIC 0 vector 60
msi: routing MSI IRQ 261 to local APIC 0 vector 61
msi: routing MSI IRQ 262 to local APIC 0 vector 62
msi: routing MSI IRQ 263 to local APIC 0 vector 63
ahci0: using IRQs 256-263 for MSI
ahci0: AHCI v1.20 with 6 3Gbps ports, Port Multiplier supported
ahci0: quirks=0x200<NOAA>
ahci0: Caps: 64bit NCQ SNTF ALP AL 3Gbps PM PMD SSC PSC 32cmd 6ports
ahci0: Caps2: BOH
ahcich0: <AHCI channel> at channel 0 on ahci0
ahcich0: Caps:
random: harvesting attach, 8 bytes (4 bits) from ahcich0
ahcich1: <AHCI channel> at channel 1 on ahci0
ahcich1: Caps:
random: harvesting attach, 8 bytes (4 bits) from ahcich1
ahcich2: not probed (disabled)
ahcich3: not probed (disabled)
ahcich4: not probed (disabled)
ahcich5: not probed (disabled)
random: harvesting attach, 8 bytes (4 bits) from ahci0
pcib2: <ACPI PCI-PCI bridge> at device 16.0 on pci0
pcib0: allocated type 4 (0x1000-0x1fff) for rid 1c of pcib2
pcib0: allocated type 3 (0xd2000000-0xd30fffff) for rid 20 of pcib2
pcib0: allocated type 3 (0xc0000000-0xd1ffffff) for rid 24 of pcib2
pcib2:   domain            0
pcib2:   secondary bus     2
pcib2:   subordinate bus   2
pcib2:   I/O decode        0x1000-0x1fff
pcib2:   memory decode     0xd2000000-0xd30fffff
pcib2:   prefetched decode 0xc0000000-0xd1ffffff
pci2: <ACPI PCI bus> on pcib2
pcib2: allocated bus range (2-2) for rid 0 of pci2
pci2: domain=0, physical bus=2
found->	vendor=0x10de, dev=0x0863, revid=0xb1
	domain=0, bus=2, slot=0, func=0
	class=03-00-00, hdrtype=0x00, mfdev=0
	cmdreg=0x0002, statreg=0x0010, cachelnsz=64 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=255
	powerspec 2  supports D0 D3  current D0
	MSI supports 1 message, 64 bit
	map[10]: type Memory, range 32, base 0xd2000000, size 24, enabled
pcib2: allocated memory range (0xd2000000-0xd2ffffff) for rid 10 of pci0:2:0:0
	map[14]: type Prefetchable Memory, range 64, base 0xc0000000, size 28, enabled
pcib2: allocated prefetch range (0xc0000000-0xcfffffff) for rid 14 of pci0:2:0:0
	map[1c]: type Prefetchable Memory, range 64, base 0xd0000000, size 25, enabled
pcib2: allocated prefetch range (0xd0000000-0xd1ffffff) for rid 1c of pci0:2:0:0
	map[24]: type I/O Port, range 32, base 0x1000, size  7, port disabled
pcib2: allocated I/O port range (0x1000-0x107f) for rid 24 of pci0:2:0:0
vgapci0: <VGA-compatible display> port 0x1000-0x107f mem 0xd2000000-0xd2ffffff,0xc0000000-0xcfffffff,0xd0000000-0xd1ffffff at device 0.0 on pci2
random: harvesting attach, 8 bytes (4 bits) from vgapci0
random: harvesting attach, 8 bytes (4 bits) from pci2
random: harvesting attach, 8 bytes (4 bits) from pcib2
pcib3: <ACPI PCI-PCI bridge> at device 21.0 on pci0
pcib0: allocated type 3 (0xd3200000-0xd32fffff) for rid 20 of pcib3
pcib3:   domain            0
pcib3:   secondary bus     3
pcib3:   subordinate bus   3
pcib3:   memory decode     0xd3200000-0xd32fffff
pcib3: could not get PCI interrupt routing table for \134_SB_.PCI0.RP04 - AE_NOT_FOUND
pci3: <ACPI PCI bus> on pcib3
pcib3: allocated bus range (3-3) for rid 0 of pci3
pci3: domain=0, physical bus=3
found->	vendor=0x14e4, dev=0x432b, revid=0x01
	domain=0, bus=3, slot=0, func=0
	class=02-80-00, hdrtype=0x00, mfdev=0
	cmdreg=0x0000, statreg=0x0010, cachelnsz=64 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=255
	powerspec 3  supports D0 D1 D2 D3  current D0
	MSI supports 1 message, 64 bit
	map[10]: type Memory, range 64, base 0xd3200000, size 14, memory disabled
pcib3: allocated memory range (0xd3200000-0xd3203fff) for rid 10 of pci0:3:0:0
pci3: <network> at device 0.0 (no driver attached)
random: harvesting attach, 8 bytes (4 bits) from pci3
random: harvesting attach, 8 bytes (4 bits) from pcib3
pcib4: <ACPI PCI-PCI bridge> at device 22.0 on pci0
pcib0: allocated type 3 (0xd3100000-0xd31fffff) for rid 20 of pcib4
pcib4:   domain            0
pcib4:   secondary bus     4
pcib4:   subordinate bus   4
pcib4:   memory decode     0xd3100000-0xd31fffff
pcib4: could not get PCI interrupt routing table for \134_SB_.PCI0.RP05 - AE_NOT_FOUND
pci4: <ACPI PCI bus> on pcib4
pcib4: allocated bus range (4-4) for rid 0 of pci4
pci4: domain=0, physical bus=4
found->	vendor=0x11c1, dev=0x5901, revid=0x07
	domain=0, bus=4, slot=0, func=0
	class=0c-00-10, hdrtype=0x00, mfdev=0
	cmdreg=0x0006, statreg=0x0010, cachelnsz=64 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=255
	powerspec 3  supports D0 D1 D2 D3  current D0
	MSI supports 1 message, 64 bit
	map[10]: type Memory, range 64, base 0xd3100000, size 12, enabled
pcib4: allocated memory range (0xd3100000-0xd3100fff) for rid 10 of pci0:4:0:0
pci4: <serial bus, FireWire> at device 0.0 (no driver attached)
random: harvesting attach, 8 bytes (4 bits) from pci4
random: harvesting attach, 8 bytes (4 bits) from pcib4
random: harvesting attach, 8 bytes (4 bits) from pci0
random: harvesting attach, 8 bytes (4 bits) from pcib0
battery0: <ACPI Control Method Battery> on acpi0
random: harvesting attach, 8 bytes (4 bits) from battery0
random: harvesting attach, 8 bytes (4 bits) from atdma0
random: harvesting attach, 8 bytes (4 bits) from fpupnp0
ACPI: Enabled 3 GPEs in block 00 to 1F
ACPI: Enabled 3 GPEs in block 20 to 5F
random: harvesting attach, 8 bytes (4 bits) from acpi0
random: harvesting attach, 8 bytes (4 bits) from apic0
acpi0: wakeup code va 0xfffffe02273f2000 pa 0x80000
random: harvesting attach, 8 bytes (4 bits) from nexus0
ahc_isa_identify 0: ioport 0xc00 alloc failed
ahc_isa_identify 1: ioport 0x1c00 alloc failed
ahc_isa_identify 2: ioport 0x2c00 alloc failed
ahc_isa_identify 3: ioport 0x3c00 alloc failed
ahc_isa_identify 4: ioport 0x4c00 alloc failed
ahc_isa_identify 5: ioport 0x5c00 alloc failed
ahc_isa_identify 6: ioport 0x6c00 alloc failed
ahc_isa_identify 7: ioport 0x7c00 alloc failed
ahc_isa_identify 8: ioport 0x8c00 alloc failed
ahc_isa_identify 9: ioport 0x9c00 alloc failed
ahc_isa_identify 10: ioport 0xac00 alloc failed
ahc_isa_identify 11: ioport 0xbc00 alloc failed
ahc_isa_identify 12: ioport 0xcc00 alloc failed
ahc_isa_identify 13: ioport 0xdc00 alloc failed
ahc_isa_identify 14: ioport 0xec00 alloc failed
pcib0: allocated type 3 (0xa0000-0xa07ff) for rid 0 of orm0
pcib0: allocated type 3 (0xa0800-0xa0fff) for rid 0 of orm0
pcib0: allocated type 3 (0xa1000-0xa17ff) for rid 0 of orm0
pcib0: allocated type 3 (0xa1800-0xa1fff) for rid 0 of orm0
pcib0: allocated type 3 (0xa2000-0xa27ff) for rid 0 of orm0
pcib0: allocated type 3 (0xa2800-0xa2fff) for rid 0 of orm0
pcib0: allocated type 3 (0xa3000-0xa37ff) for rid 0 of orm0
pcib0: allocated type 3 (0xa3800-0xa3fff) for rid 0 of orm0
pcib0: allocated type 3 (0xa4000-0xa47ff) for rid 0 of orm0
pcib0: allocated type 3 (0xa4800-0xa4fff) for rid 0 of orm0
pcib0: allocated type 3 (0xa5000-0xa57ff) for rid 0 of orm0
pcib0: allocated type 3 (0xa5800-0xa5fff) for rid 0 of orm0
pcib0: allocated type 3 (0xa6000-0xa67ff) for rid 0 of orm0
pcib0: allocated type 3 (0xa6800-0xa6fff) for rid 0 of orm0
pcib0: allocated type 3 (0xa7000-0xa77ff) for rid 0 of orm0
pcib0: allocated type 3 (0xa7800-0xa7fff) for rid 0 of orm0
pcib0: allocated type 3 (0xa8000-0xa87ff) for rid 0 of orm0
pcib0: allocated type 3 (0xa8800-0xa8fff) for rid 0 of orm0
pcib0: allocated type 3 (0xa9000-0xa97ff) for rid 0 of orm0
pcib0: allocated type 3 (0xa9800-0xa9fff) for rid 0 of orm0
pcib0: allocated type 3 (0xaa000-0xaa7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xaa800-0xaafff) for rid 0 of orm0
pcib0: allocated type 3 (0xab000-0xab7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xab800-0xabfff) for rid 0 of orm0
pcib0: allocated type 3 (0xac000-0xac7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xac800-0xacfff) for rid 0 of orm0
pcib0: allocated type 3 (0xad000-0xad7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xad800-0xadfff) for rid 0 of orm0
pcib0: allocated type 3 (0xae000-0xae7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xae800-0xaefff) for rid 0 of orm0
pcib0: allocated type 3 (0xaf000-0xaf7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xaf800-0xaffff) for rid 0 of orm0
pcib0: allocated type 3 (0xb0000-0xb07ff) for rid 0 of orm0
pcib0: allocated type 3 (0xb0800-0xb0fff) for rid 0 of orm0
pcib0: allocated type 3 (0xb1000-0xb17ff) for rid 0 of orm0
pcib0: allocated type 3 (0xb1800-0xb1fff) for rid 0 of orm0
pcib0: allocated type 3 (0xb2000-0xb27ff) for rid 0 of orm0
pcib0: allocated type 3 (0xb2800-0xb2fff) for rid 0 of orm0
pcib0: allocated type 3 (0xb3000-0xb37ff) for rid 0 of orm0
pcib0: allocated type 3 (0xb3800-0xb3fff) for rid 0 of orm0
pcib0: allocated type 3 (0xb4000-0xb47ff) for rid 0 of orm0
pcib0: allocated type 3 (0xb4800-0xb4fff) for rid 0 of orm0
pcib0: allocated type 3 (0xb5000-0xb57ff) for rid 0 of orm0
pcib0: allocated type 3 (0xb5800-0xb5fff) for rid 0 of orm0
pcib0: allocated type 3 (0xb6000-0xb67ff) for rid 0 of orm0
pcib0: allocated type 3 (0xb6800-0xb6fff) for rid 0 of orm0
pcib0: allocated type 3 (0xb7000-0xb77ff) for rid 0 of orm0
pcib0: allocated type 3 (0xb7800-0xb7fff) for rid 0 of orm0
pcib0: allocated type 3 (0xb8000-0xb87ff) for rid 0 of orm0
pcib0: allocated type 3 (0xb8800-0xb8fff) for rid 0 of orm0
pcib0: allocated type 3 (0xb9000-0xb97ff) for rid 0 of orm0
pcib0: allocated type 3 (0xb9800-0xb9fff) for rid 0 of orm0
pcib0: allocated type 3 (0xba000-0xba7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xba800-0xbafff) for rid 0 of orm0
pcib0: allocated type 3 (0xbb000-0xbb7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xbb800-0xbbfff) for rid 0 of orm0
pcib0: allocated type 3 (0xbc000-0xbc7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xbc800-0xbcfff) for rid 0 of orm0
pcib0: allocated type 3 (0xbd000-0xbd7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xbd800-0xbdfff) for rid 0 of orm0
pcib0: allocated type 3 (0xbe000-0xbe7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xbe800-0xbefff) for rid 0 of orm0
pcib0: allocated type 3 (0xbf000-0xbf7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xbf800-0xbffff) for rid 0 of orm0
pcib0: allocated type 3 (0xc0000-0xc07ff) for rid 0 of orm0
pcib0: allocated type 3 (0xc0800-0xc0fff) for rid 0 of orm0
pcib0: allocated type 3 (0xc1000-0xc17ff) for rid 0 of orm0
pcib0: allocated type 3 (0xc1800-0xc1fff) for rid 0 of orm0
pcib0: allocated type 3 (0xc2000-0xc27ff) for rid 0 of orm0
pcib0: allocated type 3 (0xc2800-0xc2fff) for rid 0 of orm0
pcib0: allocated type 3 (0xc3000-0xc37ff) for rid 0 of orm0
pcib0: allocated type 3 (0xc3800-0xc3fff) for rid 0 of orm0
pcib0: allocated type 3 (0xc4000-0xc47ff) for rid 0 of orm0
pcib0: allocated type 3 (0xc4800-0xc4fff) for rid 0 of orm0
pcib0: allocated type 3 (0xc5000-0xc57ff) for rid 0 of orm0
pcib0: allocated type 3 (0xc5800-0xc5fff) for rid 0 of orm0
pcib0: allocated type 3 (0xc6000-0xc67ff) for rid 0 of orm0
pcib0: allocated type 3 (0xc6800-0xc6fff) for rid 0 of orm0
pcib0: allocated type 3 (0xc7000-0xc77ff) for rid 0 of orm0
pcib0: allocated type 3 (0xc7800-0xc7fff) for rid 0 of orm0
pcib0: allocated type 3 (0xc8000-0xc87ff) for rid 0 of orm0
pcib0: allocated type 3 (0xc8800-0xc8fff) for rid 0 of orm0
pcib0: allocated type 3 (0xc9000-0xc97ff) for rid 0 of orm0
pcib0: allocated type 3 (0xc9800-0xc9fff) for rid 0 of orm0
pcib0: allocated type 3 (0xca000-0xca7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xca800-0xcafff) for rid 0 of orm0
pcib0: allocated type 3 (0xcb000-0xcb7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xcb800-0xcbfff) for rid 0 of orm0
pcib0: allocated type 3 (0xcc000-0xcc7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xcc800-0xccfff) for rid 0 of orm0
pcib0: allocated type 3 (0xcd000-0xcd7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xcd800-0xcdfff) for rid 0 of orm0
pcib0: allocated type 3 (0xce000-0xce7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xce800-0xcefff) for rid 0 of orm0
pcib0: allocated type 3 (0xcf000-0xcf7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xcf800-0xcffff) for rid 0 of orm0
pcib0: allocated type 3 (0xd0000-0xd07ff) for rid 0 of orm0
pcib0: allocated type 3 (0xd0800-0xd0fff) for rid 0 of orm0
pcib0: allocated type 3 (0xd1000-0xd17ff) for rid 0 of orm0
pcib0: allocated type 3 (0xd1800-0xd1fff) for rid 0 of orm0
pcib0: allocated type 3 (0xd2000-0xd27ff) for rid 0 of orm0
pcib0: allocated type 3 (0xd2800-0xd2fff) for rid 0 of orm0
pcib0: allocated type 3 (0xd3000-0xd37ff) for rid 0 of orm0
pcib0: allocated type 3 (0xd3800-0xd3fff) for rid 0 of orm0
pcib0: allocated type 3 (0xd4000-0xd47ff) for rid 0 of orm0
pcib0: allocated type 3 (0xd4800-0xd4fff) for rid 0 of orm0
pcib0: allocated type 3 (0xd5000-0xd57ff) for rid 0 of orm0
pcib0: allocated type 3 (0xd5800-0xd5fff) for rid 0 of orm0
pcib0: allocated type 3 (0xd6000-0xd67ff) for rid 0 of orm0
pcib0: allocated type 3 (0xd6800-0xd6fff) for rid 0 of orm0
pcib0: allocated type 3 (0xd7000-0xd77ff) for rid 0 of orm0
pcib0: allocated type 3 (0xd7800-0xd7fff) for rid 0 of orm0
pcib0: allocated type 3 (0xd8000-0xd87ff) for rid 0 of orm0
pcib0: allocated type 3 (0xd8800-0xd8fff) for rid 0 of orm0
pcib0: allocated type 3 (0xd9000-0xd97ff) for rid 0 of orm0
pcib0: allocated type 3 (0xd9800-0xd9fff) for rid 0 of orm0
pcib0: allocated type 3 (0xda000-0xda7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xda800-0xdafff) for rid 0 of orm0
pcib0: allocated type 3 (0xdb000-0xdb7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xdb800-0xdbfff) for rid 0 of orm0
pcib0: allocated type 3 (0xdc000-0xdc7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xdc800-0xdcfff) for rid 0 of orm0
pcib0: allocated type 3 (0xdd000-0xdd7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xdd800-0xddfff) for rid 0 of orm0
pcib0: allocated type 3 (0xde000-0xde7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xde800-0xdefff) for rid 0 of orm0
pcib0: allocated type 3 (0xdf000-0xdf7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xdf800-0xdffff) for rid 0 of orm0
pcib0: allocated type 3 (0xe0000-0xe07ff) for rid 0 of orm0
pcib0: allocated type 3 (0xe0800-0xe0fff) for rid 0 of orm0
pcib0: allocated type 3 (0xe1000-0xe17ff) for rid 0 of orm0
pcib0: allocated type 3 (0xe1800-0xe1fff) for rid 0 of orm0
pcib0: allocated type 3 (0xe2000-0xe27ff) for rid 0 of orm0
pcib0: allocated type 3 (0xe2800-0xe2fff) for rid 0 of orm0
pcib0: allocated type 3 (0xe3000-0xe37ff) for rid 0 of orm0
pcib0: allocated type 3 (0xe3800-0xe3fff) for rid 0 of orm0
pcib0: allocated type 3 (0xe4000-0xe47ff) for rid 0 of orm0
pcib0: allocated type 3 (0xe4800-0xe4fff) for rid 0 of orm0
pcib0: allocated type 3 (0xe5000-0xe57ff) for rid 0 of orm0
pcib0: allocated type 3 (0xe5800-0xe5fff) for rid 0 of orm0
pcib0: allocated type 3 (0xe6000-0xe67ff) for rid 0 of orm0
pcib0: allocated type 3 (0xe6800-0xe6fff) for rid 0 of orm0
pcib0: allocated type 3 (0xe7000-0xe77ff) for rid 0 of orm0
pcib0: allocated type 3 (0xe7800-0xe7fff) for rid 0 of orm0
pcib0: allocated type 3 (0xe8000-0xe87ff) for rid 0 of orm0
pcib0: allocated type 3 (0xe8800-0xe8fff) for rid 0 of orm0
pcib0: allocated type 3 (0xe9000-0xe97ff) for rid 0 of orm0
pcib0: allocated type 3 (0xe9800-0xe9fff) for rid 0 of orm0
pcib0: allocated type 3 (0xea000-0xea7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xea800-0xeafff) for rid 0 of orm0
pcib0: allocated type 3 (0xeb000-0xeb7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xeb800-0xebfff) for rid 0 of orm0
pcib0: allocated type 3 (0xec000-0xec7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xec800-0xecfff) for rid 0 of orm0
pcib0: allocated type 3 (0xed000-0xed7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xed800-0xedfff) for rid 0 of orm0
pcib0: allocated type 3 (0xee000-0xee7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xee800-0xeefff) for rid 0 of orm0
pcib0: allocated type 3 (0xef000-0xef7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xef800-0xeffff) for rid 0 of orm0
pcib0: allocated type 3 (0xf0000-0xf07ff) for rid 0 of orm0
pcib0: allocated type 3 (0xf0800-0xf0fff) for rid 0 of orm0
pcib0: allocated type 3 (0xf1000-0xf17ff) for rid 0 of orm0
pcib0: allocated type 3 (0xf1800-0xf1fff) for rid 0 of orm0
pcib0: allocated type 3 (0xf2000-0xf27ff) for rid 0 of orm0
pcib0: allocated type 3 (0xf2800-0xf2fff) for rid 0 of orm0
pcib0: allocated type 3 (0xf3000-0xf37ff) for rid 0 of orm0
pcib0: allocated type 3 (0xf3800-0xf3fff) for rid 0 of orm0
pcib0: allocated type 3 (0xf4000-0xf47ff) for rid 0 of orm0
pcib0: allocated type 3 (0xf4800-0xf4fff) for rid 0 of orm0
pcib0: allocated type 3 (0xf5000-0xf57ff) for rid 0 of orm0
pcib0: allocated type 3 (0xf5800-0xf5fff) for rid 0 of orm0
pcib0: allocated type 3 (0xf6000-0xf67ff) for rid 0 of orm0
pcib0: allocated type 3 (0xf6800-0xf6fff) for rid 0 of orm0
pcib0: allocated type 3 (0xf7000-0xf77ff) for rid 0 of orm0
pcib0: allocated type 3 (0xf7800-0xf7fff) for rid 0 of orm0
pcib0: allocated type 3 (0xf8000-0xf87ff) for rid 0 of orm0
pcib0: allocated type 3 (0xf8800-0xf8fff) for rid 0 of orm0
pcib0: allocated type 3 (0xf9000-0xf97ff) for rid 0 of orm0
pcib0: allocated type 3 (0xf9800-0xf9fff) for rid 0 of orm0
pcib0: allocated type 3 (0xfa000-0xfa7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xfa800-0xfafff) for rid 0 of orm0
pcib0: allocated type 3 (0xfb000-0xfb7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xfb800-0xfbfff) for rid 0 of orm0
pcib0: allocated type 3 (0xfc000-0xfc7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xfc800-0xfcfff) for rid 0 of orm0
pcib0: allocated type 3 (0xfd000-0xfd7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xfd800-0xfdfff) for rid 0 of orm0
pcib0: allocated type 3 (0xfe000-0xfe7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xfe800-0xfefff) for rid 0 of orm0
pcib0: allocated type 3 (0xff000-0xff7ff) for rid 0 of orm0
pcib0: allocated type 3 (0xff800-0xfffff) for rid 0 of orm0
isa_probe_children: disabling PnP devices
atrtc: atrtc0 already exists; skipping it
attimer: attimer0 already exists; skipping it
sc: sc0 already exists; skipping it
isa_probe_children: probing non-PnP devices
sc0 failed to probe on isa0
vga0 failed to probe on isa0
pcib0: allocated type 4 (0x60-0x60) for rid 0 of atkbdc0
pcib0: allocated type 4 (0x64-0x64) for rid 1 of atkbdc0
atkbdc0: AT keyboard controller not found
atkbdc0 failed to probe at port 0x60,0x64 on isa0
pcib0: allocated type 4 (0x3f0-0x3f5) for rid 0 of fdc0
pcib0: allocated type 4 (0x3f7-0x3f7) for rid 1 of fdc0
fdc0 failed to probe at port 0x3f0-0x3f5,0x3f7 irq 6 drq 2 on isa0
ppc0: cannot reserve I/O port range
ppc0 failed to probe at irq 7 on isa0
pcib0: allocated type 4 (0x3f8-0x3f8) for rid 0 of uart0
uart0 failed to probe at port 0x3f8 irq 4 on isa0
pcib0: allocated type 4 (0x2f8-0x2f8) for rid 0 of uart1
uart1 failed to probe at port 0x2f8 irq 3 on isa0
isa_probe_children: probing PnP devices
random: harvesting attach, 8 bytes (4 bits) from acpi_perf0
random: harvesting attach, 8 bytes (4 bits) from acpi_perf1
est0: <Enhanced SpeedStep Frequency Control> on cpu0
random: harvesting attach, 8 bytes (4 bits) from cpufreq0
random: harvesting attach, 8 bytes (4 bits) from est0
est1: <Enhanced SpeedStep Frequency Control> on cpu1
random: harvesting attach, 8 bytes (4 bits) from cpufreq1
random: harvesting attach, 8 bytes (4 bits) from est1
Device configuration finished.
procfs registered
lapic: Divisor 2, Frequency 132670039 Hz
Timecounters tick every 1.000 msec
vlan: initialized, using hash tables with chaining
lo0: bpf attached
IPsec: Initialized Security Association Processing.
tcp_init: net.inet.tcp.tcbhashsize auto tuned to 65536
hpt27xx: no controller detected.
hptnr: no controller detected.
hptrr: no controller detected.
nvme cam probe device init
hdacc0: <Cirrus Logic CS4206 HDA CODEC> at cad 0 on hdac0
hdaa0: <Cirrus Logic CS4206 Audio Function Group> at nid 1 on hdacc0
hdaa0: Subsystem ID: 0x106b4d00
hdaa0: NumGPIO=4 NumGPO=0 NumGPI=0 GPIWake=0 GPIUnsol=0
hdaa0:  GPIO0: disabled
hdaa0:  GPIO1: disabled
hdaa0:  GPIO2: disabled
hdaa0:  GPIO3: output state=0
hdaa0: Original pins configuration:
hdaa0: nid   0x    as seq device       conn  jack    loc        color   misc
hdaa0:  9 0e2b4030 3  0  Headphones    Jack  Combo   0x0e       Green   0
hdaa0: 10 90100121 2  1  Speaker       Fixed Unknown Internal   Unknown 1
hdaa0: 11 90100120 2  0  Speaker       Fixed Unknown Internal   Unknown 1
hdaa0: 12 0f8b3050 5  0  Line-in       Jack  Combo   0x0f       Blue    0
hdaa0: 13 90a00110 1  0  Mic           Fixed Unknown Internal   Unknown 1
hdaa0: 14 400000f0 15 0  Line-out      None  Unknown 0x00       Unknown 0
hdaa0: 15 400000f0 15 0  Line-out      None  Unknown 0x00       Unknown 0
hdaa0: 16 014be040 4  0  SPDIF-out     Jack  Combo   Rear       White   0
hdaa0: 18 400000f0 15 0  Line-out      None  Unknown 0x00       Unknown 0
hdaa0: 21 400000f0 15 0  Line-out      None  Unknown 0x00       Unknown 0
hdaa0: Patched pins configuration:
hdaa0: nid   0x    as seq device       conn  jack    loc        color   misc
hdaa0:  9 0e2b4030 3  0  Headphones    Jack  Combo   0x0e       Green   0
hdaa0: 10 90100121 2  1  Speaker       Fixed Unknown Internal   Unknown 1
hdaa0: 11 90100120 2  0  Speaker       Fixed Unknown Internal   Unknown 1
hdaa0: 12 0f8b3050 5  0  Line-in       Jack  Combo   0x0f       Blue    0
hdaa0: 13 90a00110 1  0  Mic           Fixed Unknown Internal   Unknown 1
hdaa0: 14 400000f0 15 0  Line-out      None  Unknown 0x00       Unknown 0 DISA
hdaa0: 15 400000f0 15 0  Line-out      None  Unknown 0x00       Unknown 0 DISA
hdaa0: 16 014be040 4  0  SPDIF-out     Jack  Combo   Rear       White   0
hdaa0: 18 400000f0 15 0  Line-out      None  Unknown 0x00       Unknown 0 DISA
hdaa0: 21 400000f0 15 0  Line-out      None  Unknown 0x00       Unknown 0 DISA
hdaa0: 5 associations found:
hdaa0: Association 0 (1) in:
hdaa0:  Pin nid=13 seq=0
hdaa0: Association 1 (2) out:
hdaa0:  Pin nid=11 seq=0
hdaa0:  Pin nid=10 seq=1
hdaa0: Association 2 (3) out:
hdaa0:  Pin nid=9 seq=0
hdaa0: Association 3 (4) out:
hdaa0:  Pin nid=16 seq=0
hdaa0: Association 4 (5) in:
hdaa0:  Pin nid=12 seq=0
hdaa0: Tracing association 0 (1)
hdaa0:  Unable to trace pin 13 to ADC 5, undo traces
hdaa0:  Pin 13 traced to ADC 6
hdaa0: Association 0 (1) trace succeeded
hdaa0: Tracing association 1 (2)
hdaa0:  Pin 11 traced to DAC 4
hdaa0:  Pin 10 traced to DAC 3
hdaa0: Association 1 (2) trace succeeded
hdaa0: Tracing association 2 (3)
hdaa0:  Pin 9 traced to DAC 2
hdaa0: Association 2 (3) trace succeeded
hdaa0: Tracing association 3 (4)
hdaa0:  Pin 16 traced to DAC 8
hdaa0: Association 3 (4) trace succeeded
hdaa0: Tracing association 4 (5)
hdaa0:  Pin 12 traced to ADC 5
hdaa0: Association 4 (5) trace succeeded
hdaa0: Looking for additional ADC for association 0 (1)
hdaa0: Looking for additional DAC for association 1 (2)
hdaa0: Looking for additional DAC for association 2 (3)
hdaa0: Looking for additional DAC for association 3 (4)
hdaa0: Looking for additional ADC for association 4 (5)
hdaa0: Tracing input monitor
hdaa0: Tracing other input monitors
hdaa0:  Tracing nid 12 to out
hdaa0:  Tracing nid 13 to out
hdaa0: Tracing beeper
hdaa0: GPIO commit
hdaa0:  GPIO0: disabled
hdaa0:  GPIO1: output state=1
hdaa0:  GPIO2: disabled
hdaa0:  GPIO3: output state=1
hdaa0: FG config/quirks: forcestereo ivref50 ivref80 ivref100 ivref
pcm0: <Cirrus Logic CS4206 (Internal Analog 3.1/2.0)> at nid 11,10 and 13 on hdaa0
pcm0: Playback:
pcm0:      Stream cap: 0x00000003 FLOAT32 PCM
pcm0:         PCM cap: 0x001e07f0 16 20 24 32 bits, 32 44 48 88 96 176 192 KHz
pcm0:             DAC: 4 3
pcm0: 
pcm0:     nid=11 [pin: Speaker (Fixed)]
pcm0:       + <- nid=4 [audio output] [src: pcm]
pcm0: 
pcm0:     nid=10 [pin: Speaker (Fixed)]
pcm0:       + <- nid=3 [audio output] [src: pcm]
pcm0: 
pcm0: Record:
pcm0:      Stream cap: 0x00000003 FLOAT32 PCM
pcm0:         PCM cap: 0x001e01f5 16 20 24 32 bits, 8 16 32 44 48 88 96 KHz
pcm0:             ADC: 6
pcm0: 
pcm0:     nid=6 [audio input]
pcm0:       + <- nid=13 [pin: Mic (Fixed)] [src: monitor]
pcm0: 
pcm0: Master Volume (OSS: vol): -57/6dB
pcm0:    +- ctl  2 (nid   3 out):    -57/6dB (128 steps) + mute
pcm0:    +- ctl  3 (nid   4 out):    -57/6dB (128 steps) + mute
pcm0: 
pcm0: PCM Volume (OSS: pcm): -57/6dB
pcm0:    +- ctl  2 (nid   3 out):    -57/6dB (128 steps) + mute
pcm0:    +- ctl  3 (nid   4 out):    -57/6dB (128 steps) + mute
pcm0: 
pcm0: Microphone2 Volume (OSS: monitor): 0/30dB
pcm0:    +- ctl  5 (nid   6 in   0): -51/12dB (64 steps) + mute
pcm0:    +- ctl  7 (nid  13 out):    0/30dB (4 steps)
pcm0: 
pcm0: Recording Level (OSS: rec): -51/12dB
pcm0:    +- ctl  5 (nid   6 in   0): -51/12dB (64 steps) + mute
pcm0:    +- ctl  7 (nid  13 out):    0/30dB (4 steps)
pcm0: 
pcm0: Mixer "vol":
pcm0: Mixer "pcm":
pcm0: Mixer "rec":
pcm0: Mixer "monitor":
pcm0: Playback channel set is: Front Left, Front Right, Front Center, Low Frequency Effects, 
pcm0: Playback channel matrix is: 2.0 (unknown)
pcm0: Automatically set rec source to: monitor
pcm0: Recording channel set is: Front Left, Front Right, 
pcm0: Recording channel matrix is: 2.0 (unknown)
random: harvesting attach, 8 bytes (4 bits) from pcm0
pcm1: <Cirrus Logic CS4206 (Analog)> at nid 9 and 12 on hdaa0
pcm1: Playback:
pcm1:      Stream cap: 0x00000003 FLOAT32 PCM
pcm1:         PCM cap: 0x001e07f0 16 20 24 32 bits, 32 44 48 88 96 176 192 KHz
pcm1:             DAC: 2
pcm1: 
pcm1:     nid=9 [pin: Headphones (Green Jack)]
pcm1:       + <- nid=2 [audio output] [src: pcm]
pcm1: 
pcm1: Record:
pcm1:      Stream cap: 0x00000003 FLOAT32 PCM
pcm1:         PCM cap: 0x001e01f5 16 20 24 32 bits, 8 16 32 44 48 88 96 KHz
pcm1:             ADC: 5
pcm1: 
pcm1:     nid=5 [audio input]
pcm1:       + <- nid=12 [pin: Line-in (Blue Jack)] [src: line]
pcm1: 
pcm1: Master Volume (OSS: vol): -57/6dB
pcm1:    +- ctl  1 (nid   2 out):    -57/6dB (128 steps) + mute
pcm1: 
pcm1: PCM Volume (OSS: pcm): -57/6dB
pcm1:    +- ctl  1 (nid   2 out):    -57/6dB (128 steps) + mute
pcm1: 
pcm1: Line-in Volume (OSS: line): 0/30dB
pcm1:    +- ctl  4 (nid   5 in   0): -51/12dB (64 steps) + mute
pcm1:    +- ctl  6 (nid  12 out):    0/30dB (4 steps)
pcm1: 
pcm1: Recording Level (OSS: rec): -51/12dB
pcm1:    +- ctl  4 (nid   5 in   0): -51/12dB (64 steps) + mute
pcm1:    +- ctl  6 (nid  12 out):    0/30dB (4 steps)
pcm1: 
pcm1: Mixer "vol":
pcm1: Mixer "pcm":
pcm1: Mixer "line":
pcm1: Mixer "rec":
pcm1: Playback channel set is: Front Left, Front Right, 
pcm1: Playback channel matrix is: 2.0 (disconnected)
pcm1: Recording channel set is: Front Left, Front Right, 
pcm1: Recording channel matrix is: 2.0 (disconnected)
random: harvesting attach, 8 bytes (4 bits) from pcm1
pcm2: <Cirrus Logic CS4206 (Rear Digital)> at nid 16 on hdaa0
pcm2: Playback:
pcm2:      Stream cap: 0x00000007 AC3 FLOAT32 PCM
pcm2:         PCM cap: 0x001e07f0 16 20 24 32 bits, 32 44 48 88 96 176 192 KHz
pcm2:             DAC: 8
pcm2: 
pcm2:     nid=16 [pin: SPDIF-out (White Jack)]
pcm2:       + <- nid=8 [audio output] [src: pcm]
pcm2: 
pcm2: Mixer "vol" -> "none": child=0x00000010
pcm2: Mixer "pcm": parent="vol"
pcm2: Soft PCM mixer ENABLED
pcm2: Playback channel set is: Front Left, Front Right, 
pcm2: Playback channel matrix is: 2.0 (unknown)
random: harvesting attach, 8 bytes (4 bits) from pcm2
random: harvesting attach, 8 bytes (4 bits) from hdaa0
random: harvesting attach, 8 bytes (4 bits) from hdacc0
usbus0: 12Mbps Full Speed USB v1.0
usbus1: 480Mbps High Speed USB v2.0
usbus2: 12Mbps Full Speed USB v1.0
ugen0.1: <nVidia> at usbus0
uhub0: <nVidia OHCI root HUB, class 9/0, rev 1.00/1.00, addr 1> on usbus0
ugen1.1: <nVidia> at usbus1
uhub1: <nVidia EHCI root HUB, class 9/0, rev 2.00/1.00, addr 1> on usbus1
ugen2.1: <nVidia> at usbus2
uhub2: <nVidia OHCI root HUB, class 9/0, rev 1.00/1.00, addr 1> on usbus2
usbus3: 480Mbps High Speed USB v2.0
ahcich0: AHCI reset...
ahcich0: SATA connect time=0us status=00000123
ugen3.1: <nVidia> at usbus3
uhub3: <nVidia EHCI root HUB, class 9/0, rev 2.00/1.00, addr 1> on usbus3
ahcich0: AHCI reset: device found
ahcich0: AHCI reset: device ready after 0ms
ahcich1: AHCI reset...
ahcich1: SATA connect time=0us status=00000113
ahcich1: AHCI reset: device found
ahcich1: AHCI reset: device ready after 0ms
acpi_acad0: acline initialization start
acpi_acad0: On Line
acpi_acad0: acline initialization done, tried 1 times
pass0 at ahcich0 bus 0 scbus0 target 0 lun 0
pass0: <Crucial CT500MX200SSD1 MU01> ACS-3 ATA SATA 3.x device
pass0: Serial Number 14520E65E3DA
pass0: 300.000MB/s transfers (SATA 2.x, UDMA6, PIO 8192bytes)
pass0: Command Queueing enabled
pass1 at ahcich1 bus 0 scbus1 target 0 lun 0
pass1: <HL-DT-ST DVDRW  GS23N SB00> Removable CD-ROM SCSI device
pass1: Serial Number KZZ96KG1812
pass1: 150.000MB/s transfers (SATA 1.x, UDMA6, ATAPI 12bytes, PIO 8192bytes)
ada0 at ahcich0 bus 0 scbus0 target 0 lun 0
GEOM: new disk cd0
cd0 at ahcich1 bus 0 scbus1 target 0 lun 0
cd0: <HL-DT-ST DVDRW  GS23N SB00> Removable CD-ROM SCSI device
cd0: Serial Number KZZ96KG1812
cd0: 150.000MB/s transfers (SATA 1.x, UDMA6, ATAPI 12bytes, PIO 8192bytes)
cd0: Attempt to query device size failed: NOT READY, Medium not present
GEOM: new disk ada0
ada0: <Crucial CT500MX200SSD1 MU01> ACS-3 ATA SATA 3.x device
ada0: Serial Number 14520E65E3DA
ada0: 300.000MB/s transfers (SATA 2.x, UDMA6, PIO 8192bytes)
battery0: battery initialization start
ada0: Command Queueing enabled
ada0: 476940MB (976773168 512 byte sectors)
ada0: quirks=0x2<NCQ_TRIM_BROKEN>
SMP: AP CPU #1 Launched!
cpu1 AP:
     ID: 0x01000000   VER: 0x00050014 LDR: 0x00000000 DFR: 0xffffffff
  lint0: 0x00010700 lint1: 0x00000400 TPR: 0x00000000 SVR: 0x000001ff
  timer: 0x000100ef therm: 0x00010000 err: 0x000000f0 pmc: 0x00010400
ioapic0: routing intpin 9 (ISA IRQ 9) to lapic 1 vector 48
ioapic0: routing intpin 18 (PCI IRQ 18) to lapic 1 vector 49
ioapic0: routing intpin 22 (PCI IRQ 22) to lapic 1 vector 50
msi: Assigning MSI IRQ 256 to local APIC 1 vector 56
msi: Assigning MSI IRQ 257 to local APIC 1 vector 57
msi: Assigning MSI IRQ 258 to local APIC 1 vector 58
msi: Assigning MSI IRQ 259 to local APIC 1 vector 59
msi: Assigning MSI IRQ 260 to local APIC 1 vector 60
msi: Assigning MSI IRQ 261 to local APIC 1 vector 61
msi: Assigning MSI IRQ 262 to local APIC 1 vector 62
msi: Assigning MSI IRQ 263 to local APIC 1 vector 63
TSC timecounter disables C2 and C3.
SMP: passed TSC synchronization test
TSC timecounter discards lower 1 bit(s)
Timecounter "TSC-low" frequency 1127695157 Hz quality 1000
Trying to mount root from ufs:/dev/ufs/FreeBSD_Install [ro,noatime]...
uhub2: 5 ports with 5 removable, self powered
random: harvesting attach, 8 bytes (4 bits) from uhub2
Root mount waiting for: usbus3 usbus1 usbus0
uhub0: 7 ports with 7 removable, self powered
random: harvesting attach, 8 bytes (4 bits) from uhub0
battery0: battery initialization done, tried 1 times
Root mount waiting for: usbus3 usbus1
uhub3: 5 ports with 5 removable, self powered
random: harvesting attach, 8 bytes (4 bits) from uhub3
Root mount waiting for: usbus3 usbus1
uhub1: 7 ports with 7 removable, self powered
random: harvesting attach, 8 bytes (4 bits) from uhub1
Root mount waiting for: usbus3 usbus1
ugen2.2: <Apple Inc.> at usbus2
uhub4: <Apple Inc. BRCM2046 Hub, class 9/0, rev 2.00/1.00, addr 2> on usbus2
ugen1.2: <Apple Inc.> at usbus1
uhub4: 3 ports with 0 removable, self powered
random: harvesting attach, 8 bytes (4 bits) from uhub4
Root mount waiting for: usbus3 usbus1
ugen2.3: <Apple Inc.> at usbus2
ugen0.2: <Apple Computer, Inc.> at usbus0
ugen2.4: <vendor 0x05ac> at usbus2
ukbd0: <vendor 0x05ac product 0x820a, class 0/0, rev 2.00/1.00, addr 4> on usbus2
kbd: new array size 4
kbd1 at ukbd0
kbd1: ukbd0, generic (0), config:0x0, flags:0x3d0000
random: harvesting attach, 8 bytes (4 bits) from ukbd0
Root mount waiting for: usbus3
ugen0.3: <Apple Inc.> at usbus0
ukbd1: <Apple Internal Keyboard> on usbus0
kbd2 at ukbd1
kbd2: ukbd1, generic (0), config:0x0, flags:0x3d0000
random: harvesting attach, 8 bytes (4 bits) from ukbd1
ugen3.2: <vendor 0x13fe> at usbus3
umass0: <vendor 0x13fe USB DISK 3.0, class 0/0, rev 2.10/1.00, addr 2> on usbus3
umass0:  SCSI over Bulk-Only; quirks = 0x8100
umass0:2:0: Attached to scbus2
random: harvesting attach, 8 bytes (4 bits) from umass0
pass2 at umass-sim0 bus 0 scbus2 target 0 lun 0
pass2: < USB DISK 3.0 PMAP> Removable Direct Access SPC-4 SCSI device
pass2: Serial Number 070856340990FF51
pass2: 40.000MB/s transfers
GEOM: new disk da0
da0 at umass-sim0 bus 0 scbus2 target 0 lun 0
da0: < USB DISK 3.0 PMAP> Removable Direct Access SPC-4 SCSI device
da0: Serial Number 070856340990FF51
da0: 40.000MB/s transfers
da0: 7385MB (15124992 512 byte sectors)
da0: quirks=0x3<NO_SYNC_CACHE,NO_6_BYTE>
da0: Delete methods: <NONE(*),ZERO>
GEOM: da0: the secondary GPT header is not in the last LBA.
ugen2.5: <vendor 0x05ac> at usbus2
GEOM: diskid/DISK-070856340990FF51: the secondary GPT header is not in the last LBA.
ugen3.3: <Apple> at usbus3
umass1: <Apple Card Reader, class 0/0, rev 2.00/98.33, addr 3> on usbus3
umass1:  SCSI over Bulk-Only; quirks = 0x4000
umass1:3:1: Attached to scbus3
random: harvesting attach, 8 bytes (4 bits) from umass1
(probe0:umass-sim1:1:0:0): Down reving Protocol Version from 2 to 0?
pass3 at umass-sim1 bus 1 scbus3 target 0 lun 0
pass3: <APPLE SD Card Reader 1.00> Removable Direct Access SCSI device
pass3: Serial Number 000000009833
pass3: 40.000MB/s transfers
da1 at umass-sim1 bus 1 scbus3 target 0 lun 0
da1: <APPLE SD Card Reader 1.00> Removable Direct Access SCSI device
da1: Serial Number 000000009833
da1: 40.000MB/s transfers
da1: Attempt to query device size failed: NOT READY, Medium not present
da1: quirks=0x2<NO_6_BYTE>
da1: Delete methods: <NONE(*),ZERO>
GEOM: new disk da1
mountroot: waiting for device /dev/ufs/FreeBSD_Install...
start_init: trying /sbin/init
GEOM: diskid/DISK-070856340990FF51: the secondary GPT header is not in the last LBA.
random: unblocking device.
nfe0: link state changed to DOWN
ubt0: <Apple Inc. Bluetooth USB Host Controller, rev 2.00/2.07, addr 3> on usbus2
random: harvesting attach, 8 bytes (4 bits) from ubt0
uhid0: <Apple Computer, Inc. IR Receiver, class 0/0, rev 2.00/0.16, addr 2> on usbus0
random: harvesting attach, 8 bytes (4 bits) from uhid0
uhid1: <Touchpad> on usbus0
random: harvesting attach, 8 bytes (4 bits) from uhid1
ums0: <Touchpad> on usbus0
ums1: <vendor 0x05ac product 0x820b, class 0/0, rev 2.00/1.00, addr 5> on usbus2
ums0: 3 buttons and [XY] coordinates ID=2
random: harvesting attach, 8 bytes (4 bits) from ums0
ums1: 3 buttons and [XY] coordinates ID=2
random: harvesting attach, 8 bytes (4 bits) from ums1
WARNING: attempt to domain_add(bluetooth) after domainfinalize()
WARNING: attempt to domain_add(netgraph) after domainfinalize()
ugen2.4: <vendor 0x05ac> at usbus2 (disconnected)
ukbd0: at uhub4, port 2, addr 4 (disconnected)
ugen2.5: <vendor 0x05ac> at usbus2 (disconnected)
ums1: at uhub4, port 3, addr 5 (disconnected)
