Copyright (c) 2003-2014 The DragonFly Project.
Copyright (c) 1992-2003 The FreeBSD Project.
Copyright (c) 1979, 1980, 1983, 1986, 1988, 1989, 1991, 1992, 1993, 1994
	The Regents of the University of California. All rights reserved.
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
DragonFly 55619ec-RELEASE #7: Sat Nov 22 21:25:25 UTC 2014
    root@:/usr/obj/usr/src/sys/X86_64_GENERIC
TSC clock: 2192836030 Hz, i8254 clock: 1193145 Hz
CPU: Intel(R) Core(TM)2 Duo CPU     T7500  @ 2.20GHz (2192.92-MHz K8-class CPU)
  Origin = "GenuineIntel"  Id = 0x6fb  Stepping = 11
  Features=0xafebfbff<FPU,VME,DE,PSE,TSC,MSR,PAE,MCE,CX8,APIC,SEP,MTRR,PGE,MCA,CMOV,PAT,PSE36,CLFLUSH,DTS,ACPI,MMX,FXSR,SSE,SSE2,SS,TM,PBE>
  Features2=0xe3bd<SSE3,DTES64,MON,DS_CPL,VMX,EST,TM2,SSSE3,CX16,xTPR,PDCM>
  AMD Features=0x20000800<SYSCALL,LM>
  AMD Features2=0x1<LAHF>
  Thermal and PM Features=0x3<SENSOR,TURBO>
  MONITOR/MWAIT Features=0x3<CST,INTBRK>
real memory  = 3210796032 (3062 MB)
avail memory = 3008692224 (2869 MB)
lapic: divisor index 0, frequency 99677681 Hz
Initialize MI interrupts
module iwn already present!
VMM: VMENTRY_LOAD_IA32_EFER not supported by this CPU
FQ scheduler policy version 1.1 loaded
wdog: In-kernel automatic watchdog reset enabled
kbd1 at kbdmux0
disk scheduler: set policy of vn0 to noop
disk scheduler: set policy of vn1 to noop
disk scheduler: set policy of vn2 to noop
disk scheduler: set policy of vn3 to noop
disk scheduler: set policy of md0 to noop
md0: Malloc disk
cryptosoft0: <software crypto> on motherboard
aesni0: No AESNI support.
padlock0: No ACE support.
rdrand0: No RdRand support.
pcib0: <Host to PCI bridge> pcibus 0 on motherboard
pci0: <PCI bus> on pcib0
vgapci0: <VGA-compatible display> port 0x8110-0x8117 mem 0xc0000000-0xcfffffff,0xd8100000-0xd81fffff irq 11 at device 2.0 on pci0
agp0: <Intel GM965 SVGA controller> on vgapci0
agp0: aperture size is 256M, detected 7676k stolen memory
vgapci1: <VGA-compatible display> mem 0xd8200000-0xd82fffff at device 2.1 on pci0
uhci0: <Intel 82801H (ICH8) USB controller USB-D> port 0x80c0-0x80df irq 11 at device 26.0 on pci0
usbus0: <Intel 82801H (ICH8) USB controller USB-D> on uhci0
uhci1: <Intel 82801H (ICH8) USB controller USB-E> port 0x80a0-0x80bf irq 10 at device 26.1 on pci0
usbus0: 12Mbps Full Speed USB v1.0
ugen0.1: <Intel> at usbus0
uhub0: <Intel UHCI root HUB, class 9/0, rev 1.00/1.00, addr 1> on usbus0
usbus1: <Intel 82801H (ICH8) USB controller USB-E> on uhci1
ehci0: <Intel 82801H (ICH8) USB 2.0 controller USB2-B> mem 0xdc504c00-0xdc504fff irq 11 at device 26.7 on pci0
usbus2: EHCI version 1.0
usbus1: 12Mbps Full Speed USB v1.0
ugen1.1: <Intel> at usbus1
uhub1: <Intel UHCI root HUB, class 9/0, rev 1.00/1.00, addr 1> on usbus1
usbus2: <Intel 82801H (ICH8) USB 2.0 controller USB2-B> on ehci0
pcm0: <Intel 82801H High Definition Audio Controller> mem 0xdc500000-0xdc503fff irq 11 at device 27.0 on pci0
pcib1: <PCI-PCI bridge> irq 11 at device 28.0 on pci0
pcib1: Disable PCI Express hot-plug interrupts(0x0009)
pci1: <PCI bus> on pcib1
pcib2: <PCI-PCI bridge> irq 11 at device 28.1 on pci0
pcib2: Disable PCI Express hot-plug interrupts(0x0009)
pci2: <PCI bus> on pcib2
pcib3: <PCI-PCI bridge> irq 11 at device 28.2 on pci0
pcib3: Disable PCI Express hot-plug interrupts(0x0009)
pci3: <PCI bus> on pcib3
mskc0: <Marvell Yukon 88E8055 Gigabit Ethernet> port 0x4000-0x40ff mem 0xd9400000-0xd9403fff irq 11 at device 0.0 on pci3
msk0: <Marvell Technology Group Ltd. Yukon EC Ultra Id 0xb4 Rev 0x02> on mskc0
miibus0: <MII bus> on msk0
e1000phy0: <Marvell 88E1149 Gigabit PHY> on miibus0
e1000phy0:  10baseT, 10baseT-FDX, 100baseTX, 100baseTX-FDX, 1000baseT, 1000baseT-FDX, auto
usbus2: 480Mbps High Speed USB v2.0
msk0: MAC address: 00:0a:e4:15:ef:97
pcib4: <PCI-PCI bridge> irq 11 at device 28.3 on pci0
pcib4: Disable PCI Express hot-plug interrupts(0x0009)
pci4: <PCI bus> on pcib4
iwn0: <Intel Wireless WiFi Link 4965> mem 0xd8300000-0xd8301fff irq 11 at device 0.0 on pci4
ugen2.1: <Intel> at usbus2
uhub2: <Intel EHCI root HUB, class 9/0, rev 2.00/1.00, addr 1> on usbus2
uhci2: <Intel 82801H (ICH8) USB controller USB-A> port 0x8080-0x809f irq 11 at device 29.0 on pci0
usbus3: <Intel 82801H (ICH8) USB controller USB-A> on uhci2
uhci3: <Intel 82801H (ICH8) USB controller USB-B> port 0x8060-0x807f irq 11 at device 29.1 on pci0
usbus3: 12Mbps Full Speed USB v1.0
ugen3.1: <Intel> at usbus3
uhub3: <Intel UHCI root HUB, class 9/0, rev 1.00/1.00, addr 1> on usbus3
uhub0: 2 ports with 2 removable, self powered
usbus4: <Intel 82801H (ICH8) USB controller USB-B> on uhci3
uhci4: <Intel 82801H (ICH8) USB controller USB-C> port 0x8040-0x805f irq 11 at device 29.2 on pci0
usbus4: 12Mbps Full Speed USB v1.0
ugen4.1: <Intel> at usbus4
uhub4: <Intel UHCI root HUB, class 9/0, rev 1.00/1.00, addr 1> on usbus4
uhub1: 2 ports with 2 removable, self powered
usbus5: <Intel 82801H (ICH8) USB controller USB-C> on uhci4
ehci1: <Intel 82801H (ICH8) USB 2.0 controller USB2-A> mem 0xdc504800-0xdc504bff irq 11 at device 29.7 on pci0
usbus6: EHCI version 1.0
usbus5: 12Mbps Full Speed USB v1.0
ugen5.1: <Intel> at usbus5
uhub5: <Intel UHCI root HUB, class 9/0, rev 1.00/1.00, addr 1> on usbus5
usbus6: <Intel 82801H (ICH8) USB 2.0 controller USB2-A> on ehci1
pcib5: <PCI-PCI bridge> at device 30.0 on pci0
pci5: <PCI bus> on pcib5
cbb0: <TI6411 PCI-CardBus Bridge> mem 0xd400a000-0xd400afff irq 11 at device 6.0 on pci5
cardbus0: <CardBus bus> on cbb0
pccard0: <16-bit PCCard bus> on cbb0
fwohci0: vendor=104c, dev=8032
fwohci0: <1394 Open Host Controller Interface> mem 0xd4000000-0xd4003fff,0xd400b000-0xd400b7ff irq 10 at device 6.2 on pci5
fwohci0: OHCI version 1.10 (ROM=0)
fwohci0: No. of Isochronous channel is 4.
fwohci0: EUI64 00:0a:e4:08:32:00:00:0d
fwohci0: Phy 1394a available S400, 2 ports.
fwohci0: Link S400, max_rec 2048 bytes.
firewire0: <IEEE1394(FireWire) bus> on fwohci0
fwe0: <Ethernet over FireWire> on firewire0
fwohci0: BUS reset
usbus6: 480Mbps High Speed USB v2.0
fwe0: MAC address: 02:0a:e4:00:00:0d
sbp0: <SBP-2/SCSI over FireWire> on firewire0
fwohci0: Initiate bus reset
Unknown tcode 14
fwohci0: node_id=0xc800ffc0, gen=2, CYCLEMASTER mode
firewire0: 1 nodes, maxhop <= 0, cable IRM = 0 (me)
firewire0: bus manager 0 (me)
pci5: <simple comms> (vendor 0x104c, dev 0x8035) at device 6.5 irq 11
isab0: <PCI-ISA bridge> at device 31.0 on pci0
isa0: <ISA bus> on isab0
atapci0: <Intel ATA controller> port 0x80e0-0x80ef,0x376,0x170-0x177,0x3f6,0x1f0-0x1f7 irq 11 at device 31.1 on pci0
ata0: <ATA channel 0> on atapci0
ugen6.1: <Intel> at usbus6
uhub6: <Intel EHCI root HUB, class 9/0, rev 2.00/1.00, addr 1> on usbus6
disk scheduler: set policy of acd0 to noop
acd0: DVDR <TEAC DV-W28E-R/W.0A> at ata0-slave PIO4
ata1: <ATA channel 1> on atapci0
ahci0: <AHCI-PCI-SATA> port 0x8020-0x803f,0x8118-0x811b,0x80f0-0x80f7,0x811c-0x811f,0x80f8-0x80ff mem 0xdc504000-0xdc5047ff irq 11 at device 31.2 on pci0
uhub3: 2 ports with 2 removable, self powered
uhub4: 2 ports with 2 removable, self powered
uhub5: 2 ports with 2 removable, self powered
uhub2: 4 ports with 4 removable, self powered
ahci0: Intel hocus pocus
ahci0: AHCI 1.1 cap 0xff22ffc2<S64A,NCQ,SSNTF,SMPS,SSS,SALP,SAL,SCLO,SPM,PMD,SSC,PSC,CCCS,EMS>, 3 ports, 32 tags/port, gen 2 (3Gbps)
ahci0.0: Caps 42004<HPCP,MPSS,POD>
ahci0.1: Caps 42004<HPCP,MPSS,POD>
uhub6: 6 ports with 6 removable, self powered
ahci0.2: Caps 42004<HPCP,MPSS,POD>
ahci0.1: No device detected
ahci0.2: No device detected
ahci0.0: PMPROBE(2) No Port Multiplier was found.
ahci0.0: PMPROBE(2) No Port Multiplier was found.
ahci0.0: Found DISK "Hitachi HTS541680J9SA00 SB2OC7KP" serial="SB228DGGKDZL1H"
ahci0.0: tags=32/32 satacap=0502 satacap2=0000 satafea=005e NCQ=YES capacity=76319.08MB
ahci0.0: f85=7469 f86=3c49 f87=4163 WC=enabled RA=enabled SEC=freezing
pci0: <serial bus, SMBus> (vendor 0x8086, dev 0x283e) at device 31.3 irq 11
atkbdc0: <Keyboard controller (i8042)> at port 0x60,0x64 on isa0
atkbd0: <AT Keyboard> irq 1 on atkbdc0
kbd0 at atkbd0
psm0: <PS/2 Mouse> irq 12 on atkbdc0
psm0: model Synaptics Touchpad, device ID 0
vga0: <Generic ISA VGA> at port 0x3c0-0x3df iomem 0xa0000-0xbffff on isa0
sc0: <System console> at flags 0x100 on isa0
sc0: VGA <16 virtual consoles, flags=0x300>
sio0 at port 0x3f8-0x3ff irq 4 flags 0x10 on isa0
sio0: type 16550A
sio1: can't drain, serial port might not exist, disabling
ppc0: cannot reserve I/O port range
hpt27xx: no controller detected.
pcm0: <HDA Codec: Realtek ALC883>
pcm0: <HDA Driver Revision: 20071129_0050>
CAM: Configuring 6 busses
CAM: finished configuring all busses
disk scheduler: set policy of cd0 to noop
disk scheduler: set policy of da0 to noop
da0 at ahci0 bus 0 target 0 lun 0
da0: <SATA Hitachi HTS54168 SB2O> Fixed Direct Access SCSI-4 device 
da0: Serial Number SB228DGGKDZL1H
da0: 150.000MB/s transfers
da0: 76319MB (156301488 512 byte sectors: 255H 63S/T 9729C)
cd0 at ata0 bus 0 target 1 lun 0
cd0: <TEAC DV-W28E-R W.0A> Removable CD-ROM SCSI-0 device 
cd0: 16.000MB/s transfers
cd0: cd present [7104 x 2048 byte records]
no B_DEVMAGIC (bootdev=0)
Mounting root from hammer:serno/SB228DGGKDZL1H.s1d
HAMMER(ROOT) recovery check seqno=010c16b6
HAMMER(ROOT) recovery range 300000001745bc98-30000000174870d0
HAMMER(ROOT) recovery nexto 300000001746e9c8 endseqno=010c183f
HAMMER(ROOT) recovery undo  300000001745bc98-30000000174870d0 (177208 bytes)(RW)
HAMMER(ROOT) Found REDO_SYNC 300000001746ea00
HAMMER(ROOT) recovery complete
HAMMER(ROOT) recovery redo  300000001745bc98-30000000174870d0 (177208 bytes)(RW)
HAMMER(ROOT) Embedded extended redo 300000001746ea00, -77160 extbytes
HAMMER(ROOT) End redo recovery
DMA space used: 6936k, remaining available: 16384k
Mounting devfs
wlan0: MAC address: 00:1f:3b:c8:0a:87
dscheck(cd0): b_bcount 512 is not on a sector boundary (ssize 2048)
dscheck(cd0): b_bcount 512 is not on a sector boundary (ssize 2048)
dscheck(cd0): b_bcount 512 is not on a sector boundary (ssize 2048)
dscheck(cd0): b_bcount 512 is not on a sector boundary (ssize 2048)
dscheck(cd0): b_bcount 512 is not on a sector boundary (ssize 2048)
dscheck(cd0): b_bcount 512 is not on a sector boundary (ssize 2048)
dscheck(cd0): b_bcount 512 is not on a sector boundary (ssize 2048)
dscheck(cd0): b_bcount 512 is not on a sector boundary (ssize 2048)
dscheck(cd0): b_bcount 512 is not on a sector boundary (ssize 2048)
dscheck(cd0): b_bcount 512 is not on a sector boundary (ssize 2048)
dscheck(acd0): b_bcount 512 is not on a sector boundary (ssize 2048)
dscheck(acd0): b_bcount 512 is not on a sector boundary (ssize 2048)
dscheck(acd0): b_bcount 512 is not on a sector boundary (ssize 2048)
dscheck(acd0): b_bcount 512 is not on a sector boundary (ssize 2048)
dscheck(acd0): b_bcount 512 is not on a sector boundary (ssize 2048)
dscheck(acd0): b_bcount 512 is not on a sector boundary (ssize 2048)
dscheck(acd0): b_bcount 512 is not on a sector boundary (ssize 2048)
dscheck(acd0): b_bcount 512 is not on a sector boundary (ssize 2048)
dscheck(acd0): b_bcount 512 is not on a sector boundary (ssize 2048)
dscheck(acd0): b_bcount 512 is not on a sector boundary (ssize 2048)
disk scheduler: set policy of md1 to noop
md1: Malloc disk
dscheck(vn3): b_bcount 2 is not on a sector boundary (ssize 512)
dscheck(vn2): b_bcount 2 is not on a sector boundary (ssize 512)
dscheck(vn1): b_bcount 2 is not on a sector boundary (ssize 512)
dscheck(vn0): b_bcount 2 is not on a sector boundary (ssize 512)
Waiting (max 60 seconds) for system thread swapcached to stop...stopped
Waiting (max 60 seconds) for system thread vnlru to stop...stopped
Waiting (max 60 seconds) for system thread consttyd to stop...stopped
Waiting (max 60 seconds) for system thread bufdaemon_hw to stop...stopped
Waiting (max 60 seconds) for system thread bufdaemon to stop...stopped

syncing disks... 
done
vflush: Warning, cannot destroy busy device vnode
unmount of filesystem mounted from devfs failed (BUSY)
unmount(0xffffffe0214a9e00): Forced unmount: 0 namecache references still present
unmount(0xffffffe0214a9e00): Forced unmount: 2 mount refs still present
Uptime: 9m7s
usbus0: Controller shutdown
uhub0: at usbus0, port 1, addr 1 (disconnected)
uhub0: detached
usbus0: Controller shutdown complete
usbus1: Controller shutdown
uhub1: at usbus1, port 1, addr 1 (disconnected)
uhub1: detached
usbus1: Controller shutdown complete
usbus2: Controller shutdown
uhub2: at usbus2, port 1, addr 1 (disconnected)
uhub2: detached
usbus2: Controller shutdown complete
usbus3: Controller shutdown
uhub3: at usbus3, port 1, addr 1 (disconnected)
uhub3: detached
usbus3: Controller shutdown complete
usbus4: Controller shutdown
uhub4: at usbus4, port 1, addr 1 (disconnected)
uhub4: detached
usbus4: Controller shutdown complete
usbus5: Controller shutdown
uhub5: at usbus5, port 1, addr 1 (disconnected)
uhub5: detached
usbus5: Controller shutdown complete
usbus6: Controller shutdown
uhub6: at usbus6, port 1, addr 1 (disconnected)
uhub6: detached
usbus6: Controller shutdown complete
Rebooting...
Copyright (c) 2003-2014 The DragonFly Project.
Copyright (c) 1992-2003 The FreeBSD Project.
Copyright (c) 1979, 1980, 1983, 1986, 1988, 1989, 1991, 1992, 1993, 1994
	The Regents of the University of California. All rights reserved.
Slab ZoneSize set to 128KB
Leaving critical section, allowing interrupts
ACPI SDT: RSDP not in EBDA
ACPI SDT: RSDP in BIOS mem
ACPI FADT: SCI irq 9, conform/conform
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
DragonFly 55619ec-RELEASE #7: Sat Nov 22 21:25:25 UTC 2014
    root@:/usr/obj/usr/src/sys/X86_64_GENERIC
Calibrating clock(s) ...
TSC clock: 2192856545 Hz, i8254 clock: 1193156 Hz
CLK_USE_I8254_CALIBRATION not specified - using default frequency
CLK_USE_TSC_CALIBRATION not specified - using old calibration method
CPU: Intel(R) Core(TM)2 Duo CPU     T7500  @ 2.20GHz (2192.91-MHz K8-class CPU)
  Origin = "GenuineIntel"  Id = 0x6fb  Stepping = 11
  Features=0xafebfbff<FPU,VME,DE,PSE,TSC,MSR,PAE,MCE,CX8,APIC,SEP,MTRR,PGE,MCA,CMOV,PAT,PSE36,CLFLUSH,DTS,ACPI,MMX,FXSR,SSE,SSE2,SS,TM,PBE>
  Features2=0xe3bd<SSE3,DTES64,MON,DS_CPL,VMX,EST,TM2,SSSE3,CX16,xTPR,PDCM>
  AMD Features=0x20000800<SYSCALL,LM>
  AMD Features2=0x1<LAHF>
  Thermal and PM Features=0x3<SENSOR,TURBO>
  MONITOR/MWAIT Features=0x3<CST,INTBRK>
npx mask: 0x0000ffff
real memory  = 3210796032 (3062 MB)
Physical memory chunk(s):
0x00020000 - 0x0007ffff, 393216 bytes (96 pages)
0x00100000 - 0x001fffff, 1048576 bytes (256 pages)
0x022c0000 - 0xbf4bffff, 3172990976 bytes (774656 pages)
0xbf500000 - 0xbf51ffff, 131072 bytes (32 pages)
0xbf540000 - 0xbf59ffff, 393216 bytes (96 pages)
0xbf5c0000 - 0xbf65ffff, 655360 bytes (160 pages)
avail memory = 3007909888 (2868 MB)
ACPI MADT: LAPIC address 0xfee00000, flags 0x1
ACPI MADT: BSP apic id 0
ACPI MADT: cpu id 1, apic id 0
lapic: divisor index 0, frequency 99677652 Hz
SMP: CPU0 apic_initialize():
     lint0: 0x00000700 lint1: 0x00010400 TPR: 0x00000000 SVR: 0x000001ff
SMP: Waiting APs LAPIC initialization
ELCR Found.  ISA IRQs programmed as:
  0  1  2  3  4  5  6  7  8  9 10 11 12 13 14 15
  E  E  E  E  E  E  E  E  E  E  L  L  E  E  E  E
Initialize MI interrupts
MWAIT hints (2 C1 hints):
  C1/0 hint 0x0000
  C1/1 hint 0x0001
  C2/0 hint 0x0010
  C2/1 hint 0x0011
MWAIT deep hints:
  C1/0 hint 0x0000
  C1/1 hint 0x0001
  C2/0 hint 0x0010
  C2/1 hint 0x0011
  C3/0 hint 0x0020
  C3/1 hint 0x0021
  C4/0 hint 0x0030
  C4/1 hint 0x0031
objcache: magazine cap [6, 134]
Finish MP startup
Active CPU Mask: 0000000000000001
Preloaded elf kernel "kernel" at 0xffffffff81d18000.
Preloaded elf obj module "if_iwi.ko" at 0xffffffff81d18520.
Preloaded elf obj module "sound.ko" at 0xffffffff81d18e40.
Preloaded elf obj module "snd_hda.ko" at 0xffffffff81d197e0.
Preloaded acpi_dsdt "acpi_dsdt.aml" at 0xffffffff81d1a100.
Preloaded elf obj module "acpi.ko" at 0xffffffff81d1a150.
Preloaded elf obj module "ehci.ko" at 0xffffffff81d1a7a8.
Preloaded elf obj module "xhci.ko" at 0xffffffff81d1b000.
Preloaded elf obj module "if_iwn.ko" at 0xffffffff81d1b918.
Preloaded elf obj module "iwn4965fw.ko" at 0xffffffff81d1c1b8.
module iwn already present!
Bits within APICID: logical_CPU_bits: 0; core_bits: 0
CPU Topology: cores_per_chip: 1; threads_per_core: 1; chips_per_package: 1;
VMM: VMENTRY_LOAD_IA32_EFER not supported by this CPU
start dummy scheduler helpers on cpus: 0
Start scheduler helpers on cpus:
	cpu0 - Unknown cpunode->type=1. Siblings:  no siblings
Start scheduler helpers on cpus:
	cpu0 - Unknown cpunode->type=1. Siblings:  no siblings
FQ scheduler policy version 1.1 loaded
wdog: In-kernel automatic watchdog reset enabled
ath_rate: <SampleRate bit-rate selection algorithm>
wlan: <802.11 Link Layer>
ath_dfs: WTF module
firmware: 'iwn4965fw' version 0: 187972 bytes loaded at 0xffffffff81ce50c0
kbd: new array size 4
kbd1 at kbdmux0
No policy for vn0 specified, or policy not found
disk scheduler: set policy of vn0 to noop
No policy for vn1 specified, or policy not found
disk scheduler: set policy of vn1 to noop
No policy for vn2 specified, or policy not found
disk scheduler: set policy of vn2 to noop
No policy for vn3 specified, or policy not found
disk scheduler: set policy of vn3 to noop
crypto: <crypto core>
No policy for md0 specified, or policy not found
disk scheduler: set policy of md0 to noop
md0: Malloc disk
md0: invalid primary partition table: no magic
hpt27xx: RocketRAID 27xx controller driver v1.0 (Nov 22 2014 21:24:20)
hptrr: RocketRAID 17xx/2xxx SATA controller driver v1.2
ICU: rman cpu0 0 - 1
ICU: rman cpu0 3 - 95
ICU: rman cpu0 97 - 191
ACPI: RSDP 0x00000000000FE020 000024 (v02 ITRXGD)
ACPI: XSDT 0x00000000BF6FE120 00006C (v01 ITRXGD ITXGDTBL 00000001      01000013)
ACPI: FACP 0x00000000BF6FD000 0000F4 (v04 ITRXGD ITXGDTBL 00000001 MSFT 01000013)
ACPI BIOS Warning (bug): 32/64X address mismatch in FADT/PmTimerBlock: 0x00000408/0x000000EC6C617470, using 64-bit address (20140424/tbfadt-620)
ACPI BIOS Warning (bug): 32/64X length mismatch in FADT/PmTimerBlock: 32/0 (20140424/tbfadt-648)
ACPI BIOS Warning (bug): 32/64X address mismatch in FADT/Gpe0Block: 0x00000428/0x478B66000000BC90, using 64-bit address (20140424/tbfadt-620)
ACPI BIOS Warning (bug): 32/64X length mismatch in FADT/Gpe0Block: 64/0 (20140424/tbfadt-648)
ACPI BIOS Warning (bug): 32/64X length mismatch in FADT/Gpe1Block: 0/102 (20140424/tbfadt-648)
ACPI BIOS Warning (bug): Optional FADT field Gpe1Block has zero address or length: 0x3064687004478B1A/0x0 (20140424/tbfadt-678)
ACPI BIOS Warning (bug): Invalid length for FADT/PmTimerBlock: 0, using default 32 (20140424/tbfadt-730)
ACPI: DSDT 0x00000000BF6F2000 Logical table override, new table: 0xFFFFFFFF81A6FD00
ACPI: DSDT 0xFFFFFFFF81A6FD00 00A851 (v01 ITRXGD ITXGDTBL 00000001 INTL 20141107)
ACPI: FACS 0x00000000BF685000 000040
ACPI: APIC 0x00000000BF6F1000 000068 (v02 ITRXGD ITXGDTBL 00000001 MSFT 01000013)
ACPI: HPET 0x00000000BF6F0000 000038 (v01 ITRXGD ITXGDTBL 00000001 MSFT 01000013)
ACPI: MCFG 0x00000000BF6EF000 00003C (v01 ITRXGD ITXGDTBL 00000001 MSFT 01000013)
ACPI: SLIC 0x00000000BF6EE000 000176 (v01 ITRXGD ITXGDTBL 00000001 MSFT 01000013)
ACPI: SSDT 0x00000000BF6ED000 00026E (v01 PmRef  Cpu0Ist  00003000 INTL 20051117)
ACPI: SSDT 0x00000000BF6EC000 000481 (v01 PmRef  Cpu0Cst  00003001 INTL 20051117)
ACPI: SSDT 0x00000000BF6EB000 0004C4 (v01 PmRef  CpuPm    00003000 INTL 20051117)
ACPI: SSDT 0x00000000BF6EA000 000232 (v01 PmRef  Cpu0Tst  00003000 INTL 20051117)
cryptosoft0.nexus0.root0
cryptosoft0: <software crypto> [tentative] on motherboard
crypto: assign cryptosoft0 driver id 0, flags 234881024
crypto: cryptosoft0 registers alg 1 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 2 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 3 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 4 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 5 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 16 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 6 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 7 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 18 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 19 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 20 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 8 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 15 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 9 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 10 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 13 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 14 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 11 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 22 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 23 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 24 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 28 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 25 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 26 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 27 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 21 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 29 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 30 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 31 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 32 flags 0 maxoplen 0
crypto: cryptosoft0 registers alg 17 flags 0 maxoplen 0
cryptosoft0: <software crypto> [attached!] on motherboard
aesni0: No AESNI support.
padlock0: No ACE support.
rdrand0: No RdRand support.
acpi0.nexus0.root0
acpi0: <ITRXGD ITXGDTBL> [tentative] on motherboard
ACPI: All ACPI Tables successfully acquired
PCIe: Memory Mapped configuration base @ 0xe0000000, bus [0, 255]
PCIe: Using Memory Mapped configuration
ACPI Error: Unsupported address space: 0x5C (20140424/hwregs-120)
ACPI Exception: AE_SUPPORT, Could not create GPE Block 0 (20140424/evgpeinit-150)
ACPI FADT: SCI testing interrupt mode ...
ACPI FADT: SCI testing level/low
ICU: irq 9, edge -> level
ACPI FADT: SCI select level/low
ACPI: Executed 1 blocks of module-level executable AML code
objcache_reclaimlist
objcache_reclaimlist
objcache_reclaimlist
objcache_reclaimlist
acpi0: Power Button (fixed)
Warning: ACPI is disabling APM's device.  You can't run both
acpi_ec0.acpi0.nexus0.root0
acpi_ec0: <Embedded Controller: GPE 0x17> [tentative] port 0x66,0x62 on acpi0
acpi_ec0: can't install GPE handler for \\_SB_.PCI0.LPC_.EC0_ - AE_BAD_PARAMETER
device_probe_and_attach: acpi_ec0 attach returned 6
pci_link0:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   11   N     0  3 4 5 7 9 10 11 12
  Validation          0   11   N     0  3 4 5 7 9 10 11 12
  After Disable       0  255   N     0  3 4 5 7 9 10 11 12
pci_link1:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   11   N     0  3 4 5 7 9 10 11 12
  Validation          0   11   N     0  3 4 5 7 9 10 11 12
  After Disable       0  255   N     0  3 4 5 7 9 10 11 12
pci_link2:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   11   N     0  3 4 5 7 9 10 11 12
  Validation          0   11   N     0  3 4 5 7 9 10 11 12
  After Disable       0  255   N     0  3 4 5 7 9 10 11 12
pci_link3:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   11   N     0  3 4 5 7 9 10 11 12
  Validation          0   11   N     0  3 4 5 7 9 10 11 12
  After Disable       0  255   N     0  3 4 5 7 9 10 11 12
pci_link4:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0  255   N     0  3 4 5 7 9 10 11 12
  Validation          0  255   N     0  3 4 5 7 9 10 11 12
  After Disable       0  255   N     0  3 4 5 7 9 10 11 12
pci_link5:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   10   N     0  3 4 5 7 9 10 11 12
  Validation          0   10   N     0  3 4 5 7 9 10 11 12
  After Disable       0  255   N     0  3 4 5 7 9 10 11 12
pci_link6:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   11   N     0  3 4 5 7 9 10 11 12
  Validation          0   11   N     0  3 4 5 7 9 10 11 12
  After Disable       0  255   N     0  3 4 5 7 9 10 11 12
pci_link7:        Index  IRQ  Rtd  Ref  IRQs
  Initial Probe       0   11   N     0  3 4 5 7 9 10 11 12
  Validation          0   11   N     0  3 4 5 7 9 10 11 12
  After Disable       0  255   N     0  3 4 5 7 9 10 11 12
acpi_lid0.acpi0.nexus0.root0
acpi_lid0: <Control Method Lid Switch> [tentative] on acpi0
acpi_lid0: enable wake failed
acpi_lid0: <Control Method Lid Switch> [attached!] on acpi0
acpi_button0.acpi0.nexus0.root0
acpi_button0: <Sleep Button> [tentative] on acpi0
acpi_button0: enable wake failed
acpi_button0: <Sleep Button> [attached!] on acpi0
pcib0.acpi0.nexus0.root0
pcib0: <ACPI Host-PCI bridge> [tentative] port 0xcf8-0xcff on acpi0
ACPI: Found matching pin for 0.2.INTA at func 0: 11
ACPI: Found matching pin for 0.26.INTA at func 0: 11
ACPI: Found matching pin for 0.26.INTB at func 1: 10
ACPI: Found matching pin for 0.26.INTC at func 7: 11
ACPI: Found matching pin for 0.27.INTA at func 0: 11
ACPI: Found matching pin for 0.28.INTA at func 0: 11
ACPI: Found matching pin for 0.28.INTB at func 1: 11
ACPI: Found matching pin for 0.28.INTC at func 2: 11
ACPI: Found matching pin for 0.28.INTD at func 3: 11
ACPI: Found matching pin for 0.29.INTA at func 0: 11
ACPI: Found matching pin for 0.29.INTB at func 1: 11
ACPI: Found matching pin for 0.29.INTC at func 2: 11
ACPI: Found matching pin for 0.31.INTB at func 1: 11
ACPI: Found matching pin for 0.31.INTC at func 2: 11
ACPI: Found matching pin for 0.31.INTD at func 3: 11
pci0.pcib0.acpi0.nexus0.root0
pci0: <ACPI PCI bus> [tentative] on pcib0
pci0: domain=0, physical bus=0
found->	vendor=0x8086, dev=0x2a00, revid=0x03
	domain=0, bus=0, slot=0, func=0
	class=06-00-00, hdrtype=0x00, mfdev=0
	cmdreg=0x0006, statreg=0x2090, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
found->	vendor=0x8086, dev=0x2a02, revid=0x03
	domain=0, bus=0, slot=2, func=0
	class=03-00-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0007, statreg=0x0090, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=11
	powerspec 3  supports D0 D3  current D0
	MSI supports 1 message
	map[10]: type Memory, range 64, base 0xd8100000, size 20, enabled
	map[18]: type Prefetchable Memory, range 64, base 0xc0000000, size 28, enabled
	map[20]: type I/O Port, range 32, base 0x8110, size  3, enabled
pcib0: matched entry for 0.2.INTA (src \\_SB_.PCI0.LPC_.LNKA:0)
pcib0: slot 2 INTA routed to irq 11 via \\_SB_.PCI0.LPC_.LNKA
found->	vendor=0x8086, dev=0x2a03, revid=0x03
	domain=0, bus=0, slot=2, func=1
	class=03-80-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0007, statreg=0x0090, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	powerspec 3  supports D0 D3  current D0
	map[10]: type Memory, range 64, base 0xd8200000, size 20, enabled
found->	vendor=0x8086, dev=0x2834, revid=0x03
	domain=0, bus=0, slot=26, func=0
	class=0c-03-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0005, statreg=0x0280, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=11
	map[20]: type I/O Port, range 32, base 0x80c0, size  5, enabled
pcib0: matched entry for 0.26.INTA (src \\_SB_.PCI0.LPC_.LNKA:0)
pcib0: slot 26 INTA routed to irq 11 via \\_SB_.PCI0.LPC_.LNKA
unknown: Reserved 0x20 bytes for rid 0x20 type 4 at 0x80c0
found->	vendor=0x8086, dev=0x2835, revid=0x03
	domain=0, bus=0, slot=26, func=1
	class=0c-03-00, hdrtype=0x00, mfdev=0
	cmdreg=0x0005, statreg=0x0280, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=b, irq=10
	map[20]: type I/O Port, range 32, base 0x80a0, size  5, enabled
pcib0: matched entry for 0.26.INTB (src \\_SB_.PCI0.LPC_.LNKF:0)
pcib0: slot 26 INTB routed to irq 10 via \\_SB_.PCI0.LPC_.LNKF
unknown: Reserved 0x20 bytes for rid 0x20 type 4 at 0x80a0
found->	vendor=0x8086, dev=0x283a, revid=0x03
	domain=0, bus=0, slot=26, func=7
	class=0c-03-20, hdrtype=0x00, mfdev=0
	cmdreg=0x0006, statreg=0x0290, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=c, irq=11
	powerspec 2  supports D0 D3  current D0
	map[10]: type Memory, range 32, base 0xdc504c00, size 10, enabled
pcib0: matched entry for 0.26.INTC (src \\_SB_.PCI0.LPC_.LNKC:0)
pcib0: slot 26 INTC routed to irq 11 via \\_SB_.PCI0.LPC_.LNKC
unknown: Reserved 0x400 bytes for rid 0x10 type 3 at 0xdc504c00
found->	vendor=0x8086, dev=0x284b, revid=0x03
	domain=0, bus=0, slot=27, func=0
	class=04-03-00, hdrtype=0x00, mfdev=0
	cmdreg=0x0006, statreg=0x0010, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=11
	powerspec 2  supports D0 D3  current D0
	MSI supports 1 message, 64 bit
	PCI Express ver.1 cap=0x0091[ROOTDEV]
	map[10]: type Memory, range 64, base 0xdc500000, size 14, enabled
pcib0: matched entry for 0.27.INTA (src \\_SB_.PCI0.LPC_.LNKG:0)
pcib0: slot 27 INTA routed to irq 11 via \\_SB_.PCI0.LPC_.LNKG
found->	vendor=0x8086, dev=0x283f, revid=0x03
	domain=0, bus=0, slot=28, func=0
	class=06-04-00, hdrtype=0x01, mfdev=1
	cmdreg=0x0007, statreg=0x0010, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=11
	powerspec 2  supports D0 D3  current D0
	MSI supports 1 message
	PCI Express ver.1 cap=0x0141[ROOT], slotcap=0x0000a0e0[HOTPLUG]
pcib0: matched entry for 0.28.INTA (src \\_SB_.PCI0.LPC_.LNKB:0)
pcib0: slot 28 INTA routed to irq 11 via \\_SB_.PCI0.LPC_.LNKB
found->	vendor=0x8086, dev=0x2841, revid=0x03
	domain=0, bus=0, slot=28, func=1
	class=06-04-00, hdrtype=0x01, mfdev=1
	cmdreg=0x0007, statreg=0x0010, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=b, irq=11
	powerspec 2  supports D0 D3  current D0
	MSI supports 1 message
	PCI Express ver.1 cap=0x0141[ROOT], slotcap=0x0008a0e0[HOTPLUG]
pcib0: matched entry for 0.28.INTB (src \\_SB_.PCI0.LPC_.LNKA:0)
pcib0: slot 28 INTB routed to irq 11 via \\_SB_.PCI0.LPC_.LNKA
found->	vendor=0x8086, dev=0x2843, revid=0x03
	domain=0, bus=0, slot=28, func=2
	class=06-04-00, hdrtype=0x01, mfdev=1
	cmdreg=0x0007, statreg=0x0010, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=c, irq=11
	powerspec 2  supports D0 D3  current D0
	MSI supports 1 message
	PCI Express ver.1 cap=0x0141[ROOT], slotcap=0x0010a0e0[HOTPLUG]
pcib0: matched entry for 0.28.INTC (src \\_SB_.PCI0.LPC_.LNKC:0)
pcib0: slot 28 INTC routed to irq 11 via \\_SB_.PCI0.LPC_.LNKC
found->	vendor=0x8086, dev=0x2845, revid=0x03
	domain=0, bus=0, slot=28, func=3
	class=06-04-00, hdrtype=0x01, mfdev=1
	cmdreg=0x0007, statreg=0x0010, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=d, irq=11
	powerspec 2  supports D0 D3  current D0
	MSI supports 1 message
	PCI Express ver.1 cap=0x0141[ROOT], slotcap=0x0018a0e0[HOTPLUG]
pcib0: matched entry for 0.28.INTD (src \\_SB_.PCI0.LPC_.LNKD:0)
pcib0: slot 28 INTD routed to irq 11 via \\_SB_.PCI0.LPC_.LNKD
found->	vendor=0x8086, dev=0x2830, revid=0x03
	domain=0, bus=0, slot=29, func=0
	class=0c-03-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0005, statreg=0x0280, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=11
	map[20]: type I/O Port, range 32, base 0x8080, size  5, enabled
pcib0: matched entry for 0.29.INTA (src \\_SB_.PCI0.LPC_.LNKH:0)
pcib0: slot 29 INTA routed to irq 11 via \\_SB_.PCI0.LPC_.LNKH
unknown: Reserved 0x20 bytes for rid 0x20 type 4 at 0x8080
found->	vendor=0x8086, dev=0x2831, revid=0x03
	domain=0, bus=0, slot=29, func=1
	class=0c-03-00, hdrtype=0x00, mfdev=0
	cmdreg=0x0005, statreg=0x0280, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=b, irq=11
	map[20]: type I/O Port, range 32, base 0x8060, size  5, enabled
pcib0: matched entry for 0.29.INTB (src \\_SB_.PCI0.LPC_.LNKD:0)
pcib0: slot 29 INTB routed to irq 11 via \\_SB_.PCI0.LPC_.LNKD
unknown: Reserved 0x20 bytes for rid 0x20 type 4 at 0x8060
found->	vendor=0x8086, dev=0x2832, revid=0x03
	domain=0, bus=0, slot=29, func=2
	class=0c-03-00, hdrtype=0x00, mfdev=0
	cmdreg=0x0005, statreg=0x0280, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=c, irq=11
	map[20]: type I/O Port, range 32, base 0x8040, size  5, enabled
pcib0: matched entry for 0.29.INTC (src \\_SB_.PCI0.LPC_.LNKC:0)
pcib0: slot 29 INTC routed to irq 11 via \\_SB_.PCI0.LPC_.LNKC
unknown: Reserved 0x20 bytes for rid 0x20 type 4 at 0x8040
found->	vendor=0x8086, dev=0x2836, revid=0x03
	domain=0, bus=0, slot=29, func=7
	class=0c-03-20, hdrtype=0x00, mfdev=0
	cmdreg=0x0006, statreg=0x0290, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=11
	powerspec 2  supports D0 D3  current D0
	map[10]: type Memory, range 32, base 0xdc504800, size 10, enabled
pcib0: matched entry for 0.29.INTA (src \\_SB_.PCI0.LPC_.LNKH:0)
pcib0: slot 29 INTA routed to irq 11 via \\_SB_.PCI0.LPC_.LNKH
unknown: Reserved 0x400 bytes for rid 0x10 type 3 at 0xdc504800
found->	vendor=0x8086, dev=0x2448, revid=0xf3
	domain=0, bus=0, slot=30, func=0
	class=06-04-01, hdrtype=0x01, mfdev=0
	cmdreg=0x0007, statreg=0x0010, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
found->	vendor=0x8086, dev=0x2815, revid=0x03
	domain=0, bus=0, slot=31, func=0
	class=06-01-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0007, statreg=0x0210, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
found->	vendor=0x8086, dev=0x2850, revid=0x03
	domain=0, bus=0, slot=31, func=1
	class=01-01-8a, hdrtype=0x00, mfdev=0
	cmdreg=0x0005, statreg=0x0288, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=b, irq=11
	map[20]: type I/O Port, range 32, base 0x80e0, size  4, enabled
pcib0: matched entry for 0.31.INTB (src \\_SB_.PCI0.LPC_.LNKD:0)
pcib0: slot 31 INTB routed to irq 11 via \\_SB_.PCI0.LPC_.LNKD
found->	vendor=0x8086, dev=0x2829, revid=0x03
	domain=0, bus=0, slot=31, func=2
	class=01-06-01, hdrtype=0x00, mfdev=0
	cmdreg=0x0007, statreg=0x02b0, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=c, irq=11
	powerspec 3  supports D0 D3  current D0
	MSI supports 4 messages
	map[10]: type I/O Port, range 32, base 0x80f8, size  3, enabled
	map[14]: type I/O Port, range 32, base 0x811c, size  2, enabled
	map[18]: type I/O Port, range 32, base 0x80f0, size  3, enabled
	map[1c]: type I/O Port, range 32, base 0x8118, size  2, enabled
	map[20]: type I/O Port, range 32, base 0x8020, size  5, enabled
	map[24]: type Memory, range 32, base 0xdc504000, size 11, enabled
pcib0: matched entry for 0.31.INTC (src \\_SB_.PCI0.LPC_.LNKD:0)
pcib0: slot 31 INTC routed to irq 11 via \\_SB_.PCI0.LPC_.LNKD
found->	vendor=0x8086, dev=0x283e, revid=0x03
	domain=0, bus=0, slot=31, func=3
	class=0c-05-00, hdrtype=0x00, mfdev=0
	cmdreg=0x0003, statreg=0x0280, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=d, irq=11
	map[10]: type Memory, range 32, base 0xdc505000, size  8, enabled
	map[20]: type I/O Port, range 32, base 0x8000, size  5, enabled
pcib0: matched entry for 0.31.INTD (src \\_SB_.PCI0.LPC_.LNKD:0)
pcib0: slot 31 INTD routed to irq 11 via \\_SB_.PCI0.LPC_.LNKD
vgapci0.pci0.pcib0.acpi0.nexus0.root0
vgapci0: <VGA-compatible display> [tentative] port 0x8110-0x8117 mem 0xc0000000-0xcfffffff,0xd8100000-0xd81fffff irq 11 at device 2.0 on pci0
agp0.vgapci0.pci0.pcib0.acpi0.nexus0.root0
agp0: <Intel GM965 SVGA controller> [tentative] on vgapci0
vgapci0: Reserved 0x10000000 bytes for rid 0x18 type 3 at 0xc0000000
vgapci0: Reserved 0x100000 bytes for rid 0x10 type 3 at 0xd8100000
agp0: Allocated flush page phys 0x80000000 virt 0xffffffe05b619000
agp0: aperture size is 256M, detected 7676k stolen memory
agp0: AGP_I965_PGTBL_CTL2: 00000000
agp0: AGP_I855_GCC1: 0x30
agp0: AGP_I965_MSAC: 0x00
agp0: Mappable GTT entries: 65536
agp0: Total GTT entries: 131072
agp0: <Intel GM965 SVGA controller> [attached!] on vgapci0
vgapci0: <VGA-compatible display> [attached!] port 0x8110-0x8117 mem 0xc0000000-0xcfffffff,0xd8100000-0xd81fffff irq 11 at device 2.0 on pci0
vgapci1.pci0.pcib0.acpi0.nexus0.root0
vgapci1: <VGA-compatible display> [tentative] mem 0xd8200000-0xd82fffff at device 2.1 on pci0
vgapci1: <VGA-compatible display> [attached!] mem 0xd8200000-0xd82fffff at device 2.1 on pci0
uhci0.pci0.pcib0.acpi0.nexus0.root0
uhci0: <Intel 82801H (ICH8) USB controller USB-D> [tentative] port 0x80c0-0x80df irq 11 at device 26.0 on pci0
usbus0.uhci0.pci0.pcib0.acpi0.nexus0.root0
usbus0: <Intel 82801H (ICH8) USB controller USB-D> [tentative] on uhci0
usbus0: <Intel 82801H (ICH8) USB controller USB-D> [attached!] on uhci0
uhci0: <Intel 82801H (ICH8) USB controller USB-D> [attached!] port 0x80c0-0x80df irq 11 at device 26.0 on pci0
uhci1.pci0.pcib0.acpi0.nexus0.root0
uhci1: <Intel 82801H (ICH8) USB controller USB-E> [tentative] port 0x80a0-0x80bf irq 10 at device 26.1 on pci0
usbus0: 12Mbps Full Speed USB v1.0
ugen0.1: <Intel> at usbus0
uhub0: <Intel UHCI root HUB, class 9/0, rev 1.00/1.00, addr 1> on usbus0
usbus1.uhci1.pci0.pcib0.acpi0.nexus0.root0
usbus1: <Intel 82801H (ICH8) USB controller USB-E> [tentative] on uhci1
usbus1: <Intel 82801H (ICH8) USB controller USB-E> [attached!] on uhci1
uhci1: <Intel 82801H (ICH8) USB controller USB-E> [attached!] port 0x80a0-0x80bf irq 10 at device 26.1 on pci0
ehci0.pci0.pcib0.acpi0.nexus0.root0
ehci0: <Intel 82801H (ICH8) USB 2.0 controller USB2-B> [tentative] mem 0xdc504c00-0xdc504fff irq 11 at device 26.7 on pci0
alignment check failed
usbus2: EHCI version 1.0
usbus1: 12Mbps Full Speed USB v1.0
ugen1.1: <Intel> at usbus1
uhub1: <Intel UHCI root HUB, class 9/0, rev 1.00/1.00, addr 1> on usbus1
usbus2.ehci0.pci0.pcib0.acpi0.nexus0.root0
usbus2: <Intel 82801H (ICH8) USB 2.0 controller USB2-B> [tentative] on ehci0
usbus2: <Intel 82801H (ICH8) USB 2.0 controller USB2-B> [attached!] on ehci0
ehci0: <Intel 82801H (ICH8) USB 2.0 controller USB2-B> [attached!] mem 0xdc504c00-0xdc504fff irq 11 at device 26.7 on pci0
pcm0.pci0.pcib0.acpi0.nexus0.root0
pcm0: <Intel 82801H High Definition Audio Controller> [tentative] mem 0xdc500000-0xdc503fff irq 11 at device 27.0 on pci0
pcm0: device ctrl 0x800
pcm0: disable nosnoop
pcm0: Reserved 0x4000 bytes for rid 0x10 type 3 at 0xdc500000
pcm0: attempting to allocate 1 MSI vector (1 supported)
alloc MSI intr 16 on cpu0
pcm0: using IRQ 16 on cpu0 for MSI
map MSI intr 16 on cpu0
pcm0: <Intel 82801H High Definition Audio Controller> [attached!] mem 0xdc500000-0xdc503fff irq 16,11 at device 27.0 on pci0
pcib1.pci0.pcib0.acpi0.nexus0.root0
pcib1: <ACPI PCI-PCI bridge> [tentative] irq 11 at device 28.0 on pci0
pcib1:   domain            0
pcib1:   secondary bus     1
pcib1:   subordinate bus   1
pcib1:   I/O decode        0x7000-0x7fff
pcib1:   memory decode     0xdb500000-0xdc4fffff
pcib1:   prefetched decode 0xd4100000-0xd50fffff
pcib1: Disable PCI Express hot-plug interrupts(0x0009)
pci1.pcib1.pci0.pcib0.acpi0.nexus0.root0
pci1: <ACPI PCI bus> [tentative] on pcib1
pci1: domain=0, physical bus=1
pci1: <ACPI PCI bus> [attached!] on pcib1
pcib1: <ACPI PCI-PCI bridge> [attached!] irq 11 at device 28.0 on pci0
pcib2.pci0.pcib0.acpi0.nexus0.root0
pcib2: <ACPI PCI-PCI bridge> [tentative] irq 11 at device 28.1 on pci0
pcib2:   domain            0
pcib2:   secondary bus     2
pcib2:   subordinate bus   2
pcib2:   I/O decode        0x6000-0x6fff
pcib2:   memory decode     0xda500000-0xdb4fffff
pcib2:   prefetched decode 0xd5100000-0xd60fffff
pcib2: Disable PCI Express hot-plug interrupts(0x0009)
pci2.pcib2.pci0.pcib0.acpi0.nexus0.root0
pci2: <ACPI PCI bus> [tentative] on pcib2
pci2: domain=0, physical bus=2
pci2: <ACPI PCI bus> [attached!] on pcib2
pcib2: <ACPI PCI-PCI bridge> [attached!] irq 11 at device 28.1 on pci0
pcib3.pci0.pcib0.acpi0.nexus0.root0
pcib3: <ACPI PCI-PCI bridge> [tentative] irq 11 at device 28.2 on pci0
pcib3:   domain            0
pcib3:   secondary bus     3
pcib3:   subordinate bus   3
pcib3:   I/O decode        0x4000-0x5fff
pcib3:   memory decode     0xd9400000-0xda4fffff
pcib3:   prefetched decode 0xd6100000-0xd70fffff
pcib3: Disable PCI Express hot-plug interrupts(0x0009)
ACPI: Found matching pin for 3.0.INTA at func 0: 11
pci3.pcib3.pci0.pcib0.acpi0.nexus0.root0
pci3: <ACPI PCI bus> [tentative] on pcib3
pci3: domain=0, physical bus=3
found->	vendor=0x11ab, dev=0x4363, revid=0x13
	domain=0, bus=3, slot=0, func=0
	class=02-00-00, hdrtype=0x00, mfdev=0
	cmdreg=0x0007, statreg=0x0010, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=11
	powerspec 3  supports D0 D1 D2 D3  current D0
	MSI supports 1 message, 64 bit
	PCI Express ver.1 cap=0x0011[LEGDEV]
	map[10]: type Memory, range 64, base 0xd9400000, size 14, enabled
pcib3: requested memory range 0xd9400000-0xd9403fff: good
	map[18]: type I/O Port, range 32, base 0x4000, size  8, enabled
pcib3: requested I/O range 0x4000-0x40ff: in range
pcib3: matched entry for 3.0.INTA (src \\_SB_.PCI0.LPC_.LNKC:0)
pcib3: slot 0 INTA routed to irq 11 via \\_SB_.PCI0.LPC_.LNKC
mskc0.pci3.pcib3.pci0.pcib0.acpi0.nexus0.root0
mskc0: <Marvell Yukon 88E8055 Gigabit Ethernet> [tentative] port 0x4000-0x40ff mem 0xd9400000-0xd9403fff irq 11 at device 0.0 on pci3
mskc0: Reserved 0x4000 bytes for rid 0x10 type 3 at 0xd9400000
mskc0: RAM buffer size : 0KB
msk0.mskc0.pci3.pcib3.pci0.pcib0.acpi0.nexus0.root0
msk0: <Marvell Technology Group Ltd. Yukon EC Ultra Id 0xb4 Rev 0x02> [tentative] on mskc0
alignment check failed
alignment check failed
miibus0.msk0.mskc0.pci3.pcib3.pci0.pcib0.acpi0.nexus0.root0
miibus0: <MII bus> [tentative] on msk0
e1000phy0.miibus0.msk0.mskc0.pci3.pcib3.pci0.pcib0.acpi0.nexus0.root0
e1000phy0: <Marvell 88E1149 Gigabit PHY> [tentative] on miibus0
e1000phy0:  10baseT, 10baseT-FDX, 100baseTX, 100baseTX-FDX, 1000baseT, 1000baseT-FDX, auto
e1000phy0: <Marvell 88E1149 Gigabit PHY> [attached!] on miibus0
miibus0: <MII bus> [attached!] on msk0
usbus2: 480Mbps High Speed USB v2.0
msk0: bpf attached
msk0: MAC address: 00:0a:e4:15:ef:97
msk0: <Marvell Technology Group Ltd. Yukon EC Ultra Id 0xb4 Rev 0x02> [attached!] on mskc0
mskc0: <Marvell Yukon 88E8055 Gigabit Ethernet> [attached!] port 0x4000-0x40ff mem 0xd9400000-0xd9403fff irq 11 at device 0.0 on pci3
pci3: <ACPI PCI bus> [attached!] on pcib3
pcib3: <ACPI PCI-PCI bridge> [attached!] irq 11 at device 28.2 on pci0
pcib4.pci0.pcib0.acpi0.nexus0.root0
pcib4: <ACPI PCI-PCI bridge> [tentative] irq 11 at device 28.3 on pci0
pcib4:   domain            0
pcib4:   secondary bus     4
pcib4:   subordinate bus   4
pcib4:   I/O decode        0x3000-0x3fff
pcib4:   memory decode     0xd8300000-0xd93fffff
pcib4:   prefetched decode 0xd7100000-0xd80fffff
pcib4: Disable PCI Express hot-plug interrupts(0x0009)
ACPI: Found matching pin for 4.0.INTA at func 0: 11
pci4.pcib4.pci0.pcib0.acpi0.nexus0.root0
pci4: <ACPI PCI bus> [tentative] on pcib4
pci4: domain=0, physical bus=4
found->	vendor=0x8086, dev=0x4229, revid=0x61
	domain=0, bus=4, slot=0, func=0
	class=02-80-00, hdrtype=0x00, mfdev=0
	cmdreg=0x0006, statreg=0x0010, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=11
	powerspec 3  supports D0 D3  current D0
	MSI supports 1 message, 64 bit
	PCI Express ver.1 cap=0x0001[DEVICE]
	map[10]: type Memory, range 64, base 0xd8300000, size 13, enabled
pcib4: requested memory range 0xd8300000-0xd8301fff: good
pcib4: matched entry for 4.0.INTA (src \\_SB_.PCI0.LPC_.LNKD:0)
pcib4: slot 0 INTA routed to irq 11 via \\_SB_.PCI0.LPC_.LNKD
iwn0.pci4.pcib4.pci0.pcib0.acpi0.nexus0.root0
iwn0: <Intel Wireless WiFi Link 4965> [tentative] mem 0xd8300000-0xd8301fff irq 11 at device 0.0 on pci4
iwn0: Reserved 0x2000 bytes for rid 0x10 type 3 at 0xd8300000
iwn0: MIMO 2T3R, MoW1, address 00:1f:3b:c8:0a:87
ugen2.1: <Intel> at usbus2
uhub2: <Intel EHCI root HUB, class 9/0, rev 2.00/1.00, addr 1> on usbus2
iwn0: 11a rates: 6Mbps 9Mbps 12Mbps 18Mbps 24Mbps 36Mbps 48Mbps 54Mbps
iwn0: 11b rates: 1Mbps 2Mbps 5.5Mbps 11Mbps
iwn0: 11g rates: 1Mbps 2Mbps 5.5Mbps 11Mbps 6Mbps 9Mbps 12Mbps 18Mbps 24Mbps 36Mbps 48Mbps 54Mbps
iwn0: 11na MCS: 15Mbps 30Mbps 45Mbps 60Mbps 90Mbps 120Mbps 135Mbps 150Mbps 30Mbps 60Mbps 90Mbps 120Mbps 180Mbps 240Mbps 270Mbps 300Mbps
iwn0: 11ng MCS: 15Mbps 30Mbps 45Mbps 60Mbps 90Mbps 120Mbps 135Mbps 150Mbps 30Mbps 60Mbps 90Mbps 120Mbps 180Mbps 240Mbps 270Mbps 300Mbps
iwn0: <Intel Wireless WiFi Link 4965> [attached!] mem 0xd8300000-0xd8301fff irq 11 at device 0.0 on pci4
pci4: <ACPI PCI bus> [attached!] on pcib4
pcib4: <ACPI PCI-PCI bridge> [attached!] irq 11 at device 28.3 on pci0
uhci2.pci0.pcib0.acpi0.nexus0.root0
uhci2: <Intel 82801H (ICH8) USB controller USB-A> [tentative] port 0x8080-0x809f irq 11 at device 29.0 on pci0
usbus3.uhci2.pci0.pcib0.acpi0.nexus0.root0
usbus3: <Intel 82801H (ICH8) USB controller USB-A> [tentative] on uhci2
usbus3: <Intel 82801H (ICH8) USB controller USB-A> [attached!] on uhci2
uhci2: <Intel 82801H (ICH8) USB controller USB-A> [attached!] port 0x8080-0x809f irq 11 at device 29.0 on pci0
uhci3.pci0.pcib0.acpi0.nexus0.root0
uhci3: <Intel 82801H (ICH8) USB controller USB-B> [tentative] port 0x8060-0x807f irq 11 at device 29.1 on pci0
usbus3: 12Mbps Full Speed USB v1.0
ugen3.1: <Intel> at usbus3
uhub3: <Intel UHCI root HUB, class 9/0, rev 1.00/1.00, addr 1> on usbus3
uhub0: 2 ports with 2 removable, self powered
usbus4.uhci3.pci0.pcib0.acpi0.nexus0.root0
usbus4: <Intel 82801H (ICH8) USB controller USB-B> [tentative] on uhci3
usbus4: <Intel 82801H (ICH8) USB controller USB-B> [attached!] on uhci3
uhci3: <Intel 82801H (ICH8) USB controller USB-B> [attached!] port 0x8060-0x807f irq 11 at device 29.1 on pci0
uhci4.pci0.pcib0.acpi0.nexus0.root0
uhci4: <Intel 82801H (ICH8) USB controller USB-C> [tentative] port 0x8040-0x805f irq 11 at device 29.2 on pci0
usbus4: 12Mbps Full Speed USB v1.0
ugen4.1: <Intel> at usbus4
uhub4: <Intel UHCI root HUB, class 9/0, rev 1.00/1.00, addr 1> on usbus4
uhub1: 2 ports with 2 removable, self powered
usbus5.uhci4.pci0.pcib0.acpi0.nexus0.root0
usbus5: <Intel 82801H (ICH8) USB controller USB-C> [tentative] on uhci4
usbus5: <Intel 82801H (ICH8) USB controller USB-C> [attached!] on uhci4
uhci4: <Intel 82801H (ICH8) USB controller USB-C> [attached!] port 0x8040-0x805f irq 11 at device 29.2 on pci0
ehci1.pci0.pcib0.acpi0.nexus0.root0
ehci1: <Intel 82801H (ICH8) USB 2.0 controller USB2-A> [tentative] mem 0xdc504800-0xdc504bff irq 11 at device 29.7 on pci0
alignment check failed
usbus6: EHCI version 1.0
usbus5: 12Mbps Full Speed USB v1.0
ugen5.1: <Intel> at usbus5
uhub5: <Intel UHCI root HUB, class 9/0, rev 1.00/1.00, addr 1> on usbus5
usbus6.ehci1.pci0.pcib0.acpi0.nexus0.root0
usbus6: <Intel 82801H (ICH8) USB 2.0 controller USB2-A> [tentative] on ehci1
usbus6: <Intel 82801H (ICH8) USB 2.0 controller USB2-A> [attached!] on ehci1
ehci1: <Intel 82801H (ICH8) USB 2.0 controller USB2-A> [attached!] mem 0xdc504800-0xdc504bff irq 11 at device 29.7 on pci0
pcib5.pci0.pcib0.acpi0.nexus0.root0
pcib5: <ACPI PCI-PCI bridge> [tentative] at device 30.0 on pci0
pcib5:   domain            0
pcib5:   secondary bus     5
pcib5:   subordinate bus   6
pcib5:   I/O decode        0x2000-0x2fff
pcib5:   memory decode     0xd2000000-0xd40fffff
pcib5:   prefetched decode 0xd0000000-0xd1ffffff
pcib5:   Subtractively decoded bridge.
ACPI: Found matching pin for 5.6.INTA at func 0: 11
ACPI: Found matching pin for 5.6.INTC at func 2: 10
pci5.pcib5.pci0.pcib0.acpi0.nexus0.root0
pci5: <ACPI PCI bus> [tentative] on pcib5
pci5: domain=0, physical bus=5
found->	vendor=0x104c, dev=0x8031, revid=0x00
	domain=0, bus=5, slot=6, func=0
	class=06-07-00, hdrtype=0x02, mfdev=1
	cmdreg=0x0007, statreg=0x0210, cachelnsz=16 (dwords)
	lattimer=0x40 (1920 ns), mingnt=0xc0 (48000 ns), maxlat=0x02 (500 ns)
	intpin=a, irq=11
	powerspec 2  supports D0 D1 D2 D3  current D0
	map[10]: type Memory, range 32, base 0xd400a000, size 12, enabled
pcib5: requested memory range 0xd400a000-0xd400afff: good
pcib5: matched entry for 5.6.INTA (src \\_SB_.PCI0.LPC_.LNKG:0)
pcib5: slot 6 INTA routed to irq 11 via \\_SB_.PCI0.LPC_.LNKG
found->	vendor=0x104c, dev=0x8032, revid=0x00
	domain=0, bus=5, slot=6, func=2
	class=0c-00-10, hdrtype=0x00, mfdev=1
	cmdreg=0x0016, statreg=0x0210, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x02 (500 ns), maxlat=0x04 (1000 ns)
	intpin=c, irq=10
	powerspec 2  supports D0 D1 D2 D3  current D0
	map[10]: type Memory, range 32, base 0xd400b000, size 11, enabled
pcib5: requested memory range 0xd400b000-0xd400b7ff: good
	map[14]: type Memory, range 32, base 0xd4000000, size 14, enabled
pcib5: requested memory range 0xd4000000-0xd4003fff: good
pcib5: matched entry for 5.6.INTC (src \\_SB_.PCI0.LPC_.LNKF:0)
pcib5: slot 6 INTC routed to irq 10 via \\_SB_.PCI0.LPC_.LNKF
found->	vendor=0x104c, dev=0x8035, revid=0x00
	domain=0, bus=5, slot=6, func=5
	class=07-80-00, hdrtype=0x00, mfdev=1
	cmdreg=0x0002, statreg=0x0210, cachelnsz=0 (dwords)
	lattimer=0x00 (0 ns), mingnt=0x00 (0 ns), maxlat=0x00 (0 ns)
	intpin=a, irq=11
	powerspec 2  supports D0 D1 D2 D3  current D0
	map[10]: type Memory, range 32, base 0xd4009000, size 12, enabled
pcib5: requested memory range 0xd4009000-0xd4009fff: good
	map[14]: type Memory, range 32, base 0xd4008000, size 12, enabled
pcib5: requested memory range 0xd4008000-0xd4008fff: good
	map[18]: type Memory, range 32, base 0xd4007000, size 12, enabled
pcib5: requested memory range 0xd4007000-0xd4007fff: good
	map[1c]: type Memory, range 32, base 0xd4006000, size 12, enabled
pcib5: requested memory range 0xd4006000-0xd4006fff: good
pcib5: matched entry for 5.6.INTA (src \\_SB_.PCI0.LPC_.LNKG:0)
pcib5: slot 6 INTA routed to irq 11 via \\_SB_.PCI0.LPC_.LNKG
cbb0.pci5.pcib5.pci0.pcib0.acpi0.nexus0.root0
cbb0: <TI6411 PCI-CardBus Bridge> [tentative] mem 0xd400a000-0xd400afff irq 11 at device 6.0 on pci5
cbb0: Reserved 0x1000 bytes for rid 0x10 type 3 at 0xd400a000
cardbus0.cbb0.pci5.pcib5.pci0.pcib0.acpi0.nexus0.root0
cardbus0: <CardBus bus> [tentative] on cbb0
cardbus0: <CardBus bus> [attached!] on cbb0
pccard0.cbb0.pci5.pcib5.pci0.pcib0.acpi0.nexus0.root0
pccard0: <16-bit PCCard bus> [tentative] on cbb0
pccard0: <16-bit PCCard bus> [attached!] on cbb0
cbb0: PCI Configuration space:
  0x00: 0x8031104c 0x02100007 0x06070000 0x00824010 
  0x10: 0xd400a000 0x020000a0 0x84060605 0xfffff000 
  0x20: 0x00000000 0xfffff000 0x00000000 0xfffffffc 
  0x30: 0x00000000 0xfffffffc 0x00000000 0x0640010b 
  0x40: 0x202217c0 0x00000001 0x00000000 0x00000000 
  0x50: 0x00000000 0x00000000 0x00000000 0x00000000 
  0x60: 0x00000000 0x00000000 0x00000000 0x00000000 
  0x70: 0x00000000 0x00000000 0x00000000 0x00000000 
  0x80: 0x08445061 0x00000000 0x001f0000 0x01aa1b02 
  0x90: 0x606402c0 0x00000000 0x00000000 0x00000000 
  0xa0: 0xfe120001 0x00c00000 0x00000000 0x00000000 
  0xb0: 0x00000000 0x00000000 0x00000000 0x00000000 
  0xc0: 0x00000000 0x00000000 0x00000000 0x00000000 
  0xd0: 0x00000000 0x00000000 0x00000000 0x00000000 
  0xe0: 0x00000000 0x00000000 0x00000000 0x00000000 
  0xf0: 0x00000000 0x00000000 0x00000000 0x00000000 
cbb0: <TI6411 PCI-CardBus Bridge> [attached!] mem 0xd400a000-0xd400afff irq 11 at device 6.0 on pci5
fwohci0: vendor=104c, dev=8032
fwohci0.pci5.pcib5.pci0.pcib0.acpi0.nexus0.root0
fwohci0: <1394 Open Host Controller Interface> [tentative] mem 0xd4000000-0xd4003fff,0xd400b000-0xd400b7ff irq 10 at device 6.2 on pci5
fwohci0: latency timer 0 -> 32.
fwohci0: cache size 0 -> 8.
fwohci0: Reserved 0x800 bytes for rid 0x10 type 3 at 0xd400b000
fwohci0: OHCI version 1.10 (ROM=0)
fwohci0: No. of Isochronous channel is 4.
fwohci0: EUI64 00:0a:e4:08:32:00:00:0d
fwohci0: resetting OHCI...done (loop=0)
fwohci0: fwphy_rddata: 0x2 loop=0, retry=0
fwohci0: fwphy_rddata: 0x3 loop=0, retry=0
fwohci0: Phy 1394a available S400, 2 ports.
fwohci0: fwphy_rddata: 0x5 loop=0, retry=0
fwohci0: Enable 1394a Enhancements
fwohci0: fwphy_rddata: 0x5 loop=0, retry=0
fwohci0: fwphy_rddata: 0x2 loop=0, retry=0
fwohci0: fwphy_rddata: 0x4 loop=0, retry=0
fwohci0: fwphy_rddata: 0x4 loop=0, retry=0
fwohci0: fwphy_rddata: 0x4 loop=0, retry=0
fwohci0: Link S400, max_rec 2048 bytes.
fwohci0: BUS_OPT 0xa002 -> 0xf800a002
fwohci0: fwohci_set_intr: 1
firewire0.fwohci0.pci5.pcib5.pci0.pcib0.acpi0.nexus0.root0
firewire0: <IEEE1394(FireWire) bus> [tentative] on fwohci0
fwe0.firewire0.fwohci0.pci5.pcib5.pci0.pcib0.acpi0.nexus0.root0
fwe0: <Ethernet over FireWire> [tentative] on firewire0
fwohci0: BUS reset
usbus6: 480Mbps High Speed USB v2.0
fwe0: bpf attached
fwe0: MAC address: 02:0a:e4:00:00:0d
fwe0: <Ethernet over FireWire> [attached!] on firewire0
sbp0.firewire0.fwohci0.pci5.pcib5.pci0.pcib0.acpi0.nexus0.root0
sbp0: <SBP-2/SCSI over FireWire> [tentative] on firewire0
sbp_attach (cold=1)
sbp_post_busreset
sbp_post_explore
sbp0: <SBP-2/SCSI over FireWire> [attached!] on firewire0
sbp_post_busreset
fwohci0: Initiate bus reset
fwohci0: fwphy_rddata: 0x1 loop=0, retry=0
fwohci0: fwphy_rddata: 0x1 loop=0, retry=0
firewire0: <IEEE1394(FireWire) bus> [attached!] on fwohci0
Unknown tcode 14
fwohci0: node_id=0xc800ffc0, gen=2, CYCLEMASTER mode
firewire0: 1 nodes, maxhop <= 0, cable IRM = 0 (me)
fwohci0: fw_set_bus_manager: 0->0 (loop=0)
firewire0: bus manager 0 (me)
send phy_config root_node=-1 gap_count=5
fwohci0: maxdesc: 2
fwohci0: start AT DMA status=0
fwohci0: <1394 Open Host Controller Interface> [attached!] mem 0xd4000000-0xd4003fff,0xd400b000-0xd400b7ff irq 10 at device 6.2 on pci5
pci5: <simple comms> (vendor 0x104c, dev 0x8035) at device 6.5 irq 11
pci5: <ACPI PCI bus> [attached!] on pcib5
pcib5: <ACPI PCI-PCI bridge> [attached!] at device 30.0 on pci0
isab0.pci0.pcib0.acpi0.nexus0.root0
isab0: <PCI-ISA bridge> [tentative] at device 31.0 on pci0
isa0.isab0.pci0.pcib0.acpi0.nexus0.root0
isa0: <ISA bus> [tentative] on isab0
isa0: <ISA bus> [attached!] on isab0
isab0: <PCI-ISA bridge> [attached!] at device 31.0 on pci0
atapci0.pci0.pcib0.acpi0.nexus0.root0
atapci0: <Intel ATA controller> [tentative] port 0x80e0-0x80ef,0x376,0x170-0x177,0x3f6,0x1f0-0x1f7 irq 11 at device 31.1 on pci0
atapci0: Reserved 0x10 bytes for rid 0x20 type 4 at 0x80e0
ata0.atapci0.pci0.pcib0.acpi0.nexus0.root0
ata0: <ATA channel 0> [tentative] on atapci0
atapci0: Reserved 0x8 bytes for rid 0x10 type 4 at 0x1f0
atapci0: Reserved 0x1 bytes for rid 0x14 type 4 at 0x3f6
ata0: reset tp1 mask=03 ostat0=00 ostat1=50
ata0: stat0=0x7f err=0x00 lsb=0x00 msb=0x7f
ata0: stat1=0x00 err=0x01 lsb=0x14 msb=0xeb
ata0: reset tp2 stat0=7f stat1=00 devices=0x8<ATAPI_SLAVE>
Current DB 0
ch = 0
 Current OP   KEY INT BR   len     Addr   Depend Stat: Cnt
53036000 OUTL ST2 ALL ALL    12 00000000 53036080 8411:000c RUN,ACTIVE, ack complete(11)
0x000000e0 0x00450000 0xffbaffff 0x00000000
ugen6.1: <Intel> at usbus6
uhub6: <Intel EHCI root HUB, class 9/0, rev 2.00/1.00, addr 1> on usbus6
uhub3: 2 ports with 2 removable, self powered
ata0-slave: pio=PIO4 wdma=WDMA2 udma=UDMA33 cable=80 wire
No policy for acd0 specified, or policy not found
disk scheduler: set policy of acd0 to noop
acd0: <TEAC DV-W28E-R/W.0A> DVDR drive at ata0 as slave
acd0: read 4133KB/s (4133KB/s) write 4133KB/s (4133KB/s), 2000KB buffer, PIO4
acd0: Reads: CDR, CDRW, CDDA stream, DVDROM, DVDR, DVDRAM, packet
acd0: Writes: CDR, CDRW, DVDR, DVDRAM, test write, burnproof
acd0: Audio: play, 256 volume levels
acd0: Mechanism: ejectable tray, unlocked
acd0: Medium: CD-R 120mm data disc
ata0: <ATA channel 0> [attached!] on atapci0
ata1.atapci0.pci0.pcib0.acpi0.nexus0.root0
ata1: <ATA channel 1> [tentative] on atapci0
atapci0: Reserved 0x8 bytes for rid 0x18 type 4 at 0x170
atapci0: Reserved 0x1 bytes for rid 0x1c type 4 at 0x376
ata1: reset tp1 mask=03 ostat0=7f ostat1=7f
ata1: stat0=0x7f err=0x7f lsb=0x7f msb=0x7f
ata1: stat0=0x7f err=0x7f lsb=0x7f msb=0x7f
ata1: stat0=0x7f err=0x7f lsb=0x7f msb=0x7f
ata1: stat0=0x7f err=0x7f lsb=0x7f msb=0x7f
ata1: stat0=0x7f err=0x7f lsb=0x7f msb=0x7f
ata1: stat0=0x7f err=0x7f lsb=0x7f msb=0x7f
ata1: stat0=0x7f err=0x7f lsb=0x7f msb=0x7f
ata1: stat0=0x7f err=0x7f lsb=0x7f msb=0x7f
ata1: stat0=0x7f err=0x7f lsb=0x7f msb=0x7f
ata1: stat0=0x7f err=0x7f lsb=0x7f msb=0x7f
ata1: stat0=0x7f err=0x7f lsb=0x7f msb=0x7f
ata1: stat0=0x7f err=0x7f lsb=0x7f msb=0x7f
ata1: stat1=0x7f err=0x7f lsb=0x7f msb=0x7f
ata1: reset tp2 stat0=ff stat1=ff devices=0x0
ata1: <ATA channel 1> [attached!] on atapci0
atapci0: <Intel ATA controller> [attached!] port 0x80e0-0x80ef,0x376,0x170-0x177,0x3f6,0x1f0-0x1f7 irq 11 at device 31.1 on pci0
ahci0.pci0.pcib0.acpi0.nexus0.root0
ahci0: <AHCI-PCI-SATA> [tentative] port 0x8020-0x803f,0x8118-0x811b,0x80f0-0x80f7,0x811c-0x811f,0x80f8-0x80ff mem 0xdc504000-0xdc5047ff irq 11 at device 31.2 on pci0
ahci0: attempting to allocate 1 MSI vector (4 supported)
alloc MSI intr 17 on cpu0
ahci0: using IRQ 17 on cpu0 for MSI
ahci0: Reserved 0x800 bytes for rid 0x24 type 3 at 0xdc504000
bus_explore done
sbp_post_explore
uhub4: 2 ports with 2 removable, self powered
uhub5: 2 ports with 2 removable, self powered
uhub2: 4 ports with 4 removable, self powered
(probe0:ata0:0:1:0): error 22
(probe0:ata0:0:1:0): Unretryable Error
(probe0:ata0:0:1:0): Down reving Protocol Version from 2 to 0?
ahci0: Intel hocus pocus
ahci0: AHCI 1.1 cap 0xff22ffc2<S64A,NCQ,SSNTF,SMPS,SSS,SALP,SAL,SCLO,SPM,PMD,SSC,PSC,CCCS,EMS>, 3 ports, 32 tags/port, gen 2 (3Gbps)
ahci0.0: Caps 42004<HPCP,MPSS,POD>
ahci0.1: Caps 42004<HPCP,MPSS,POD>
ahci0.0: START HARDRESET
uhub6: 6 ports with 6 removable, self powered
ahci0.2: Caps 42004<HPCP,MPSS,POD>
ahci0.1: START HARDRESET
map MSI intr 17 on cpu0
ahci0.2: START HARDRESET
ahci0.1: Port appears to be unplugged
ahci0.1: No device detected
ahci0.1: END HARDRESET 19
ahci0.2: Port appears to be unplugged
ahci0.2: No device detected
ahci0.2: END HARDRESET 19
ahci0.0: PMPROBE(2) No Port Multiplier was found.
ahci0.0: PMPROBE(2) No Port Multiplier was found.
ahci0.0: END HARDRESET 0
ahci0.0: START SOFTRESET 4e017<HPCP,CR,FR,MPSS,FRE,POD,SUD,ST>
ahci0.0: sig 00000101
ahci0.0: END SOFTRESET
ahci0.0: Found DISK "Hitachi HTS541680J9SA00 SB2OC7KP" serial="SB228DGGKDZL1H"
ahci0.0: tags=32/32 satacap=0502 satacap2=0000 satafea=005e NCQ=YES capacity=76319.08MB
ahci0.0: f85=7469 f86=3c49 f87=4163 WC=enabled RA=enabled SEC=frozen
ahci0.0: Set dummy xfer mode to 45
(probe0:ahci0:0:1:0): error 22
(probe0:ahci0:0:1:0): Unretryable Error
(probe0:ahci0:0:2:0): error 22
(probe0:ahci0:0:2:0): Unretryable Error
(probe0:ahci0:0:3:0): error 22
(probe0:ahci0:0:3:0): Unretryable Error
(probe0:ahci0:0:4:0): error 22
(probe0:ahci0:0:4:0): Unretryable Error
(probe0:ahci0:0:5:0): error 22
(probe0:ahci0:0:5:0): Unretryable Error
(probe0:ahci0:0:6:0): error 22
(probe0:ahci0:0:6:0): Unretryable Error
(probe0:ahci0:0:7:0): error 22
(probe0:ahci0:0:7:0): Unretryable Error
(probe0:ahci0:0:8:0): error 22
(probe0:ahci0:0:8:0): Unretryable Error
(probe0:ahci0:0:9:0): error 22
(probe0:ahci0:0:9:0): Unretryable Error
(probe0:ahci0:0:10:0): error 22
(probe0:ahci0:0:10:0): Unretryable Error
(probe0:ahci0:0:11:0): error 22
(probe0:ahci0:0:11:0): Unretryable Error
(probe0:ahci0:0:12:0): error 22
(probe0:ahci0:0:12:0): Unretryable Error
(probe0:ahci0:0:13:0): error 22
(probe0:ahci0:0:13:0): Unretryable Error
(probe0:ahci0:0:14:0): error 22
(probe0:ahci0:0:14:0): Unretryable Error
(probe0:ahci0:1:0:0): error 22
(probe0:ahci0:1:0:0): Unretryable Error
(probe0:ahci0:1:1:0): error 22
(probe0:ahci0:1:1:0): Unretryable Error
(probe0:ahci0:1:2:0): error 22
(probe0:ahci0:1:2:0): Unretryable Error
(probe0:ahci0:1:3:0): error 22
(probe0:ahci0:1:3:0): Unretryable Error
(probe0:ahci0:1:4:0): error 22
(probe0:ahci0:1:4:0): Unretryable Error
(probe0:ahci0:1:5:0): error 22
(probe0:ahci0:1:5:0): Unretryable Error
(probe0:ahci0:1:6:0): error 22
(probe0:ahci0:1:6:0): Unretryable Error
(probe0:ahci0:1:7:0): error 22
(probe0:ahci0:1:7:0): Unretryable Error
(probe0:ahci0:1:8:0): error 22
(probe0:ahci0:1:8:0): Unretryable Error
(probe0:ahci0:1:9:0): error 22
(probe0:ahci0:1:9:0): Unretryable Error
(probe0:ahci0:1:10:0): error 22
(probe0:ahci0:1:10:0): Unretryable Error
(probe0:ahci0:1:11:0): error 22
(probe0:ahci0:1:11:0): Unretryable Error
(probe0:ahci0:1:12:0): error 22
(probe0:ahci0:1:12:0): Unretryable Error
(probe0:ahci0:1:13:0): error 22
(probe0:ahci0:1:13:0): Unretryable Error
(probe0:ahci0:1:14:0): error 22
(probe0:ahci0:1:14:0): Unretryable Error
(probe0:ahci0:2:0:0): error 22
(probe0:ahci0:2:0:0): Unretryable Error
(probe0:ahci0:2:1:0): error 22
(probe0:ahci0:2:1:0): Unretryable Error
(probe0:ahci0:2:2:0): error 22
(probe0:ahci0:2:2:0): Unretryable Error
(probe0:ahci0:2:3:0): error 22
(probe0:ahci0:2:3:0): Unretryable Error
(probe0:ahci0:2:4:0): error 22
(probe0:ahci0:2:4:0): Unretryable Error
(probe0:ahci0:2:5:0): error 22
(probe0:ahci0:2:5:0): Unretryable Error
(probe0:ahci0:2:6:0): error 22
(probe0:ahci0:2:6:0): Unretryable Error
(probe0:ahci0:2:7:0): error 22
(probe0:ahci0:2:7:0): Unretryable Error
(probe0:ahci0:2:8:0): error 22
(probe0:ahci0:2:8:0): Unretryable Error
(probe0:ahci0:2:9:0): error 22
(probe0:ahci0:2:9:0): Unretryable Error
(probe0:ahci0:2:10:0): error 22
(probe0:ahci0:2:10:0): Unretryable Error
(probe0:ahci0:2:11:0): error 22
(probe0:ahci0:2:11:0): Unretryable Error
(probe0:ahci0:2:12:0): error 22
(probe0:ahci0:2:12:0): Unretryable Error
(probe0:ahci0:2:13:0): error 22
(probe0:ahci0:2:13:0): Unretryable Error
(probe0:ahci0:2:14:0): error 22
(probe0:ahci0:2:14:0): Unretryable Error
ahci0: <AHCI-PCI-SATA> [attached!] port 0x8020-0x803f,0x8118-0x811b,0x80f0-0x80f7,0x811c-0x811f,0x80f8-0x80ff mem 0xdc504000-0xdc5047ff irq 17,11 at device 31.2 on pci0
pci0: <serial bus, SMBus> (vendor 0x8086, dev 0x283e) at device 31.3 irq 11
pci0: <ACPI PCI bus> [attached!] on pcib0
pcib0: <ACPI Host-PCI bridge> [attached!] port 0xcf8-0xcff on acpi0
acpi_tz0.acpi0.nexus0.root0
acpi_tz0: <Thermal Zone> [tentative] on acpi0
acpi_tz0: <Thermal Zone> [attached!] on acpi0
acpi_tz1.acpi0.nexus0.root0
acpi_tz1: <Thermal Zone> [tentative] on acpi0
acpi_tz1: <Thermal Zone> [attached!] on acpi0
acpi_tz2.acpi0.nexus0.root0
acpi_tz2: <Thermal Zone> [tentative] on acpi0
acpi_tz2: <Thermal Zone> [attached!] on acpi0
acpi_tz3.acpi0.nexus0.root0
acpi_tz3: <Thermal Zone> [tentative] on acpi0
acpi_tz3: <Thermal Zone> [attached!] on acpi0
atkbdc0.acpi0.nexus0.root0
atkbdc0: <Keyboard controller (i8042)> [tentative] port 0x64,0x60 irq 1 on acpi0
atkbd0.atkbdc0.acpi0.nexus0.root0
atkbd0: <AT Keyboard> [tentative] irq 1 on atkbdc0
kbd0 at atkbd0
kbd0: atkbd0, generic (0), config:0x0, flags:0x3d0000
atkbd0: <AT Keyboard> [attached!] irq 1 on atkbdc0
psm0: current command byte:0067
psm0.atkbdc0.acpi0.nexus0.root0
psm0: <PS/2 Mouse> [tentative] irq 12 on atkbdc0
psm0: model Synaptics Touchpad, device ID 0-00, 4 buttons
psm0: config:00006000, flags:00000008, packet size:6
psm0: syncmask:c0, syncbits:00
psm0: <PS/2 Mouse> [attached!] irq 12 on atkbdc0
atkbdc0: <Keyboard controller (i8042)> [attached!] port 0x64,0x60 irq 1 on acpi0
sio0: irq maps: 0x1 0x11 0x1 0x1
sio0.acpi0.nexus0.root0
sio0: <16550A-compatible COM port> [tentative] port 0x3f8-0x3ff irq 4 on acpi0
sio0: type 16550A
sio0: <16550A-compatible COM port> [attached!] port 0x3f8-0x3ff irq 4 on acpi0
sio1: irq maps: 0x1 0x41 0x1 0x1
sio1.acpi0.nexus0.root0
sio1: <16550A-compatible COM port> [tentative] port 0x6f0-0x6f7 irq 6 on acpi0
sio1: type 16550A
sio1: <16550A-compatible COM port> [attached!] port 0x6f0-0x6f7 irq 6 on acpi0
sio2: irq maps: 0x1 0x21 0x1 0x1
sio2.acpi0.nexus0.root0
sio2: <16550A-compatible COM port> [tentative] port 0x6f8-0x6ff irq 5 on acpi0
sio2: type 16550A
sio2: <16550A-compatible COM port> [attached!] port 0x6f8-0x6ff irq 5 on acpi0
unknown: not probed (disabled)
unknown: not probed (disabled)
unknown: not probed (disabled)
unknown: not probed (disabled)
unknown: not probed (disabled)
battery0.acpi0.nexus0.root0
battery0: <ACPI Control Method Battery> [tentative] on acpi0
battery0: <ACPI Control Method Battery> [attached!] on acpi0
acpi_acad0.acpi0.nexus0.root0
acpi_acad0: <AC Adapter> [tentative] on acpi0
acpi_acad0: <AC Adapter> [attached!] on acpi0
cpu0.acpi0.nexus0.root0
cpu0: <ACPI CPU> [tentative] on acpi0
cpu_cst0.cpu0.acpi0.nexus0.root0
cpu_cst0: <ACPI CPU C-State> [tentative] on cpu0
C2: BitWidth(vendor) 1, BitOffset(class) 2, Address(arg0) 0x10, AccessWidth(arg1) 0x1
C2 -> cpu specific C2 sub state 0
C3: BitWidth(vendor) 1, BitOffset(class) 2, Address(arg0) 0x20, AccessWidth(arg1) 0x3
C3 -> cpu specific C3 sub state 0
cpu_cst0: non-C3 0
cpu_cst0: <ACPI CPU C-State> [attached!] on cpu0
cpu_pst0.cpu0.acpi0.nexus0.root0
cpu_pst0: <ACPI CPU P-State> [tentative] on cpu0
cpu_pst0: create pkg domain0, coord 0xfc
cpu_pst0: control reg 127 0
cpu_pst0: status reg 127 0
cpu_pst0: freq 2201, pwr 35000, xlat 10, blat 10, cv 00000c2f, sv 00000c2f
cpu_pst0: freq 2200, pwr 35000, xlat 10, blat 10, cv 00000b2b, sv 00000b2b
cpu_pst0: freq 1600, pwr 23672, xlat 10, blat 10, cv 0000081f, sv 0000081f
cpu_pst0: freq 1200, pwr 16120, xlat 10, blat 10, cv 00000617, sv 00000617
cpu_pst0: freq 600, pwr 8060, xlat 10, blat 10, cv 00008617, sv 00008617
cpu_pst0: _PPC 0
cpu_pst0: <ACPI CPU P-State> [attached!] on cpu0
clockmod0.cpu0.acpi0.nexus0.root0
clockmod0: <CPU clock modulation> [tentative] on cpu0
clock modulation:
  0x0000 100.00%
  0x001e 87.50%
  0x001c 75.00%
  0x001a 62.50%
  0x0018 50.00%
  0x0016 37.50%
  0x0014 25.00%
  0x0012 12.50%
clockmod0: <CPU clock modulation> [attached!] on cpu0
coretemp0.cpu0.acpi0.nexus0.root0
coretemp0: <CPU On-Die Thermal Sensors> [tentative] on cpu0
coretemp0: Setting TjMax=100
coretemp0: <CPU On-Die Thermal Sensors> [attached!] on cpu0
cpu0: <ACPI CPU> [attached!] on acpi0
acpi_ec0.acpi0.nexus0.root0
acpi_ec0: <Embedded Controller: GPE 0x17> [tentative] port 0x66,0x62 on acpi0
acpi_ec0: can't install GPE handler for \\_SB_.PCI0.LPC_.EC0_ - AE_BAD_PARAMETER
device_probe_and_attach: acpi_ec0 attach returned 6
unknown: not probed (disabled)
unknown: not probed (disabled)
unknown: not probed (disabled)
unknown: not probed (disabled)
unknown: not probed (disabled)
acpi0: <ITRXGD ITXGDTBL> [attached!] at port 0x2e-0x2f,0x4e-0x4f,0x162e-0x162f,0x164e-0x164f,0x61,0x70,0x80,0x92,0xb2-0xb3,0x63,0x65,0x67,0x600-0x60f,0x610,0x800-0x80f,0x400-0x47f,0x500-0x53f,0x200-0x20f iomem 0xe0000000-0xefffffff,0xfed1c000-0xfed1ffff,0xfed14000-0xfed17fff,0xfed18000-0xfed18fff,0xfed19000-0xfed19fff,0xfed30000-0xfed30fff,0xfec00000-0xfec00fff,0xfee00000-0xfee00fff irq 9 on motherboard
atkbdc-: atkbdc0 exists, using next available unit number
sio-: sio0 exists, using next available unit number
sio-: sio1 exists, using next available unit number
sio-: sio2 exists, using next available unit number
sio-: sio3 exists, using next available unit number
Trying Read_Port at 203
Trying Read_Port at 243
Trying Read_Port at 283
Trying Read_Port at 2c3
Trying Read_Port at 303
Trying Read_Port at 343
Trying Read_Port at 383
Trying Read_Port at 3c3
isa_probe_children: disabling PnP devices
isa_probe_children: probing non-PnP devices
pmtimer0.isa0.isab0.pci0.pcib0.acpi0.nexus0.root0
pmtimer0 [tentative] on isa0
pmtimer0 [attached!] on isa0
adv0 [tentative] failed to probe on isa0
atkbdc1: <Keyboard controller (i8042)> [tentative] failed to probe at port 0x60 on isa0
vga0.isa0.isab0.pci0.pcib0.acpi0.nexus0.root0
vga0: <Generic ISA VGA> [tentative] at port 0x3c0-0x3df iomem 0xa0000-0xbffff on isa0
fb0: vga0, vga, type:VGA (5), flags:0x7007f
fb0: port:0x3c0-0x3df, mem:0xa0000 0x20000
fb0: init mode:24, bios mode:3, current mode:24
fb0: window:0xffffffff800b8000 size:32k gran:32k, buf:0 size:32k
VGA parameters upon power-up
 50 18 10 00 00 00 03 00 02 67 5f 4f 50 82 55 81
 bf 1f 00 4f 0d 0e 00 00 07 80 9c 8e 8f 28 1f 96
 b9 a3 ff 00 01 02 03 04 05 14 07 38 39 3a 3b 3c
 3d 3e 3f 0c 00 0f 08 00 00 00 00 00 10 0e 00 ff
VGA parameters in BIOS for mode 24
 50 18 10 00 10 00 03 00 02 67 5f 4f 50 82 55 81
 bf 1f 00 4f 0d 0e 00 00 00 00 9c 8e 8f 28 1f 96
 b9 a3 ff 00 01 02 03 04 05 14 07 38 39 3a 3b 3c
 3d 3e 3f 0c 00 0f 08 00 00 00 00 00 10 0e 00 ff
VGA parameters to be used for mode 24
 50 18 10 00 10 00 03 00 02 67 5f 4f 50 82 55 81
 bf 1f 00 4f 0d 0e 00 00 00 00 9c 8e 8f 28 1f 96
 b9 a3 ff 00 01 02 03 04 05 14 07 38 39 3a 3b 3c
 3d 3e 3f 0c 00 0f 08 00 00 00 00 00 10 0e 00 ff
vga0: <Generic ISA VGA> [attached!] at port 0x3c0-0x3df iomem 0xa0000-0xbffff on isa0
sc0.isa0.isab0.pci0.pcib0.acpi0.nexus0.root0
sc0: <System console> [tentative] at flags 0x100 on isa0
sc0: VGA <16 virtual consoles, flags=0x300>
sc0: fb0, kbd1, terminal emulator: sc (syscons terminal)
sc0: <System console> [attached!] at flags 0x100 on isa0
lm0 [tentative] failed to probe at port 0x290-0x297 on isa0
it0 [tentative] failed to probe at port 0x290-0x297 on isa0
it1 [tentative] failed to probe at port 0xc00-0xc07 on isa0
it2 [tentative] failed to probe at port 0xd00-0xd07 on isa0
it3 [tentative] failed to probe at port 0x228-0x22f on isa0
wbsio0: wbsio_probe port 0x2e: Device ID 0xea, Rev 0x11
wbsio0 [tentative] failed to probe at port 0x2e-0x2f on isa0
wbsio1 [tentative] failed to probe at port 0x4e-0x4f on isa0
sio3 [tentative] failed to probe at port 0x3f8 irq 4 flags 0x10 on isa0
sio4: can't drain, serial port might not exist, disabling
sio4 [tentative] failed to probe at port 0x2f8-0x2ff irq 3 on isa0
sio5: not probed (disabled)
sio6: not probed (disabled)
ppc0: cannot reserve I/O port range
ppc0: <Parallel port> [tentative] failed to probe at irq 7 on isa0
ed0: not probed (disabled)
lnc0: not probed (disabled)
cs0: not probed (disabled)
sn0: not probed (disabled)
isa_probe_children: probing PnP devices
battery0: battery initialization start
ACPI Error: No handler for Region [RAM_] (0xffffffe0215e2478) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BST] (Node 0xffffffe0096f88e8), AE_NOT_EXIST (20140424/psparse-553)
battery0: error fetching current battery status -- AE_NOT_EXIST
ACPI Error: No handler for Region [RAM_] (0xffffffe0215e2478) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BIF] (Node 0xffffffe0096f88a0), AE_NOT_EXIST (20140424/psparse-553)
battery0: error fetching current battery info -- AE_NOT_EXIST
faith0: bpf attached
lo0: bpf attached
ppp0: bpf attached
sl0: bpf attached
hpt27xx: no controller detected.
hptrr: no controller detected.
pcm0: Mixer "vol": child=0x00000010
pcm0: Mixer "pcm": parent="vol"
pcm0: Mixer "mic":
pcm0: Mixer "rec":
pcm0: Soft PCM mixer ENABLED
pcm0: sndbuf_setmap 2720000, 4000; 0xffffffe06ce2b000 -> 2720000
pcm0: sndbuf_setmap 2724000, 4000; 0xffffffe06ce33000 -> 2724000
pcm0: <HDA Codec: Realtek ALC883>
pcm0: <HDA Driver Revision: 20071129_0050>
CAM: Configuring bus: sbp0
CAM: Configuring bus: ata0
CAM: Configuring bus: ata1
CAM: Configuring bus: ahci0
CAM: Configuring bus: ahci0
CAM: Configuring bus: ahci0
CAM: Configuring 6 busses
(probe0:sbp0:0:0:0): error 22
(probe0:sbp0:0:0:0): Unretryable Error
(probe1:sbp0:0:1:0): error 22
(probe1:sbp0:0:1:0): Unretryable Error
(probe2:sbp0:0:2:0): error 22
(probe2:sbp0:0:2:0): Unretryable Error
(probe3:sbp0:0:3:0): error 22
(probe3:sbp0:0:3:0): Unretryable Error
(probe4:sbp0:0:4:0): error 22
(probe4:sbp0:0:4:0): Unretryable Error
(probe5:sbp0:0:5:0): error 22
(probe5:sbp0:0:5:0): Unretryable Error
(probe6:sbp0:0:6:0): error 22
(probe6:sbp0:0:6:0): Unretryable Error
CAM: Finished configuring bus: sbp0
CAM: Finished configuring bus: ata1
(probe0:ahci0:0:1:0): error 22
(probe0:ahci0:0:1:0): Unretryable Error
(probe0:ahci0:0:2:0): error 22
(probe0:ahci0:0:2:0): Unretryable Error
(probe0:ahci0:0:3:0): error 22
(probe0:ahci0:0:3:0): Unretryable Error
(probe0:ahci0:0:4:0): error 22
(probe0:ahci0:0:4:0): Unretryable Error
(probe0:ahci0:0:5:0): error 22
(probe0:ahci0:0:5:0): Unretryable Error
(probe0:ahci0:0:6:0): error 22
(probe0:ahci0:0:6:0): Unretryable Error
(probe0:ahci0:0:7:0): error 22
(probe0:ahci0:0:7:0): Unretryable Error
(probe0:ahci0:0:8:0): error 22
(probe0:ahci0:0:8:0): Unretryable Error
(probe0:ahci0:0:9:0): error 22
(probe0:ahci0:0:9:0): Unretryable Error
(probe0:ahci0:0:10:0): error 22
(probe0:ahci0:0:10:0): Unretryable Error
(probe0:ahci0:0:11:0): error 22
(probe0:ahci0:0:11:0): Unretryable Error
(probe0:ahci0:0:12:0): error 22
(probe0:ahci0:0:12:0): Unretryable Error
(probe0:ahci0:0:13:0): error 22
(probe0:ahci0:0:13:0): Unretryable Error
(probe0:ahci0:0:14:0): error 22
(probe0:ahci0:0:14:0): Unretryable Error
CAM: Finished configuring bus: ahci0
(probe9:ahci0:1:0:0): error 22
(probe9:ahci0:1:0:0): Unretryable Error
(probe0:ahci0:1:1:0): error 22
(probe0:ahci0:1:1:0): Unretryable Error
(probe0:ahci0:1:2:0): error 22
(probe0:ahci0:1:2:0): Unretryable Error
(probe0:ahci0:1:3:0): error 22
(probe0:ahci0:1:3:0): Unretryable Error
(probe0:ahci0:1:4:0): error 22
(probe0:ahci0:1:4:0): Unretryable Error
(probe0:ahci0:1:5:0): error 22
(probe0:ahci0:1:5:0): Unretryable Error
(probe0:ahci0:1:6:0): error 22
(probe0:ahci0:1:6:0): Unretryable Error
(probe0:ahci0:1:7:0): error 22
(probe0:ahci0:1:7:0): Unretryable Error
(probe0:ahci0:1:8:0): error 22
(probe0:ahci0:1:8:0): Unretryable Error
(probe0:ahci0:1:9:0): error 22
(probe0:ahci0:1:9:0): Unretryable Error
(probe0:ahci0:1:10:0): error 22
(probe0:ahci0:1:10:0): Unretryable Error
(probe0:ahci0:1:11:0): error 22
(probe0:ahci0:1:11:0): Unretryable Error
(probe0:ahci0:1:12:0): error 22
(probe0:ahci0:1:12:0): Unretryable Error
(probe0:ahci0:1:13:0): error 22
(probe0:ahci0:1:13:0): Unretryable Error
(probe0:ahci0:1:14:0): error 22
(probe0:ahci0:1:14:0): Unretryable Error
CAM: Finished configuring bus: ahci0
(probe10:ahci0:2:0:0): error 22
(probe10:ahci0:2:0:0): Unretryable Error
(probe0:ahci0:2:1:0): error 22
(probe0:ahci0:2:1:0): Unretryable Error
(probe0:ahci0:2:2:0): error 22
(probe0:ahci0:2:2:0): Unretryable Error
(probe0:ahci0:2:3:0): error 22
(probe0:ahci0:2:3:0): Unretryable Error
(probe0:ahci0:2:4:0): error 22
(probe0:ahci0:2:4:0): Unretryable Error
(probe0:ahci0:2:5:0): error 22
(probe0:ahci0:2:5:0): Unretryable Error
(probe0:ahci0:2:6:0): error 22
(probe0:ahci0:2:6:0): Unretryable Error
(probe0:ahci0:2:7:0): error 22
(probe0:ahci0:2:7:0): Unretryable Error
(probe0:ahci0:2:8:0): error 22
(probe0:ahci0:2:8:0): Unretryable Error
(probe0:ahci0:2:9:0): error 22
(probe0:ahci0:2:9:0): Unretryable Error
(probe0:ahci0:2:10:0): error 22
(probe0:ahci0:2:10:0): Unretryable Error
(probe0:ahci0:2:11:0): error 22
(probe0:ahci0:2:11:0): Unretryable Error
(probe0:ahci0:2:12:0): error 22
(probe0:ahci0:2:12:0): Unretryable Error
(probe0:ahci0:2:13:0): error 22
(probe0:ahci0:2:13:0): Unretryable Error
(probe0:ahci0:2:14:0): error 22
(probe0:ahci0:2:14:0): Unretryable Error
CAM: Finished configuring bus: ahci0
(probe7:ata0:0:1:0): error 22
(probe7:ata0:0:1:0): Unretryable Error
CAM: Finished configuring bus: ata0
CAM: finished configuring all busses
pass0 at ata0 bus 0 target 1 lun 0
pass0: <TEAC DV-W28E-R W.0A> Removable CD-ROM SCSI-0 device 
pass0: 16.000MB/s transfers
pass1 at ahci0 bus 0 target 0 lun 0
pass1: <SATA Hitachi HTS54168 SB2O> Fixed Direct Access SCSI-4 device 
pass1: Serial Number SB228DGGKDZL1H
pass1: 150.000MB/s transfers
sg0 at ata0 bus 0 target 1 lun 0
sg0: <TEAC DV-W28E-R W.0A> Removable CD-ROM SCSI-0 device 
sg0: 16.000MB/s transfers
sg1 at ahci0 bus 0 target 0 lun 0
sg1: <SATA Hitachi HTS54168 SB2O> Fixed Direct Access SCSI-4 device 
sg1: Serial Number SB228DGGKDZL1H
sg1: 150.000MB/s transfers
No policy for da0 specified, or policy not found
disk scheduler: set policy of da0 to noop
da0: si_iosize_max:131072
No policy for cd0 specified, or policy not found
disk scheduler: set policy of cd0 to noop
da0 at ahci0 bus 0 target 0 lun 0
da0: <SATA Hitachi HTS54168 SB2O> Fixed Direct Access SCSI-4 device 
da0: Serial Number SB228DGGKDZL1H
da0: 150.000MB/s transfers
da0: 76319MB (156301488 512 byte sectors: 255H 63S/T 9729C)
cd0 at ata0 bus 0 target 1 lun 0
cd0: <TEAC DV-W28E-R W.0A> Removable CD-ROM SCSI-0 device 
cd0: 16.000MB/s transfers
cd0: cd present [7104 x 2048 byte records]
da0: type 0xa5, start 63, end = 156296447, size 156296385 : OK
cd0: invalid primary partition table: no magic
cd0: invalid primary partition table: no magic
cd0: invalid primary partition table: no magic
no B_DEVMAGIC (bootdev=0)
ATA PseudoRAID loaded
Mounting root from hammer:serno/SB228DGGKDZL1H.s1d
HAMMER(ROOT) recovery check seqno=010c3439
HAMMER(ROOT) recovery range 3000000017797838-3000000017797838
HAMMER(ROOT) recovery nexto 3000000017797838 endseqno=010c343a
HAMMER(ROOT) mounted clean, no recovery needed
DMA space used: 6936k, remaining available: 16384k
Mounting devfs
start_init: trying /sbin/init
ACPI Error: No handler for Region [RAM_] (0xffffffe0215e2478) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BIF] (Node 0xffffffe0096f88a0), AE_NOT_EXIST (20140424/psparse-553)
battery0: error fetching current battery info -- AE_NOT_EXIST
ACPI Error: No handler for Region [RAM_] (0xffffffe0215e2478) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BIF] (Node 0xffffffe0096f88a0), AE_NOT_EXIST (20140424/psparse-553)
battery0: error fetching current battery info -- AE_NOT_EXIST
ACPI Error: No handler for Region [RAM_] (0xffffffe0215e2478) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BST] (Node 0xffffffe0096f88e8), AE_NOT_EXIST (20140424/psparse-553)
battery0: error fetching current battery status -- AE_NOT_EXIST
ACPI Error: No handler for Region [RAM_] (0xffffffe0215e2478) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BST] (Node 0xffffffe0096f88e8), AE_NOT_EXIST (20140424/psparse-553)
battery0: error fetching current battery status -- AE_NOT_EXIST
ACPI Error: No handler for Region [RAM_] (0xffffffe0215e2478) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BST] (Node 0xffffffe0096f88e8), AE_NOT_EXIST (20140424/psparse-553)
battery0: error fetching current battery status -- AE_NOT_EXIST
ACPI Error: No handler for Region [RAM_] (0xffffffe0215e2478) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BST] (Node 0xffffffe0096f88e8), AE_NOT_EXIST (20140424/psparse-553)
battery0: error fetching current battery status -- AE_NOT_EXIST
ACPI Error: No handler for Region [RAM_] (0xffffffe0215e2478) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BST] (Node 0xffffffe0096f88e8), AE_NOT_EXIST (20140424/psparse-553)
battery0: error fetching current battery status -- AE_NOT_EXIST
ACPI Error: No handler for Region [RAM_] (0xffffffe0215e2478) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BST] (Node 0xffffffe0096f88e8), AE_NOT_EXIST (20140424/psparse-553)
battery0: error fetching current battery status -- AE_NOT_EXIST
ACPI Error: No handler for Region [RAM_] (0xffffffe0215e2478) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.ADP1._PSR] (Node 0xffffffe0096f8df8), AE_NOT_EXIST (20140424/psparse-553)
ACPI Error: No handler for Region [RAM_] (0xffffffe0215e2478) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.ADP1._PSR] (Node 0xffffffe0096f8df8), AE_NOT_EXIST (20140424/psparse-553)
kthread 0xffffffe0214f1e80 syncer6 has exited
ACPI Error: No handler for Region [RAM_] (0xffffffe0215e2478) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BIF] (Node 0xffffffe0096f88a0), AE_NOT_EXIST (20140424/psparse-553)
battery0: error fetching current battery info -- AE_NOT_EXIST
kthread 0xffffffe0214f1900 syncer7 has exited
kthread 0xffffffe0214f1e80 syncer8 has exited
kthread 0xffffffe0214f1900 syncer9 has exited
kthread 0xffffffe0214f1e80 syncer10 has exited
kthread 0xffffffe0214f1900 syncer11 has exited
kthread 0xffffffe0214f1e80 syncer12 has exited
wlan0: bpf attached
wlan0: bpf attached
wlan0: MAC address: 00:1f:3b:c8:0a:87
ACPI Error: No handler for Region [RAM_] (0xffffffe0215e2478) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BIF] (Node 0xffffffe0096f88a0), AE_NOT_EXIST (20140424/psparse-553)
battery0: error fetching current battery info -- AE_NOT_EXIST
ACPI Error: No handler for Region [RAM_] (0xffffffe0215e2478) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BIF] (Node 0xffffffe0096f88a0), AE_NOT_EXIST (20140424/psparse-553)
battery0: error fetching current battery info -- AE_NOT_EXIST
