Copyright (c) 2003-2014 The DragonFly Project.
Copyright (c) 1992-2003 The FreeBSD Project.
Copyright (c) 1979, 1980, 1983, 1986, 1988, 1989, 1991, 1992, 1993, 1994
	The Regents of the University of California. All rights reserved.
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
MPTABLE: warning PCI int dst apic id 2 does not exist
DragonFly 55619ec-RELEASE #7: Sat Nov 22 21:25:25 UTC 2014
    root@:/usr/obj/usr/src/sys/X86_64_GENERIC
TSC clock: 2192850000 Hz, i8254 clock: 1193153 Hz
CPU: Intel(R) Core(TM)2 Duo CPU     T7500  @ 2.20GHz (2192.91-MHz K8-class CPU)
  Origin = "GenuineIntel"  Id = 0x6fb  Stepping = 11
  Features=0xafebfbff<FPU,VME,DE,PSE,TSC,MSR,PAE,MCE,CX8,APIC,SEP,MTRR,PGE,MCA,CMOV,PAT,PSE36,CLFLUSH,DTS,ACPI,MMX,FXSR,SSE,SSE2,SS,TM,PBE>
  Features2=0xe3bd<SSE3,DTES64,MON,DS_CPL,VMX,EST,TM2,SSSE3,CX16,xTPR,PDCM>
  AMD Features=0x20000800<SYSCALL,LM>
  AMD Features2=0x1<LAHF>
  Thermal and PM Features=0x3<SENSOR,TURBO>
  MONITOR/MWAIT Features=0x3<CST,INTBRK>
real memory  = 3210796032 (3062 MB)
avail memory = 3002417152 (2863 MB)
lapic: divisor index 0, frequency 99677611 Hz
Initialize MI interrupts
module iwn already present!
VMM: VMENTRY_LOAD_IA32_EFER not supported by this CPU
FQ scheduler policy version 1.1 loaded
wdog: In-kernel automatic watchdog reset enabled
kbd1 at kbdmux0
disk scheduler: set policy of vn0 to noop
disk scheduler: set policy of vn1 to noop
disk scheduler: set policy of vn2 to noop
disk scheduler: set policy of vn3 to noop
disk scheduler: set policy of md0 to noop
md0: Malloc disk
ACPI: RSDP 0x00000000000FE020 000024 (v02 ITRXGD)
ACPI: XSDT 0x00000000BF6FE120 00006C (v01 ITRXGD ITXGDTBL 00000001      01000013)
ACPI: FACP 0x00000000BF6FD000 0000F4 (v04 ITRXGD ITXGDTBL 00000001 MSFT 01000013)
ACPI BIOS Warning (bug): 32/64X address mismatch in FADT/PmTimerBlock: 0x00000408/0x000000EC6C617470, using 64-bit address (20140424/tbfadt-620)
ACPI BIOS Warning (bug): 32/64X length mismatch in FADT/PmTimerBlock: 32/0 (20140424/tbfadt-648)
ACPI BIOS Warning (bug): 32/64X address mismatch in FADT/Gpe0Block: 0x00000428/0x478B66000000BC90, using 64-bit address (20140424/tbfadt-620)
ACPI BIOS Warning (bug): 32/64X length mismatch in FADT/Gpe0Block: 64/0 (20140424/tbfadt-648)
ACPI BIOS Warning (bug): 32/64X length mismatch in FADT/Gpe1Block: 0/102 (20140424/tbfadt-648)
ACPI BIOS Warning (bug): Optional FADT field Gpe1Block has zero address or length: 0x3064687004478B1A/0x0 (20140424/tbfadt-678)
ACPI BIOS Warning (bug): Invalid length for FADT/PmTimerBlock: 0, using default 32 (20140424/tbfadt-730)
ACPI: DSDT 0x00000000BF6F2000 Logical table override, new table: 0xFFFFFFFF81832C60
ACPI: DSDT 0xFFFFFFFF81832C60 00A851 (v01 ITRXGD ITXGDTBL 00000001 INTL 20141107)
ACPI: FACS 0x00000000BF685000 000040
ACPI: APIC 0x00000000BF6F1000 000068 (v02 ITRXGD ITXGDTBL 00000001 MSFT 01000013)
ACPI: HPET 0x00000000BF6F0000 000038 (v01 ITRXGD ITXGDTBL 00000001 MSFT 01000013)
ACPI: MCFG 0x00000000BF6EF000 00003C (v01 ITRXGD ITXGDTBL 00000001 MSFT 01000013)
ACPI: SLIC 0x00000000BF6EE000 000176 (v01 ITRXGD ITXGDTBL 00000001 MSFT 01000013)
ACPI: SSDT 0x00000000BF6ED000 00026E (v01 PmRef  Cpu0Ist  00003000 INTL 20051117)
ACPI: SSDT 0x00000000BF6EC000 000481 (v01 PmRef  Cpu0Cst  00003001 INTL 20051117)
ACPI: SSDT 0x00000000BF6EB000 0004C4 (v01 PmRef  CpuPm    00003000 INTL 20051117)
ACPI: SSDT 0x00000000BF6EA000 000232 (v01 PmRef  Cpu0Tst  00003000 INTL 20051117)
cryptosoft0: <software crypto> on motherboard
aesni0: No AESNI support.
padlock0: No ACE support.
rdrand0: No RdRand support.
acpi0: <ITRXGD ITXGDTBL> on motherboard
ACPI: Overriding _OS definition with "Windows 2001"
ACPI: All ACPI Tables successfully acquired
ACPI Error: Unsupported address space: 0x5C (20140424/hwregs-120)
ACPI Exception: AE_SUPPORT, Could not create GPE Block 0 (20140424/evgpeinit-150)
ACPI FADT: SCI testing interrupt mode ...
ACPI FADT: SCI select level/low
ACPI: Executed 1 blocks of module-level executable AML code
objcache_reclaimlist
objcache_reclaimlist
objcache_reclaimlist
objcache_reclaimlist
acpi0: Power Button (fixed)
Warning: ACPI is disabling APM's device.  You can't run both
acpi_ec0: <Embedded Controller: GPE 0x17> port 0x66,0x62 on acpi0
acpi_ec0: can't install GPE handler for \\_SB_.PCI0.LPC_.EC0_ - AE_BAD_PARAMETER
device_probe_and_attach: acpi_ec0 attach returned 6
acpi_lid0: <Control Method Lid Switch> on acpi0
acpi_lid0: enable wake failed
acpi_button0: <Sleep Button> on acpi0
acpi_button0: enable wake failed
pcib0: <ACPI Host-PCI bridge> port 0xcf8-0xcff on acpi0
pci0: <ACPI PCI bus> on pcib0
vgapci0: <VGA-compatible display> port 0x8110-0x8117 mem 0xc0000000-0xcfffffff,0xd8100000-0xd81fffff irq 11 at device 2.0 on pci0
agp0: <Intel GM965 SVGA controller> on vgapci0
agp0: aperture size is 256M, detected 7676k stolen memory
vgapci1: <VGA-compatible display> mem 0xd8200000-0xd82fffff at device 2.1 on pci0
uhci0: <Intel 82801H (ICH8) USB controller USB-D> port 0x80c0-0x80df irq 11 at device 26.0 on pci0
usbus0: <Intel 82801H (ICH8) USB controller USB-D> on uhci0
uhci1: <Intel 82801H (ICH8) USB controller USB-E> port 0x80a0-0x80bf irq 10 at device 26.1 on pci0
usbus0: 12Mbps Full Speed USB v1.0
ugen0.1: <Intel> at usbus0
uhub0: <Intel UHCI root HUB, class 9/0, rev 1.00/1.00, addr 1> on usbus0
usbus1: <Intel 82801H (ICH8) USB controller USB-E> on uhci1
ehci0: <Intel 82801H (ICH8) USB 2.0 controller USB2-B> mem 0xdc504c00-0xdc504fff irq 11 at device 26.7 on pci0
usbus2: EHCI version 1.0
usbus1: 12Mbps Full Speed USB v1.0
ugen1.1: <Intel> at usbus1
uhub1: <Intel UHCI root HUB, class 9/0, rev 1.00/1.00, addr 1> on usbus1
usbus2: <Intel 82801H (ICH8) USB 2.0 controller USB2-B> on ehci0
pci0: <multimedia, HDA> (vendor 0x8086, dev 0x284b) at device 27.0 irq 11
pcib1: <ACPI PCI-PCI bridge> irq 11 at device 28.0 on pci0
pcib1: Disable PCI Express hot-plug interrupts(0x0009)
pci1: <ACPI PCI bus> on pcib1
pcib2: <ACPI PCI-PCI bridge> irq 11 at device 28.1 on pci0
pcib2: Disable PCI Express hot-plug interrupts(0x0009)
pci2: <ACPI PCI bus> on pcib2
pcib3: <ACPI PCI-PCI bridge> irq 11 at device 28.2 on pci0
pcib3: Disable PCI Express hot-plug interrupts(0x0009)
pci3: <ACPI PCI bus> on pcib3
mskc0: <Marvell Yukon 88E8055 Gigabit Ethernet> port 0x4000-0x40ff mem 0xd9400000-0xd9403fff irq 11 at device 0.0 on pci3
msk0: <Marvell Technology Group Ltd. Yukon EC Ultra Id 0xb4 Rev 0x02> on mskc0
miibus0: <MII bus> on msk0
e1000phy0: <Marvell 88E1149 Gigabit PHY> on miibus0
e1000phy0:  10baseT, 10baseT-FDX, 100baseTX, 100baseTX-FDX, 1000baseT, 1000baseT-FDX, auto
usbus2: 480Mbps High Speed USB v2.0
msk0: MAC address: 00:0a:e4:15:ef:97
pcib4: <ACPI PCI-PCI bridge> irq 11 at device 28.3 on pci0
pcib4: Disable PCI Express hot-plug interrupts(0x0009)
pci4: <ACPI PCI bus> on pcib4
iwn0: <Intel Wireless WiFi Link 4965> mem 0xd8300000-0xd8301fff irq 11 at device 0.0 on pci4
ugen2.1: <Intel> at usbus2
uhub2: <Intel EHCI root HUB, class 9/0, rev 2.00/1.00, addr 1> on usbus2
uhci2: <Intel 82801H (ICH8) USB controller USB-A> port 0x8080-0x809f irq 11 at device 29.0 on pci0
usbus3: <Intel 82801H (ICH8) USB controller USB-A> on uhci2
uhci3: <Intel 82801H (ICH8) USB controller USB-B> port 0x8060-0x807f irq 11 at device 29.1 on pci0
usbus3: 12Mbps Full Speed USB v1.0
ugen3.1: <Intel> at usbus3
uhub3: <Intel UHCI root HUB, class 9/0, rev 1.00/1.00, addr 1> on usbus3
uhub0: 2 ports with 2 removable, self powered
usbus4: <Intel 82801H (ICH8) USB controller USB-B> on uhci3
uhci4: <Intel 82801H (ICH8) USB controller USB-C> port 0x8040-0x805f irq 11 at device 29.2 on pci0
usbus4: 12Mbps Full Speed USB v1.0
ugen4.1: <Intel> at usbus4
uhub4: <Intel UHCI root HUB, class 9/0, rev 1.00/1.00, addr 1> on usbus4
uhub1: 2 ports with 2 removable, self powered
usbus5: <Intel 82801H (ICH8) USB controller USB-C> on uhci4
ehci1: <Intel 82801H (ICH8) USB 2.0 controller USB2-A> mem 0xdc504800-0xdc504bff irq 11 at device 29.7 on pci0
usbus6: EHCI version 1.0
usbus5: 12Mbps Full Speed USB v1.0
ugen5.1: <Intel> at usbus5
uhub5: <Intel UHCI root HUB, class 9/0, rev 1.00/1.00, addr 1> on usbus5
usbus6: <Intel 82801H (ICH8) USB 2.0 controller USB2-A> on ehci1
pcib5: <ACPI PCI-PCI bridge> at device 30.0 on pci0
pci5: <ACPI PCI bus> on pcib5
cbb0: <TI6411 PCI-CardBus Bridge> mem 0xd400a000-0xd400afff irq 11 at device 6.0 on pci5
cardbus0: <CardBus bus> on cbb0
pccard0: <16-bit PCCard bus> on cbb0
fwohci0: vendor=104c, dev=8032
fwohci0: <1394 Open Host Controller Interface> mem 0xd4000000-0xd4003fff,0xd400b000-0xd400b7ff irq 10 at device 6.2 on pci5
fwohci0: OHCI version 1.10 (ROM=0)
fwohci0: No. of Isochronous channel is 4.
fwohci0: EUI64 00:0a:e4:08:32:00:00:0d
fwohci0: Phy 1394a available S400, 2 ports.
fwohci0: Link S400, max_rec 2048 bytes.
firewire0: <IEEE1394(FireWire) bus> on fwohci0
fwe0: <Ethernet over FireWire> on firewire0
fwohci0: BUS reset
usbus6: 480Mbps High Speed USB v2.0
fwe0: MAC address: 02:0a:e4:00:00:0d
sbp0: <SBP-2/SCSI over FireWire> on firewire0
fwohci0: Initiate bus reset
Unknown tcode 14
fwohci0: node_id=0xc800ffc0, gen=2, CYCLEMASTER mode
firewire0: 1 nodes, maxhop <= 0, cable IRM = 0 (me)
firewire0: bus manager 0 (me)
pci5: <simple comms> (vendor 0x104c, dev 0x8035) at device 6.5 irq 11
isab0: <PCI-ISA bridge> at device 31.0 on pci0
isa0: <ISA bus> on isab0
atapci0: <Intel ATA controller> port 0x80e0-0x80ef,0x376,0x170-0x177,0x3f6,0x1f0-0x1f7 irq 11 at device 31.1 on pci0
ata0: <ATA channel 0> on atapci0
ugen6.1: <Intel> at usbus6
uhub6: <Intel EHCI root HUB, class 9/0, rev 2.00/1.00, addr 1> on usbus6
disk scheduler: set policy of acd0 to noop
acd0: DVDR <TEAC DV-W28E-R/W.0A> at ata0-slave UDMA33
ata1: <ATA channel 1> on atapci0
ahci0: <AHCI-PCI-SATA> port 0x8020-0x803f,0x8118-0x811b,0x80f0-0x80f7,0x811c-0x811f,0x80f8-0x80ff mem 0xdc504000-0xdc5047ff irq 11 at device 31.2 on pci0
uhub3: 2 ports with 2 removable, self powered
uhub4: 2 ports with 2 removable, self powered
uhub5: 2 ports with 2 removable, self powered
uhub2: 4 ports with 4 removable, self powered
ahci0: Intel hocus pocus
ahci0: AHCI 1.1 cap 0xff22ffc2<S64A,NCQ,SSNTF,SMPS,SSS,SALP,SAL,SCLO,SPM,PMD,SSC,PSC,CCCS,EMS>, 3 ports, 32 tags/port, gen 2 (3Gbps)
ahci0.0: Caps 42004<HPCP,MPSS,POD>
ahci0.1: Caps 42004<HPCP,MPSS,POD>
uhub6: 6 ports with 6 removable, self powered
ahci0.2: Caps 42004<HPCP,MPSS,POD>
ahci0.1: No device detected
ahci0.2: No device detected
ahci0.0: PMPROBE(2) No Port Multiplier was found.
ahci0.0: PMPROBE(2) No Port Multiplier was found.
ahci0.0: Found DISK "Hitachi HTS541680J9SA00 SB2OC7KP" serial="SB228DGGKDZL1H"
ahci0.0: tags=32/32 satacap=0502 satacap2=0000 satafea=005e NCQ=YES capacity=76319.08MB
ahci0.0: f85=7469 f86=3c49 f87=4163 WC=enabled RA=enabled SEC=freezing
pci0: <serial bus, SMBus> (vendor 0x8086, dev 0x283e) at device 31.3 irq 11
acpi_tz0: <Thermal Zone> on acpi0
acpi_tz1: <Thermal Zone> on acpi0
acpi_tz2: <Thermal Zone> on acpi0
acpi_tz3: <Thermal Zone> on acpi0
atkbdc0: <Keyboard controller (i8042)> port 0x64,0x60 irq 1 on acpi0
atkbd0: <AT Keyboard> irq 1 on atkbdc0
kbd0 at atkbd0
psm0: <PS/2 Mouse> irq 12 on atkbdc0
psm0: model Synaptics Touchpad, device ID 0
sio0: <16550A-compatible COM port> port 0x3f8-0x3ff irq 4 on acpi0
sio0: type 16550A
sio1: <16550A-compatible COM port> port 0x6f0-0x6f7 irq 6 on acpi0
sio1: type 16550A
sio2: <16550A-compatible COM port> port 0x6f8-0x6ff irq 5 on acpi0
sio2: type 16550A
battery0: <ACPI Control Method Battery> on acpi0
acpi_acad0: <AC Adapter> on acpi0
cpu0: <ACPI CPU> on acpi0
cpu_cst0: <ACPI CPU C-State> on cpu0
cpu_pst0: <ACPI CPU P-State> on cpu0
clockmod0: <CPU clock modulation> on cpu0
coretemp0: <CPU On-Die Thermal Sensors> on cpu0
acpi_ec0: <Embedded Controller: GPE 0x17> port 0x66,0x62 on acpi0
acpi_ec0: can't install GPE handler for \\_SB_.PCI0.LPC_.EC0_ - AE_BAD_PARAMETER
device_probe_and_attach: acpi_ec0 attach returned 6
pmtimer0 on isa0
vga0: <Generic ISA VGA> at port 0x3c0-0x3df iomem 0xa0000-0xbffff on isa0
sc0: <System console> at flags 0x100 on isa0
sc0: VGA <16 virtual consoles, flags=0x300>
sio4: can't drain, serial port might not exist, disabling
ppc0: cannot reserve I/O port range
ACPI Error: No handler for Region [RAM_] (0xffffffe021521438) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BST] (Node 0xffffffe0096f88a0), AE_NOT_EXIST (20140424/psparse-553)
ACPI Error: No handler for Region [RAM_] (0xffffffe021521438) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BIF] (Node 0xffffffe0096f8858), AE_NOT_EXIST (20140424/psparse-553)
hpt27xx: no controller detected.
CAM: Configuring 6 busses
CAM: finished configuring all busses
disk scheduler: set policy of da0 to noop
disk scheduler: set policy of cd0 to noop
da0 at ahci0 bus 0 target 0 lun 0
da0: <SATA Hitachi HTS54168 SB2O> Fixed Direct Access SCSI-4 device 
da0: Serial Number SB228DGGKDZL1H
da0: 150.000MB/s transfers
da0: 76319MB (156301488 512 byte sectors: 255H 63S/T 9729C)
cd0 at ata0 bus 0 target 1 lun 0
cd0: <TEAC DV-W28E-R W.0A> Removable CD-ROM SCSI-0 device 
cd0: 33.000MB/s transfers
cd0: cd present [7104 x 2048 byte records]
no B_DEVMAGIC (bootdev=0)
Mounting root from hammer:serno/SB228DGGKDZL1H.s1d
HAMMER(ROOT) recovery check seqno=00ef7b31
HAMMER(ROOT) recovery range 30000000027847c8-30000000027847c8
HAMMER(ROOT) recovery nexto 30000000027847c8 endseqno=00ef7b32
HAMMER(ROOT) mounted clean, no recovery needed
DMA space used: 6904k, remaining available: 16384k
Mounting devfs
ACPI Error: No handler for Region [RAM_] (0xffffffe021521438) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BIF] (Node 0xffffffe0096f8858), AE_NOT_EXIST (20140424/psparse-553)
ACPI Error: No handler for Region [RAM_] (0xffffffe021521438) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BIF] (Node 0xffffffe0096f8858), AE_NOT_EXIST (20140424/psparse-553)
ACPI Error: No handler for Region [RAM_] (0xffffffe021521438) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BST] (Node 0xffffffe0096f88a0), AE_NOT_EXIST (20140424/psparse-553)
ACPI Error: No handler for Region [RAM_] (0xffffffe021521438) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BST] (Node 0xffffffe0096f88a0), AE_NOT_EXIST (20140424/psparse-553)
ACPI Error: No handler for Region [RAM_] (0xffffffe021521438) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BST] (Node 0xffffffe0096f88a0), AE_NOT_EXIST (20140424/psparse-553)
ACPI Error: No handler for Region [RAM_] (0xffffffe021521438) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BST] (Node 0xffffffe0096f88a0), AE_NOT_EXIST (20140424/psparse-553)
ACPI Error: No handler for Region [RAM_] (0xffffffe021521438) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BST] (Node 0xffffffe0096f88a0), AE_NOT_EXIST (20140424/psparse-553)
ACPI Error: No handler for Region [RAM_] (0xffffffe021521438) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BST] (Node 0xffffffe0096f88a0), AE_NOT_EXIST (20140424/psparse-553)
ACPI Error: No handler for Region [RAM_] (0xffffffe021521438) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.ADP1._PSR] (Node 0xffffffe0096f8db0), AE_NOT_EXIST (20140424/psparse-553)
ACPI Error: No handler for Region [RAM_] (0xffffffe021521438) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.ADP1._PSR] (Node 0xffffffe0096f8db0), AE_NOT_EXIST (20140424/psparse-553)
ACPI Error: No handler for Region [RAM_] (0xffffffe021521438) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BIF] (Node 0xffffffe0096f8858), AE_NOT_EXIST (20140424/psparse-553)
wlan0: MAC address: 00:1f:3b:c8:0a:87
ACPI Error: No handler for Region [RAM_] (0xffffffe021521438) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BIF] (Node 0xffffffe0096f8858), AE_NOT_EXIST (20140424/psparse-553)
ACPI Error: No handler for Region [RAM_] (0xffffffe021521438) [EmbeddedControl] (20140424/evregion-181)
ACPI Error: Region EmbeddedControl (ID=3) has no handler (20140424/exfldio-323)
ACPI Error: Method parse/execution failed [\\_SB_.PCI0.LPC_.EC0_.BAT0._BIF] (Node 0xffffffe0096f8858), AE_NOT_EXIST (20140424/psparse-553)
