Copyright (c) 2003, 2004, 2005, 2006, 2007 The DragonFly Project.
Copyright (c) 1992-2003 The FreeBSD Project.
Copyright (c) 1979, 1980, 1983, 1986, 1988, 1989, 1991, 1992, 1993, 1994
	The Regents of the University of California. All rights reserved.
DragonFly 1.9.0-DEVELOPMENT #0: Fri Mar  2 07:09:09 EST 2007
    floid@mustelid:/usr/obj/usr/src/sys/MUSTELID_NEWATA
Calibrating clock(s) ... TSC clock: 1995041518 Hz, i8254 clock: 1193207 Hz
CLK_USE_I8254_CALIBRATION not specified - using default frequency
CLK_USE_TSC_CALIBRATION not specified - using old calibration method
CPU: AMD Athlon(tm) 64 X2 Dual Core Processor 3800+ (1995.01-MHz 686-class CPU)
  Origin = "AuthenticAMD"  Id = 0x40fb2  Stepping = 2
  Features=0x178bfbff<FPU,VME,DE,PSE,TSC,MSR,PAE,MCE,CX8,APIC,SEP,MTRR,PGE,MCA,CMOV,PAT,PSE36,CLFLUSH,MMX,FXSR,SSE,SSE2,HTT>
  Features2=0x2001<SSE3,CX16>
  Hyperthreading: 2 logical CPUs
  AMD Features=0xe8500000<<b20>,AMIE,<b27>,<b29>,DSP,3DNow!>
Data TLB: 32 entries, fully associative
Instruction TLB: 32 entries, fully associative
L1 data cache: 64 kbytes, 64 bytes/line, 1 lines/tag, 2-way associative
L1 instruction cache: 64 kbytes, 64 bytes/line, 1 lines/tag, 2-way associative
L2 internal cache: 512 kbytes, 64 bytes/line, 1 lines/tag, 8-way associative
real memory  = 2013069312 (1965888K bytes)
Physical memory chunk(s):
0x00001000 - 0x0009efff, 647168 bytes (158 pages)
0x007c8000 - 0x77fbffff, 2004844544 bytes (489464 pages)
avail memory = 1944715264 (1899136K bytes)
APIC_IO: MP table broken: IRQ 15 not ISA when IRQ 14 is!
Programming 24 pins in IOAPIC #0
IOAPIC #0 intpin 1 -> irq 1
IOAPIC #0 intpin 2 -> irq 0
IOAPIC #0 intpin 4 -> irq 4
IOAPIC #0 intpin 6 -> irq 6
IOAPIC #0 intpin 7 -> irq 7
IOAPIC #0 intpin 8 -> irq 8
IOAPIC #0 intpin 12 -> irq 12
IOAPIC #0 intpin 13 -> irq 13
IOAPIC #0 intpin 14 -> irq 14
IOAPIC #0 intpin 15 -> irq 15
SMP: CPU0 apic_initialize():
     lint0: 0x00000700 lint1: 0x00010400 TPR: 0x00000000 SVR: 0x000001ff
DragonFly/MP: Multiprocessor motherboard
 cpu0 (BSP): apic id:  0, version: 0x80050010, at 0xfee00000
 cpu1 (AP):  apic id:  1, version: 0x80050010, at 0xfee00000
 io0 (APIC): apic id:  2, version: 0x00178021, at 0xfec00000
bios32: Found BIOS32 Service Directory header at 0xc00f0000
bios32: Entry = 0xf0010 (c00f0010)  Rev = 0  Len = 1
pcibios: PCI BIOS entry at 0x31
pnpbios: Found PnP BIOS data at 0xc00f52e0
pnpbios: Entry = f0000:62ba  Rev = 1.0
Other BIOS signatures found:
Preloaded elf kernel "/kernel" at 0xc079b000.
Preloaded elf module "/modules/acpi.ko" at 0xc079b208.
sched_ithd: stray interrupt 7
Leaving critical section, allowing interrupts
crypto: <crypto core>
wlan: <802.11 Link Layer>
Pentium Pro MTRR support enabled
md0: Malloc disk
SMP: CPU0 bsp_apic_configure():
     lint0: 0x00010700 lint1: 0x00000400 TPR: 0x00000000 SVR: 0x000001ff
pci_open(1):	mode 1 addr port (0x0cf8) is 0x80012814
pci_open(1a):	mode1res=0x80000000 (0x80000000)
pci_cfgcheck:	device 0 [class=060000] [hdr=00] is there (id=59501002)
pcibios: BIOS version 3.00
Using $PIR table, 8 entries at 0xc00f5170
PCI-Only Interrupts: none
Location  Bus Device Pin  Link  IRQs
embedded    0   20    A   0x01  3 4 5 7 10 11 12 14 15
embedded    0   20    B   0x02  3 4 5 7 10 11 12 14 15
embedded    0   20    C   0x03  3 4 5 7 10 11 12 14 15
embedded    0   20    D   0x04  3 4 5 7 10 11 12 14 15
embedded    0   18    A   0x0c  3 4 5 7 10 11 12 14 15
embedded    0   19    A   0x04  3 4 5 7 10 11 12 14 15
embedded    0   19    B   0x02  3 4 5 7 10 11 12 14 15
embedded    0   19    C   0x03  3 4 5 7 10 11 12 14 15
embedded    0   19    D   0x03  3 4 5 7 10 11 12 14 15
embedded    1    5    A   0x02  3 4 5 7 10 11 12 14 15
embedded    1    5    B   0x03  3 4 5 7 10 11 12 14 15
embedded    1    5    C   0x04  3 4 5 7 10 11 12 14 15
embedded    1    5    D   0x01  3 4 5 7 10 11 12 14 15
slot 1      2    2    A   0x0c  3 4 5 7 10 11 12 14 15
slot 1      2    2    B   0x0d  3 4 5 7 10 11 12 14 15
slot 1      2    2    C   0x0a  3 4 5 7 10 11 12 14 15
slot 1      2    2    D   0x0b  9
slot 2      2    3    A   0x0b  9
slot 2      2    3    B   0x0c  3 4 5 7 10 11 12 14 15
slot 2      2    3    C   0x0d  3 4 5 7 10 11 12 14 15
slot 2      2    3    D   0x0a  3 4 5 7 10 11 12 14 15
embedded    2    6    A   0x0b  9
embedded    2    0    A   0x0a  3 4 5 7 10 11 12 14 15
ACPI: RSDP @ 0x0xf95e0/0x0014 (v  0 ACPIAM)
ACPI: RSDT @ 0x0x77fd0000/0x003C (v  1 A M I  OEMRSDT  0x01000725 MSFT 0x00000097)
ACPI: FACP @ 0x0x77fd0200/0x0084 (v  2 A M I  OEMFACP  0x01000725 MSFT 0x00000097)
ACPI: DSDT @ 0x0x77fd0430/0x425B (v  1  AMMR_ AMMR_B56 0x00000B56 INTL 0x20051117)
ACPI: FACS @ 0x0x77fde000/0x0040
ACPI: APIC @ 0x0x77fd0390/0x005C (v  1 A M I  OEMAPIC  0x01000725 MSFT 0x00000097)
ACPI: MCFG @ 0x0x77fd03f0/0x003C (v  1 A M I  OEMMCFG  0x01000725 MSFT 0x00000097)
ACPI: OEMB @ 0x0x77fde040/0x0060 (v  1 A M I  AMI_OEM  0x01000725 MSFT 0x00000097)
ACPI: HPET @ 0x0x77fd4690/0x0038 (v  1 A M I  OEMHPET  0x01000725 MSFT 0x00000097)
ACPI: SSDT @ 0x0x77fd46d0/0x01C4 (v  1 A M I  POWERNOW 0x00000001 AMD  0x00000001)
npx0.nexus0.root0
npx0: <math processor> [tentative] on motherboard
npx0: INT 16 interface
Using XMM optimized bcopy/copyin/copyout
npx0: <math processor> [attached!] on motherboard
acpi0.nexus0.root0
acpi0: <A M I OEMRSDT> [tentative] on motherboard
acpi0: Power Button (fixed)
Warning: ACPI is disabling APM's device.  You can't run both
ACPI timer looks GOOD min = 4, max = 6, width = 2
ACPI timer looks GOOD min = 4, max = 5, width = 1
ACPI timer looks GOOD min = 4, max = 5, width = 1
ACPI timer looks GOOD min = 4, max = 5, width = 1
ACPI timer looks GOOD min = 4, max = 5, width = 1
ACPI timer looks GOOD min = 4, max = 5, width = 1
ACPI timer looks BAD  min = 4, max = 7, width = 3
ACPI timer looks GOOD min = 4, max = 5, width = 1
ACPI timer looks GOOD min = 4, max = 5, width = 1
ACPI timer looks GOOD min = 4, max = 5, width = 1
AcpiOsDerivePciId: bus 0 dev 0 func 0
unknown: memory range not supported
unknown: memory range not supported
acpi_timer0.acpi0.nexus0.root0
acpi_timer0: <32-bit timer at 3.579545MHz> [tentative] port 0x808-0x80b on acpi0
acpi_timer0: <32-bit timer at 3.579545MHz> [attached!] port 0x808-0x80b on acpi0
cpu0.acpi0.nexus0.root0
cpu0: <ACPI CPU> [tentative] on acpi0
cpu0: CLK_VAL field overlaps THT_EN bit
cpu0: <ACPI CPU> [attached!] on acpi0
acpi_button0.acpi0.nexus0.root0
acpi_button0: <Power Button> [tentative] on acpi0
acpi_button0: <Power Button> [attached!] on acpi0
unknown: not probed (disabled)
unknown: not probed (disabled)
unknown: not probed (disabled)
unknown: not probed (disabled)
unknown: not probed (disabled)
unknown: not probed (disabled)
unknown: not probed (disabled)
unknown: not probed (disabled)
unknown: not probed (disabled)
unknown: not probed (disabled)
acpi0: <A M I OEMRSDT> [attached!] at irq 9 on motherboard
legacypci0.nexus0.root0
legacypci0 [tentative] on motherboard
pcib0.legacypci0.nexus0.root0
pcib0: <Host to PCI bridge> [tentative] on legacypci0
pci0.pcib0.legacypci0.nexus0.root0
pci0: <PCI bus> [tentative] on pcib0
pci0: pci_attach() physical bus=0
found->	vendor=0x1002, dev=0x5950, revid=0x10
	bus=0, slot=0, func=0
	class=[BRIDGE]06-00-00, hdrtype=0x00, mfdev=0
	subordinatebus=0 	secondarybus=0
found->	vendor=0x1002, dev=0x5a3f, revid=0x00
	bus=0, slot=1, func=0
	class=[BRIDGE]06-04-00, hdrtype=0x01, mfdev=0
	subordinatebus=1 	secondarybus=1
IOAPIC #0 intpin 22 -> irq 2
Freeing (NOT implemented) redirected PCI irq 11.
	map[10]: type 1, range 32, base 0000e800, size  3
	map[14]: type 1, range 32, base 0000e400, size  2
	map[18]: type 1, range 32, base 0000e000, size  3
	map[1c]: type 1, range 32, base 0000dc00, size  2
	map[20]: type 1, range 32, base 0000d800, size  4
	map[24]: type 1, range 32, base ff6ffc00, size 10
found->	vendor=0x1002, dev=0x4380, revid=0x00
	bus=0, slot=18, func=0
	class=[STORAGE]01-01-8f, hdrtype=0x00, mfdev=0
	subordinatebus=0 	secondarybus=0
	intpin=a, irq=2
IOAPIC #0 intpin 16 -> irq 3
Freeing (NOT implemented) redirected PCI irq 10.
	map[10]: type 1, range 32, base ff6fe000, size 12
found->	vendor=0x1002, dev=0x4387, revid=0x00
	bus=0, slot=19, func=0
	class=[SERIALBUS]0c-03-10, hdrtype=0x00, mfdev=1
	subordinatebus=0 	secondarybus=0
	intpin=a, irq=3
IOAPIC #0 intpin 17 -> irq 5
Freeing (NOT implemented) redirected PCI irq 10.
	map[10]: type 1, range 32, base ff6fd000, size 12
found->	vendor=0x1002, dev=0x4388, revid=0x00
	bus=0, slot=19, func=1
	class=[SERIALBUS]0c-03-10, hdrtype=0x00, mfdev=0
	subordinatebus=0 	secondarybus=0
	intpin=b, irq=5
IOAPIC #0 intpin 18 -> irq 9
Freeing (NOT implemented) redirected PCI irq 5.
	map[10]: type 1, range 32, base ff6fc000, size 12
found->	vendor=0x1002, dev=0x4389, revid=0x00
	bus=0, slot=19, func=2
	class=[SERIALBUS]0c-03-10, hdrtype=0x00, mfdev=0
	subordinatebus=0 	secondarybus=0
	intpin=c, irq=9
Freeing (NOT implemented) redirected PCI irq 10.
	map[10]: type 1, range 32, base ff6fb000, size 12
found->	vendor=0x1002, dev=0x438a, revid=0x00
	bus=0, slot=19, func=3
	class=[SERIALBUS]0c-03-10, hdrtype=0x00, mfdev=0
	subordinatebus=0 	secondarybus=0
	intpin=b, irq=5
Freeing (NOT implemented) redirected PCI irq 5.
	map[10]: type 1, range 32, base ff6fa000, size 12
found->	vendor=0x1002, dev=0x438b, revid=0x00
	bus=0, slot=19, func=4
	class=[SERIALBUS]0c-03-10, hdrtype=0x00, mfdev=0
	subordinatebus=0 	secondarybus=0
	intpin=c, irq=9
IOAPIC #0 intpin 19 -> irq 10
Freeing (NOT implemented) redirected PCI irq 5.
	map[10]: type 1, range 32, base ff6ff800, size  8
found->	vendor=0x1002, dev=0x4386, revid=0x00
	bus=0, slot=19, func=5
	class=[SERIALBUS]0c-03-20, hdrtype=0x00, mfdev=0
	subordinatebus=0 	secondarybus=0
	intpin=d, irq=10
	map[10]: type 1, range 32, base 00000b00, size  4
found->	vendor=0x1002, dev=0x4385, revid=0x13
	bus=0, slot=20, func=0
	class=[SERIALBUS]0c-05-00, hdrtype=0x00, mfdev=1
	subordinatebus=0 	secondarybus=0
Freeing (NOT implemented) redirected PCI irq 0.
	map[20]: type 1, range 32, base 0000ff00, size  4
found->	vendor=0x1002, dev=0x438c, revid=0x00
	bus=0, slot=20, func=1
	class=[STORAGE]01-01-8a, hdrtype=0x00, mfdev=0
	subordinatebus=0 	secondarybus=0
	intpin=a, irq=3
Freeing (NOT implemented) redirected PCI irq 15.
	map[10]: type 1, range 64, base ff6f4000, size 14
found->	vendor=0x1002, dev=0x4383, revid=0x00
	bus=0, slot=20, func=2
	class=[MULTIMEDIA]04-03-00, hdrtype=0x00, mfdev=0
	subordinatebus=0 	secondarybus=0
	intpin=a, irq=3
found->	vendor=0x1002, dev=0x438d, revid=0x00
	bus=0, slot=20, func=3
	class=[BRIDGE]06-01-00, hdrtype=0x00, mfdev=1
	subordinatebus=0 	secondarybus=0
found->	vendor=0x1002, dev=0x4384, revid=0x00
	bus=0, slot=20, func=4
	class=[BRIDGE]06-04-01, hdrtype=0x01, mfdev=1
	subordinatebus=2 	secondarybus=2
found->	vendor=0x1022, dev=0x1100, revid=0x00
	bus=0, slot=24, func=0
	class=[BRIDGE]06-00-00, hdrtype=0x00, mfdev=1
	subordinatebus=0 	secondarybus=0
found->	vendor=0x1022, dev=0x1101, revid=0x00
	bus=0, slot=24, func=1
	class=[BRIDGE]06-00-00, hdrtype=0x00, mfdev=1
	subordinatebus=0 	secondarybus=0
found->	vendor=0x1022, dev=0x1102, revid=0x00
	bus=0, slot=24, func=2
	class=[BRIDGE]06-00-00, hdrtype=0x00, mfdev=1
	subordinatebus=0 	secondarybus=0
found->	vendor=0x1022, dev=0x1103, revid=0x00
	bus=0, slot=24, func=3
	class=[BRIDGE]06-00-00, hdrtype=0x00, mfdev=1
	subordinatebus=0 	secondarybus=0
pcib1.pci0.pcib0.legacypci0.nexus0.root0
pcib1: <PCI to PCI bridge (vendor=1002 device=5a3f)> [tentative] at device 1.0 on pci0
pcib1:   secondary bus     1
pcib1:   subordinate bus   1
pcib1:   I/O decode        0xa000-0xafff
pcib1:   memory decode     0xff400000-0xff4fffff
pcib1:   prefetched decode 0xcff00000-0xdfefffff
pci1.pcib1.pci0.pcib0.legacypci0.nexus0.root0
pci1: <PCI bus> [tentative] on pcib1
pci1: pci_attach() physical bus=1
Freeing (NOT implemented) redirected PCI irq 10.
	map[10]: type 1, range 32, base d0000000, size 27
	map[14]: type 1, range 32, base 0000a800, size  8
	map[18]: type 1, range 32, base ff4f0000, size 16
found->	vendor=0x1002, dev=0x5974, revid=0x00
	bus=1, slot=5, func=0
	class=[DISPLAY]03-00-00, hdrtype=0x00, mfdev=0
	subordinatebus=0 	secondarybus=0
	intpin=a, irq=5
pci1: <ATI model 5974 graphics accelerator> (vendor=0x1002, dev=0x5974) at 5.0 irq 5
pci1: <PCI bus> [attached!] on pcib1
pcib1: <PCI to PCI bridge (vendor=1002 device=5a3f)> [attached!] at device 1.0 on pci0
atapci0.pci0.pcib0.legacypci0.nexus0.root0
atapci0: <ATI SB600 SATA300 controller> [tentative] port 0xd800-0xd80f,0xdc00-0xdc03,0xe000-0xe007,0xe400-0xe403,0xe800-0xe807 mem 0xff6ffc00-0xff6fffff irq 2 at device 18.0 on pci0
ata2.atapci0.pci0.pcib0.legacypci0.nexus0.root0
ata2: <ATA channel 0> [tentative] on atapci0
ata2: SATA connect status=00000000
ata2: <ATA channel 0> [attached!] on atapci0
ata3.atapci0.pci0.pcib0.legacypci0.nexus0.root0
ata3: <ATA channel 1> [tentative] on atapci0
ata3: SATA connect status=00000000
ata3: <ATA channel 1> [attached!] on atapci0
atapci0: <ATI SB600 SATA300 controller> [attached!] port 0xd800-0xd80f,0xdc00-0xdc03,0xe000-0xe007,0xe400-0xe403,0xe800-0xe807 mem 0xff6ffc00-0xff6fffff irq 2 at device 18.0 on pci0
ohci0.pci0.pcib0.legacypci0.nexus0.root0
ohci0: <OHCI (generic) USB controller> [tentative] mem 0xff6fe000-0xff6fefff irq 3 at device 19.0 on pci0
usb0: OHCI version 1.0, legacy support
usb0.ohci0.pci0.pcib0.legacypci0.nexus0.root0
usb0: <OHCI (generic) USB controller> [tentative] on ohci0
usb0: USB revision 1.0
uhub0: 2 ports with 2 removable, self powered
intr 3 at 50001 > 50000 hz, livelocked limit engaged!
ums0: Microsoft Microsoft 3-Button Mouse with IntelliEye(TM), rev 1.10/3.00, addr 2, iclass 3/1
ums0: 3 buttons and Z dir.
usb0: <OHCI (generic) USB controller> [attached!] on ohci0
ohci0: <OHCI (generic) USB controller> [attached!] mem 0xff6fe000-0xff6fefff irq 3 at device 19.0 on pci0
ohci1.pci0.pcib0.legacypci0.nexus0.root0
ohci1: <OHCI (generic) USB controller> [tentative] mem 0xff6fd000-0xff6fdfff irq 5 at device 19.1 on pci0
usb1: OHCI version 1.0, legacy support
usb1.ohci1.pci0.pcib0.legacypci0.nexus0.root0
usb1: <OHCI (generic) USB controller> [tentative] on ohci1
usb1: USB revision 1.0
uhub1: 2 ports with 2 removable, self powered
usb1: <OHCI (generic) USB controller> [attached!] on ohci1
ohci1: <OHCI (generic) USB controller> [attached!] mem 0xff6fd000-0xff6fdfff irq 5 at device 19.1 on pci0
ohci2.pci0.pcib0.legacypci0.nexus0.root0
ohci2: <OHCI (generic) USB controller> [tentative] mem 0xff6fc000-0xff6fcfff irq 9 at device 19.2 on pci0
usb2: OHCI version 1.0, legacy support
usb2.ohci2.pci0.pcib0.legacypci0.nexus0.root0
usb2: <OHCI (generic) USB controller> [tentative] on ohci2
usb2: USB revision 1.0
uhub2: 2 ports with 2 removable, self powered
usb2: <OHCI (generic) USB controller> [attached!] on ohci2
ohci2: <OHCI (generic) USB controller> [attached!] mem 0xff6fc000-0xff6fcfff irq 9 at device 19.2 on pci0
ohci3.pci0.pcib0.legacypci0.nexus0.root0
ohci3: <OHCI (generic) USB controller> [tentative] mem 0xff6fb000-0xff6fbfff irq 5 at device 19.3 on pci0
usb3: OHCI version 1.0, legacy support
usb3.ohci3.pci0.pcib0.legacypci0.nexus0.root0
usb3: <OHCI (generic) USB controller> [tentative] on ohci3
usb3: USB revision 1.0
uhub3: 2 ports with 2 removable, self powered
usb3: <OHCI (generic) USB controller> [attached!] on ohci3
ohci3: <OHCI (generic) USB controller> [attached!] mem 0xff6fb000-0xff6fbfff irq 5 at device 19.3 on pci0
ohci4.pci0.pcib0.legacypci0.nexus0.root0
ohci4: <OHCI (generic) USB controller> [tentative] mem 0xff6fa000-0xff6fafff irq 9 at device 19.4 on pci0
usb4: OHCI version 1.0, legacy support
usb4.ohci4.pci0.pcib0.legacypci0.nexus0.root0
usb4: <OHCI (generic) USB controller> [tentative] on ohci4
usb4: USB revision 1.0
uhub4: 2 ports with 2 removable, self powered
usb4: <OHCI (generic) USB controller> [attached!] on ohci4
ohci4: <OHCI (generic) USB controller> [attached!] mem 0xff6fa000-0xff6fafff irq 9 at device 19.4 on pci0
pci0: <USB controller> (vendor=0x1002, dev=0x4386) at 19.5 irq 10
pci0: <unknown card> (vendor=0x1002, dev=0x4385) at 20.0
atapci1.pci0.pcib0.legacypci0.nexus0.root0
atapci1: <ATI SB600 UDMA133 controller> [tentative] port 0xff00-0xff0f,0x376,0x170-0x177,0x3f6,0x1f0-0x1f7 irq 3 at device 20.1 on pci0
ata0.atapci1.pci0.pcib0.legacypci0.nexus0.root0
ata0: <ATA channel 0> [tentative] on atapci1
atapci1: reserved 0x8 bytes for rid 0x10 type 4 at 0x1f0
atapci1: reserved 0x1 bytes for rid 0x14 type 4 at 0x3f6
ata0: reset tp1 mask=03 ostat0=50 ostat1=00
ata0: stat0=0x50 err=0x01 lsb=0x00 msb=0x00
ata0: stat1=0x00 err=0x01 lsb=0x00 msb=0x00
ata0: reset tp2 stat0=50 stat1=00 devices=0x1<ATA_MASTER>
ata0: <ATA channel 0> [attached!] on atapci1
ata1.atapci1.pci0.pcib0.legacypci0.nexus0.root0
ata1: <ATA channel 1> [tentative] on atapci1
atapci1: reserved 0x8 bytes for rid 0x18 type 4 at 0x170
atapci1: reserved 0x1 bytes for rid 0x1c type 4 at 0x376
ata1: reset tp1 mask=00 ostat0=ff ostat1=ff
ata1: <ATA channel 1> [attached!] on atapci1
atapci1: <ATI SB600 UDMA133 controller> [attached!] port 0xff00-0xff0f,0x376,0x170-0x177,0x3f6,0x1f0-0x1f7 irq 3 at device 20.1 on pci0
pci0: <unknown card> (vendor=0x1002, dev=0x4383) at 20.2 irq 3
isab0.pci0.pcib0.legacypci0.nexus0.root0
isab0: <PCI to ISA bridge (vendor=1002 device=438d)> [tentative] at device 20.3 on pci0
isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
isa0: <ISA bus> [tentative] on isab0
isa0: <ISA bus> [attached!] on isab0
isab0: <PCI to ISA bridge (vendor=1002 device=438d)> [attached!] at device 20.3 on pci0
pcib2.pci0.pcib0.legacypci0.nexus0.root0
pcib2: <PCI to PCI bridge (vendor=1002 device=4384)> [tentative] at device 20.4 on pci0
pcib2:   secondary bus     2
pcib2:   subordinate bus   2
pcib2:   I/O decode        0xb000-0xbfff
pcib2:   memory decode     0xff500000-0xff5fffff
pcib2:   prefetched decode 0xfff00000-0xfffff
pcib2:   Subtractively decoded bridge.
pci2.pcib2.pci0.pcib0.legacypci0.nexus0.root0
pci2: <PCI bus> [tentative] on pcib2
pci2: pci_attach() physical bus=2
IOAPIC #0 intpin 21 -> irq 11
Freeing (NOT implemented) redirected PCI irq 9.
	map[10]: type 1, range 32, base 0000b800, size  8
	map[14]: type 1, range 32, base ff5ff400, size  8
found->	vendor=0x10ec, dev=0x8167, revid=0x10
	bus=2, slot=6, func=0
	class=[NETWORK]02-00-00, hdrtype=0x00, mfdev=0
	subordinatebus=0 	secondarybus=0
	intpin=a, irq=11
pcib2: device re0 requested decoded I/O range 0xb800-0xb8ff
re0.pci2.pcib2.pci0.pcib0.legacypci0.nexus0.root0
re0: <RealTek 8169SC/8110SC Single-chip Gigabit Ethernet> [tentative] port 0xb800-0xb8ff mem 0xff5ff400-0xff5ff4ff irq 11 at device 6.0 on pci2
pcib2: device re0 requested decoded I/O range 0xb800-0xb8ff
miibus0.re0.pci2.pcib2.pci0.pcib0.legacypci0.nexus0.root0
miibus0: <MII bus> [tentative] on re0
rgephy0: rev: 2
rgephy0.miibus0.re0.pci2.pcib2.pci0.pcib0.legacypci0.nexus0.root0
rgephy0: <RTL8169S/8110S media interface> [tentative] on miibus0
rgephy0:  10baseT, 10baseT-FDX, 100baseTX, 100baseTX-FDX, 1000baseT, 1000baseT-FDX, auto
rgephy0: <RTL8169S/8110S media interface> [attached!] on miibus0
miibus0: <MII bus> [attached!] on re0
re0: bpf attached
re0: MAC address: 00:19:db:2a:83:04
re0: <RealTek 8169SC/8110SC Single-chip Gigabit Ethernet> [attached!] port 0xb800-0xb8ff mem 0xff5ff400-0xff5ff4ff irq 11 at device 6.0 on pci2
pci2: <PCI bus> [attached!] on pcib2
pcib2: <PCI to PCI bridge (vendor=1002 device=4384)> [attached!] at device 20.4 on pci0
pci0: <PCI bus> [attached!] on pcib0
pcib0: <Host to PCI bridge> [attached!] on legacypci0
legacypci0 [attached!] on motherboard
ex_isa_identify()
Trying Read_Port at 203
Trying Read_Port at 243
Trying Read_Port at 283
Trying Read_Port at 2c3
Trying Read_Port at 303
Trying Read_Port at 343
Trying Read_Port at 383
Trying Read_Port at 3c3
isa_probe_children: disabling PnP devices
isa_probe_children: probing non-PnP devices
orm0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
orm0: <Option ROM> [tentative] at iomem 0xc0000-0xcefff on isa0
orm0: <Option ROM> [attached!] at iomem 0xc0000-0xcefff on isa0
pmtimer0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
pmtimer0 [tentative] on isa0
pmtimer0 [attached!] on isa0
fdc0: ready for input in output
fdc0: cmd 3 failed at out byte 1 of 3
fdc0 [tentative] failed to probe at port 0x3f0-0x3f5,0x3f7 irq 6 drq 2 on isa0
adv0 [tentative] failed to probe on isa0
bt0: Failed Status Reg Test - ff
bt_isa_probe: Probe failed at 0x330
bt0: Failed Status Reg Test - ff
bt_isa_probe: Probe failed at 0x334
bt0: Failed Status Reg Test - ff
bt_isa_probe: Probe failed at 0x230
bt0: Failed Status Reg Test - ff
bt_isa_probe: Probe failed at 0x234
bt0: Failed Status Reg Test - ff
bt_isa_probe: Probe failed at 0x130
bt0: Failed Status Reg Test - ff
bt_isa_probe: Probe failed at 0x134
bt0 [tentative] failed to probe at port 0x134-0x137 on isa0
aha0: status reg test failed ff
aha0: status reg test failed ff
aha0: status reg test failed ff
aha0: status reg test failed ff
aha0: status reg test failed ff
aha0: status reg test failed ff
aha0 [tentative] failed to probe at port 0x134-0x137 on isa0
aic0 [tentative] failed to probe at port 0x140-0x15f on isa0
atkbdc0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
atkbdc0: <Keyboard controller (i8042)> [tentative] at port 0x60,0x64 on isa0
atkbd0.atkbdc0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
atkbd0: <AT Keyboard> [tentative] flags 0x1 irq 1 on atkbdc0
atkbd: the current kbd controller command byte 0065
atkbd: keyboard ID 0x41ab (2)
kbd0 at atkbd0
kbd0: atkbd0, AT 101/102 (2), config:0x1, flags:0x3d0000
atkbd0: <AT Keyboard> [attached!] flags 0x1 irq 1 on atkbdc0
psm0: current command byte:0065
psm0: failed to reset the aux device.
atkbdc0: <Keyboard controller (i8042)> [attached!] at port 0x60,0x64 on isa0
vga0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
vga0: <Generic ISA VGA> [tentative] at port 0x3c0-0x3df iomem 0xa0000-0xbffff on isa0
fb0: vga0, vga, type:VGA (5), flags:0x7007f
fb0: port:0x3c0-0x3df, crtc:0x3d4, mem:0xa0000 0x20000
fb0: init mode:24, bios mode:3, current mode:24
fb0: window:0xc00b8000 size:32k gran:32k, buf:0 size:32k
VGA parameters upon power-up
50 18 10 00 00 00 03 00 02 67 5f 4f 50 82 55 81 
bf 1f 00 4f 0d 0e 00 00 07 80 9c 8e 8f 28 1f 96 
b9 a3 ff 00 01 02 03 04 05 14 07 38 39 3a 3b 3c 
3d 3e 3f 0c 00 0f 08 00 00 00 00 00 10 0e 00 ff 
VGA parameters in BIOS for mode 24
50 18 10 00 10 00 03 00 02 67 5f 4f 50 82 55 81 
bf 1f 00 4f 0d 0e 00 00 00 00 9c 8e 8f 28 1f 96 
b9 a3 ff 00 01 02 03 04 05 14 07 38 39 3a 3b 3c 
3d 3e 3f 0c 00 0f 08 00 00 00 00 00 10 0e 00 ff 
EGA/VGA parameters to be used for mode 24
50 18 10 00 10 00 03 00 02 67 5f 4f 50 82 55 81 
bf 1f 00 4f 0d 0e 00 00 00 00 9c 8e 8f 28 1f 96 
b9 a3 ff 00 01 02 03 04 05 14 07 38 39 3a 3b 3c 
3d 3e 3f 0c 00 0f 08 00 00 00 00 00 10 0e 00 ff 
vga0: <Generic ISA VGA> [attached!] at port 0x3c0-0x3df iomem 0xa0000-0xbffff on isa0
sc0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
sc0: <System console> [tentative] at flags 0x100 on isa0
sc0: VGA <16 virtual consoles, flags=0x300>
sc0: fb0, kbd0, terminal emulator: sc (syscons terminal)
sc0: <System console> [attached!] at flags 0x100 on isa0
sio0: irq maps: 0x3 0x13 0x3 0x3
sio0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
sio0 [tentative] at port 0x3f8-0x3ff irq 4 flags 0x10 on isa0
sio0: type 16550A
sio0 [attached!] at port 0x3f8-0x3ff irq 4 flags 0x10 on isa0
sio1: can't drain, serial port might not exist, disabling
sio1 [tentative] failed to probe at port 0x2f8-0x2ff irq 3 on isa0
sio2: not probed (disabled)
sio3: not probed (disabled)
ppc0: parallel port found at 0x378
ppc0: using extended I/O port range
ppc0: SPP
ppc0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
ppc0: <Parallel port> [tentative] at port 0x378-0x37f irq 7 on isa0
ppc0: Generic chipset (NIBBLE-only) in COMPATIBLE mode
ppbus0.ppc0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
ppbus0: <Parallel port bus> [tentative] on ppc0
plip0.ppbus0.ppc0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
plip0: <PLIP network interface> [tentative] on ppbus0
lp0: bpf attached
plip0: <PLIP network interface> [attached!] on ppbus0
lpt0.ppbus0.ppc0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
lpt0: <Printer> [tentative] on ppbus0
lpt0: Interrupt-driven port
lpt0: <Printer> [attached!] on ppbus0
ppi0.ppbus0.ppc0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
ppi0: <Parallel I/O> [tentative] on ppbus0
ppi0: <Parallel I/O> [attached!] on ppbus0
ppbus0: <Parallel port bus> [attached!] on ppc0
ppc0: <Parallel port> [attached!] at port 0x378-0x37f irq 7 on isa0
ed0: not probed (disabled)
fe0: not probed (disabled)
ie0: not probed (disabled)
lnc0: not probed (disabled)
cs0: not probed (disabled)
sn0: not probed (disabled)
isa_probe_children: probing PnP devices
SMP: enabled INTs: 1, 2, 4, 5, 7, 9, 11, 14, 15, apic_imen: 0x00ff3549
BIOS Geometries:
 0:03ff0f3f 0..1023=1024 cylinders, 0..15=16 heads, 1..63=63 sectors
 0 accounted for
Device configuration finished.
APIC_IO: Testing 8254 interrupt delivery
APIC_IO: routing 8254 via IOAPIC #0 intpin 2
Finish MP startup
SMP: AP CPU #1 Launched!
SMP: CPU1 apic_initialize():
     lint0: 0x00010000 lint1: 0x00010400 TPR: 0x00000000 SVR: 0x000001ff
Copyright (c) 2003, 2004, 2005, 2006, 2007 The DragonFly Project.
Copyright (c) 1992-2003 The FreeBSD Project.
Copyright (c) 1979, 1980, 1983, 1986, 1988, 1989, 1991, 1992, 1993, 1994
	The Regents of the University of California. All rights reserved.
DragonFly 1.9.0-DEVELOPMENT #2: Sun Feb 25 22:15:47 EST 2007
    root@mustelid:/usr/obj/usr/src/sys/MUSTELID_OLDATA
Calibrating clock(s) ... TSC clock: 1995051322 Hz, i8254 clock: 1193212 Hz
CLK_USE_I8254_CALIBRATION not specified - using default frequency
CLK_USE_TSC_CALIBRATION not specified - using old calibration method
CPU: AMD Athlon(tm) 64 X2 Dual Core Processor 3800+ (1995.01-MHz 686-class CPU)
  Origin = "AuthenticAMD"  Id = 0x40fb2  Stepping = 2
  Features=0x178bfbff<FPU,VME,DE,PSE,TSC,MSR,PAE,MCE,CX8,APIC,SEP,MTRR,PGE,MCA,CMOV,PAT,PSE36,CLFLUSH,MMX,FXSR,SSE,SSE2,HTT>
  Features2=0x2001<SSE3,CX16>
  Hyperthreading: 2 logical CPUs
  AMD Features=0xe8500000<<b20>,AMIE,<b27>,<b29>,DSP,3DNow!>
Data TLB: 32 entries, fully associative
Instruction TLB: 32 entries, fully associative
L1 data cache: 64 kbytes, 64 bytes/line, 1 lines/tag, 2-way associative
L1 instruction cache: 64 kbytes, 64 bytes/line, 1 lines/tag, 2-way associative
L2 internal cache: 512 kbytes, 64 bytes/line, 1 lines/tag, 8-way associative
real memory  = 2013069312 (1965888K bytes)
Physical memory chunk(s):
0x00001000 - 0x0009efff, 647168 bytes (158 pages)
0x007b7000 - 0x77fbffff, 2004914176 bytes (489481 pages)
avail memory = 1944686592 (1899108K bytes)
APIC_IO: MP table broken: IRQ 15 not ISA when IRQ 14 is!
Programming 24 pins in IOAPIC #0
IOAPIC #0 intpin 1 -> irq 1
IOAPIC #0 intpin 2 -> irq 0
IOAPIC #0 intpin 4 -> irq 4
IOAPIC #0 intpin 6 -> irq 6
IOAPIC #0 intpin 7 -> irq 7
IOAPIC #0 intpin 8 -> irq 8
IOAPIC #0 intpin 12 -> irq 12
IOAPIC #0 intpin 13 -> irq 13
IOAPIC #0 intpin 14 -> irq 14
IOAPIC #0 intpin 15 -> irq 15
SMP: CPU0 apic_initialize():
     lint0: 0x00000700 lint1: 0x00010400 TPR: 0x00000000 SVR: 0x000001ff
DragonFly/MP: Multiprocessor motherboard
 cpu0 (BSP): apic id:  0, version: 0x80050010, at 0xfee00000
 cpu1 (AP):  apic id:  1, version: 0x80050010, at 0xfee00000
 io0 (APIC): apic id:  2, version: 0x00178021, at 0xfec00000
bios32: Found BIOS32 Service Directory header at 0xc00f0000
bios32: Entry = 0xf0010 (c00f0010)  Rev = 0  Len = 1
pcibios: PCI BIOS entry at 0x31
pnpbios: Found PnP BIOS data at 0xc00f52e0
pnpbios: Entry = f0000:62ba  Rev = 1.0
Other BIOS signatures found:
Preloaded elf kernel "/kernel.1.9.oldata" at 0xc078a000.
Preloaded elf module "/modules/acpi.ko" at 0xc078a200.
sched_ithd: stray interrupt 7
Leaving critical section, allowing interrupts
crypto: <crypto core>
wlan: <802.11 Link Layer>
Pentium Pro MTRR support enabled
md0: Malloc disk
SMP: CPU0 bsp_apic_configure():
     lint0: 0x00010700 lint1: 0x00000400 TPR: 0x00000000 SVR: 0x000001ff
pci_open(1):	mode 1 addr port (0x0cf8) is 0x80012814
pci_open(1a):	mode1res=0x80000000 (0x80000000)
pci_cfgcheck:	device 0 [class=060000] [hdr=00] is there (id=59501002)
pcibios: BIOS version 3.00
Using $PIR table, 8 entries at 0xc00f5170
PCI-Only Interrupts: none
Location  Bus Device Pin  Link  IRQs
embedded    0   20    A   0x01  3 4 5 7 10 11 12 14 15
embedded    0   20    B   0x02  3 4 5 7 10 11 12 14 15
embedded    0   20    C   0x03  3 4 5 7 10 11 12 14 15
embedded    0   20    D   0x04  3 4 5 7 10 11 12 14 15
embedded    0   18    A   0x0c  3 4 5 7 10 11 12 14 15
embedded    0   19    A   0x04  3 4 5 7 10 11 12 14 15
embedded    0   19    B   0x02  3 4 5 7 10 11 12 14 15
embedded    0   19    C   0x03  3 4 5 7 10 11 12 14 15
embedded    0   19    D   0x03  3 4 5 7 10 11 12 14 15
embedded    1    5    A   0x02  3 4 5 7 10 11 12 14 15
embedded    1    5    B   0x03  3 4 5 7 10 11 12 14 15
embedded    1    5    C   0x04  3 4 5 7 10 11 12 14 15
embedded    1    5    D   0x01  3 4 5 7 10 11 12 14 15
slot 1      2    2    A   0x0c  3 4 5 7 10 11 12 14 15
slot 1      2    2    B   0x0d  3 4 5 7 10 11 12 14 15
slot 1      2    2    C   0x0a  3 4 5 7 10 11 12 14 15
slot 1      2    2    D   0x0b  9
slot 2      2    3    A   0x0b  9
slot 2      2    3    B   0x0c  3 4 5 7 10 11 12 14 15
slot 2      2    3    C   0x0d  3 4 5 7 10 11 12 14 15
slot 2      2    3    D   0x0a  3 4 5 7 10 11 12 14 15
embedded    2    6    A   0x0b  9
embedded    2    0    A   0x0a  3 4 5 7 10 11 12 14 15
ACPI: RSDP @ 0x0xf95e0/0x0014 (v  0 ACPIAM)
ACPI: RSDT @ 0x0x77fd0000/0x003C (v  1 A M I  OEMRSDT  0x01000725 MSFT 0x00000097)
ACPI: FACP @ 0x0x77fd0200/0x0084 (v  2 A M I  OEMFACP  0x01000725 MSFT 0x00000097)
ACPI: DSDT @ 0x0x77fd0430/0x425B (v  1  AMMR_ AMMR_B56 0x00000B56 INTL 0x20051117)
ACPI: FACS @ 0x0x77fde000/0x0040
ACPI: APIC @ 0x0x77fd0390/0x005C (v  1 A M I  OEMAPIC  0x01000725 MSFT 0x00000097)
ACPI: MCFG @ 0x0x77fd03f0/0x003C (v  1 A M I  OEMMCFG  0x01000725 MSFT 0x00000097)
ACPI: OEMB @ 0x0x77fde040/0x0060 (v  1 A M I  AMI_OEM  0x01000725 MSFT 0x00000097)
ACPI: HPET @ 0x0x77fd4690/0x0038 (v  1 A M I  OEMHPET  0x01000725 MSFT 0x00000097)
ACPI: SSDT @ 0x0x77fd46d0/0x01C4 (v  1 A M I  POWERNOW 0x00000001 AMD  0x00000001)
npx0.nexus0.root0
npx0: <math processor> [tentative] on motherboard
npx0: INT 16 interface
Using XMM optimized bcopy/copyin/copyout
npx0: <math processor> [attached!] on motherboard
acpi0.nexus0.root0
acpi0: <A M I OEMRSDT> [tentative] on motherboard
acpi0: Power Button (fixed)
Warning: ACPI is disabling APM's device.  You can't run both
ACPI timer looks GOOD min = 4, max = 5, width = 1
ACPI timer looks GOOD min = 4, max = 5, width = 1
ACPI timer looks GOOD min = 4, max = 5, width = 1
ACPI timer looks GOOD min = 4, max = 5, width = 1
ACPI timer looks GOOD min = 4, max = 5, width = 1
ACPI timer looks GOOD min = 4, max = 5, width = 1
ACPI timer looks GOOD min = 4, max = 5, width = 1
ACPI timer looks GOOD min = 4, max = 5, width = 1
ACPI timer looks GOOD min = 4, max = 5, width = 1
ACPI timer looks GOOD min = 4, max = 5, width = 1
AcpiOsDerivePciId: bus 0 dev 0 func 0
unknown: memory range not supported
unknown: memory range not supported
acpi_timer0.acpi0.nexus0.root0
acpi_timer0: <32-bit timer at 3.579545MHz> [tentative] port 0x808-0x80b on acpi0
acpi_timer0: <32-bit timer at 3.579545MHz> [attached!] port 0x808-0x80b on acpi0
cpu0.acpi0.nexus0.root0
cpu0: <ACPI CPU> [tentative] on acpi0
cpu0: CLK_VAL field overlaps THT_EN bit
cpu0: <ACPI CPU> [attached!] on acpi0
acpi_button0.acpi0.nexus0.root0
acpi_button0: <Power Button> [tentative] on acpi0
acpi_button0: <Power Button> [attached!] on acpi0
unknown: not probed (disabled)
unknown: not probed (disabled)
unknown: not probed (disabled)
unknown: not probed (disabled)
unknown: not probed (disabled)
unknown: not probed (disabled)
unknown: not probed (disabled)
unknown: not probed (disabled)
unknown: not probed (disabled)
unknown: not probed (disabled)
acpi0: <A M I OEMRSDT> [attached!] at irq 9 on motherboard
legacypci0.nexus0.root0
legacypci0 [tentative] on motherboard
pcib0.legacypci0.nexus0.root0
pcib0: <Host to PCI bridge> [tentative] on legacypci0
pci0.pcib0.legacypci0.nexus0.root0
pci0: <PCI bus> [tentative] on pcib0
pci0: pci_attach() physical bus=0
found->	vendor=0x1002, dev=0x5950, revid=0x10
	bus=0, slot=0, func=0
	class=[BRIDGE]06-00-00, hdrtype=0x00, mfdev=0
	subordinatebus=0 	secondarybus=0
found->	vendor=0x1002, dev=0x5a3f, revid=0x00
	bus=0, slot=1, func=0
	class=[BRIDGE]06-04-00, hdrtype=0x01, mfdev=0
	subordinatebus=1 	secondarybus=1
IOAPIC #0 intpin 22 -> irq 2
Freeing (NOT implemented) redirected PCI irq 11.
	map[10]: type 1, range 32, base 0000e800, size  3
	map[14]: type 1, range 32, base 0000e400, size  2
	map[18]: type 1, range 32, base 0000e000, size  3
	map[1c]: type 1, range 32, base 0000dc00, size  2
	map[20]: type 1, range 32, base 0000d800, size  4
	map[24]: type 1, range 32, base ff6ffc00, size 10
found->	vendor=0x1002, dev=0x4380, revid=0x00
	bus=0, slot=18, func=0
	class=[STORAGE]01-01-8f, hdrtype=0x00, mfdev=0
	subordinatebus=0 	secondarybus=0
	intpin=a, irq=2
IOAPIC #0 intpin 16 -> irq 3
Freeing (NOT implemented) redirected PCI irq 10.
	map[10]: type 1, range 32, base ff6fe000, size 12
found->	vendor=0x1002, dev=0x4387, revid=0x00
	bus=0, slot=19, func=0
	class=[SERIALBUS]0c-03-10, hdrtype=0x00, mfdev=1
	subordinatebus=0 	secondarybus=0
	intpin=a, irq=3
IOAPIC #0 intpin 17 -> irq 5
Freeing (NOT implemented) redirected PCI irq 10.
	map[10]: type 1, range 32, base ff6fd000, size 12
found->	vendor=0x1002, dev=0x4388, revid=0x00
	bus=0, slot=19, func=1
	class=[SERIALBUS]0c-03-10, hdrtype=0x00, mfdev=0
	subordinatebus=0 	secondarybus=0
	intpin=b, irq=5
IOAPIC #0 intpin 18 -> irq 9
Freeing (NOT implemented) redirected PCI irq 5.
	map[10]: type 1, range 32, base ff6fc000, size 12
found->	vendor=0x1002, dev=0x4389, revid=0x00
	bus=0, slot=19, func=2
	class=[SERIALBUS]0c-03-10, hdrtype=0x00, mfdev=0
	subordinatebus=0 	secondarybus=0
	intpin=c, irq=9
Freeing (NOT implemented) redirected PCI irq 10.
	map[10]: type 1, range 32, base ff6fb000, size 12
found->	vendor=0x1002, dev=0x438a, revid=0x00
	bus=0, slot=19, func=3
	class=[SERIALBUS]0c-03-10, hdrtype=0x00, mfdev=0
	subordinatebus=0 	secondarybus=0
	intpin=b, irq=5
Freeing (NOT implemented) redirected PCI irq 5.
	map[10]: type 1, range 32, base ff6fa000, size 12
found->	vendor=0x1002, dev=0x438b, revid=0x00
	bus=0, slot=19, func=4
	class=[SERIALBUS]0c-03-10, hdrtype=0x00, mfdev=0
	subordinatebus=0 	secondarybus=0
	intpin=c, irq=9
IOAPIC #0 intpin 19 -> irq 10
Freeing (NOT implemented) redirected PCI irq 5.
	map[10]: type 1, range 32, base ff6ff800, size  8
found->	vendor=0x1002, dev=0x4386, revid=0x00
	bus=0, slot=19, func=5
	class=[SERIALBUS]0c-03-20, hdrtype=0x00, mfdev=0
	subordinatebus=0 	secondarybus=0
	intpin=d, irq=10
	map[10]: type 1, range 32, base 00000b00, size  4
found->	vendor=0x1002, dev=0x4385, revid=0x13
	bus=0, slot=20, func=0
	class=[SERIALBUS]0c-05-00, hdrtype=0x00, mfdev=1
	subordinatebus=0 	secondarybus=0
Freeing (NOT implemented) redirected PCI irq 0.
	map[10]: type 1, range 32, base 00000000, size  3
	map[14]: type 1, range 32, base 00000000, size  2
	map[18]: type 1, range 32, base 00000000, size  3
	map[1c]: type 1, range 32, base 00000000, size  2
	map[20]: type 1, range 32, base 0000ff00, size  4
found->	vendor=0x1002, dev=0x438c, revid=0x00
	bus=0, slot=20, func=1
	class=[STORAGE]01-01-8a, hdrtype=0x00, mfdev=0
	subordinatebus=0 	secondarybus=0
	intpin=a, irq=3
Freeing (NOT implemented) redirected PCI irq 15.
	map[10]: type 1, range 64, base ff6f4000, size 14
found->	vendor=0x1002, dev=0x4383, revid=0x00
	bus=0, slot=20, func=2
	class=[MULTIMEDIA]04-03-00, hdrtype=0x00, mfdev=0
	subordinatebus=0 	secondarybus=0
	intpin=a, irq=3
found->	vendor=0x1002, dev=0x438d, revid=0x00
	bus=0, slot=20, func=3
	class=[BRIDGE]06-01-00, hdrtype=0x00, mfdev=1
	subordinatebus=0 	secondarybus=0
found->	vendor=0x1002, dev=0x4384, revid=0x00
	bus=0, slot=20, func=4
	class=[BRIDGE]06-04-01, hdrtype=0x01, mfdev=1
	subordinatebus=2 	secondarybus=2
found->	vendor=0x1022, dev=0x1100, revid=0x00
	bus=0, slot=24, func=0
	class=[BRIDGE]06-00-00, hdrtype=0x00, mfdev=1
	subordinatebus=0 	secondarybus=0
found->	vendor=0x1022, dev=0x1101, revid=0x00
	bus=0, slot=24, func=1
	class=[BRIDGE]06-00-00, hdrtype=0x00, mfdev=1
	subordinatebus=0 	secondarybus=0
found->	vendor=0x1022, dev=0x1102, revid=0x00
	bus=0, slot=24, func=2
	class=[BRIDGE]06-00-00, hdrtype=0x00, mfdev=1
	subordinatebus=0 	secondarybus=0
found->	vendor=0x1022, dev=0x1103, revid=0x00
	bus=0, slot=24, func=3
	class=[BRIDGE]06-00-00, hdrtype=0x00, mfdev=1
	subordinatebus=0 	secondarybus=0
pcib1.pci0.pcib0.legacypci0.nexus0.root0
pcib1: <PCI to PCI bridge (vendor=1002 device=5a3f)> [tentative] at device 1.0 on pci0
pcib1:   secondary bus     1
pcib1:   subordinate bus   1
pcib1:   I/O decode        0xa000-0xafff
pcib1:   memory decode     0xff400000-0xff4fffff
pcib1:   prefetched decode 0xcff00000-0xdfefffff
pci1.pcib1.pci0.pcib0.legacypci0.nexus0.root0
pci1: <PCI bus> [tentative] on pcib1
pci1: pci_attach() physical bus=1
Freeing (NOT implemented) redirected PCI irq 10.
	map[10]: type 1, range 32, base d0000000, size 27
	map[14]: type 1, range 32, base 0000a800, size  8
	map[18]: type 1, range 32, base ff4f0000, size 16
found->	vendor=0x1002, dev=0x5974, revid=0x00
	bus=1, slot=5, func=0
	class=[DISPLAY]03-00-00, hdrtype=0x00, mfdev=0
	subordinatebus=0 	secondarybus=0
	intpin=a, irq=5
pci1: <ATI model 5974 graphics accelerator> (vendor=0x1002, dev=0x5974) at 5.0 irq 5
pci1: <PCI bus> [attached!] on pcib1
pcib1: <PCI to PCI bridge (vendor=1002 device=5a3f)> [attached!] at device 1.0 on pci0
atapci0.pci0.pcib0.legacypci0.nexus0.root0
atapci0: <Generic PCI ATA controller> [tentative] port 0xd800-0xd80f,0xdc00-0xdc03,0xe000-0xe007,0xe400-0xe403,0xe800-0xe807 mem 0xff6ffc00-0xff6fffff irq 2 at device 18.0 on pci0
ata-: ata2 exists, using next available unit number
ata2: iobase=0xe800 altiobase=0xe402 bmaddr=0xd800
ata2: mask=03 ostat0=7f ostat2=7f
ata2-master: ATAPI 7f 7f
ata2-slave: ATAPI 7f 7f
ata2: mask=03 stat0=7f stat1=7f
ata2-master: ATA 7f 7f
ata2-slave: ATA 7f 7f
ata2: devices=00
ata2.atapci0.pci0.pcib0.legacypci0.nexus0.root0
ata2 [tentative]: at 0xe800 on atapci0
ata2 [attached!]: at 0xe800 on atapci0
ata3: iobase=0xe000 altiobase=0xdc02 bmaddr=0xd808
ata3: mask=03 ostat0=7f ostat2=7f
ata3-master: ATAPI 7f 7f
ata3-slave: ATAPI 7f 7f
ata3: mask=03 stat0=7f stat1=7f
ata3-master: ATA 7f 7f
ata3-slave: ATA 7f 7f
ata3: devices=00
ata3.atapci0.pci0.pcib0.legacypci0.nexus0.root0
ata3 [tentative]: at 0xe000 on atapci0
ata3 [attached!]: at 0xe000 on atapci0
atapci0: <Generic PCI ATA controller> [attached!] port 0xd800-0xd80f,0xdc02,0xe000-0xe007,0xe402,0xe800-0xe807 mem 0xff6ffc00-0xff6fffff irq 2 at device 18.0 on pci0
ohci0.pci0.pcib0.legacypci0.nexus0.root0
ohci0: <OHCI (generic) USB controller> [tentative] mem 0xff6fe000-0xff6fefff irq 3 at device 19.0 on pci0
usb0: OHCI version 1.0, legacy support
usb0.ohci0.pci0.pcib0.legacypci0.nexus0.root0
usb0: <OHCI (generic) USB controller> [tentative] on ohci0
usb0: USB revision 1.0
uhub0: 2 ports with 2 removable, self powered
intr 3 at 50001 > 50000 hz, livelocked limit engaged!
ums0: Microsoft Microsoft 3-Button Mouse with IntelliEye(TM), rev 1.10/3.00, addr 2, iclass 3/1
ums0: 3 buttons and Z dir.
usb0: <OHCI (generic) USB controller> [attached!] on ohci0
ohci0: <OHCI (generic) USB controller> [attached!] mem 0xff6fe000-0xff6fefff irq 3 at device 19.0 on pci0
ohci1.pci0.pcib0.legacypci0.nexus0.root0
ohci1: <OHCI (generic) USB controller> [tentative] mem 0xff6fd000-0xff6fdfff irq 5 at device 19.1 on pci0
usb1: OHCI version 1.0, legacy support
usb1.ohci1.pci0.pcib0.legacypci0.nexus0.root0
usb1: <OHCI (generic) USB controller> [tentative] on ohci1
usb1: USB revision 1.0
uhub1: 2 ports with 2 removable, self powered
usb1: <OHCI (generic) USB controller> [attached!] on ohci1
ohci1: <OHCI (generic) USB controller> [attached!] mem 0xff6fd000-0xff6fdfff irq 5 at device 19.1 on pci0
ohci2.pci0.pcib0.legacypci0.nexus0.root0
ohci2: <OHCI (generic) USB controller> [tentative] mem 0xff6fc000-0xff6fcfff irq 9 at device 19.2 on pci0
usb2: OHCI version 1.0, legacy support
usb2.ohci2.pci0.pcib0.legacypci0.nexus0.root0
usb2: <OHCI (generic) USB controller> [tentative] on ohci2
usb2: USB revision 1.0
uhub2: 2 ports with 2 removable, self powered
usb2: <OHCI (generic) USB controller> [attached!] on ohci2
ohci2: <OHCI (generic) USB controller> [attached!] mem 0xff6fc000-0xff6fcfff irq 9 at device 19.2 on pci0
ohci3.pci0.pcib0.legacypci0.nexus0.root0
ohci3: <OHCI (generic) USB controller> [tentative] mem 0xff6fb000-0xff6fbfff irq 5 at device 19.3 on pci0
usb3: OHCI version 1.0, legacy support
usb3.ohci3.pci0.pcib0.legacypci0.nexus0.root0
usb3: <OHCI (generic) USB controller> [tentative] on ohci3
usb3: USB revision 1.0
uhub3: 2 ports with 2 removable, self powered
usb3: <OHCI (generic) USB controller> [attached!] on ohci3
ohci3: <OHCI (generic) USB controller> [attached!] mem 0xff6fb000-0xff6fbfff irq 5 at device 19.3 on pci0
ohci4.pci0.pcib0.legacypci0.nexus0.root0
ohci4: <OHCI (generic) USB controller> [tentative] mem 0xff6fa000-0xff6fafff irq 9 at device 19.4 on pci0
usb4: OHCI version 1.0, legacy support
usb4.ohci4.pci0.pcib0.legacypci0.nexus0.root0
usb4: <OHCI (generic) USB controller> [tentative] on ohci4
usb4: USB revision 1.0
uhub4: 2 ports with 2 removable, self powered
usb4: <OHCI (generic) USB controller> [attached!] on ohci4
ohci4: <OHCI (generic) USB controller> [attached!] mem 0xff6fa000-0xff6fafff irq 9 at device 19.4 on pci0
pci0: <USB controller> (vendor=0x1002, dev=0x4386) at 19.5 irq 10
pci0: <unknown card> (vendor=0x1002, dev=0x4385) at 20.0
atapci1.pci0.pcib0.legacypci0.nexus0.root0
atapci1: <Generic PCI ATA controller> [tentative] port 0xff00-0xff0f,0-0x3,0-0x7,0-0x3,0-0x7 irq 3 at device 20.1 on pci0
ata0: iobase=0x01f0 altiobase=0x03f6 bmaddr=0xff00
ata0: mask=03 ostat0=50 ostat2=00
ata0-master: ATAPI 00 00
ata0-slave: ATAPI 00 00
ata0: mask=03 stat0=50 stat1=00
ata0-master: ATA 01 a5
ata0: devices=01
ata0.atapci1.pci0.pcib0.legacypci0.nexus0.root0
ata0 [tentative]: at 0x1f0 irq 14 on atapci1
ata0 [attached!]: at 0x1f0 irq 14 on atapci1
ata1: iobase=0x0170 altiobase=0x0376 bmaddr=0xff08
ata1.atapci1.pci0.pcib0.legacypci0.nexus0.root0
ata1 [tentative]: at 0x170 irq 15 on atapci1
ata1 [attached!]: at 0x170 irq 15 on atapci1
atapci1: <Generic PCI ATA controller> [attached!] port 0xff00-0xff0f,0-0x3,0-0x7,0-0x3,0-0x7 irq 3 at device 20.1 on pci0
pci0: <unknown card> (vendor=0x1002, dev=0x4383) at 20.2 irq 3
isab0.pci0.pcib0.legacypci0.nexus0.root0
isab0: <PCI to ISA bridge (vendor=1002 device=438d)> [tentative] at device 20.3 on pci0
isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
isa0: <ISA bus> [tentative] on isab0
isa0: <ISA bus> [attached!] on isab0
isab0: <PCI to ISA bridge (vendor=1002 device=438d)> [attached!] at device 20.3 on pci0
pcib2.pci0.pcib0.legacypci0.nexus0.root0
pcib2: <PCI to PCI bridge (vendor=1002 device=4384)> [tentative] at device 20.4 on pci0
pcib2:   secondary bus     2
pcib2:   subordinate bus   2
pcib2:   I/O decode        0xb000-0xbfff
pcib2:   memory decode     0xff500000-0xff5fffff
pcib2:   prefetched decode 0xfff00000-0xfffff
pcib2:   Subtractively decoded bridge.
pci2.pcib2.pci0.pcib0.legacypci0.nexus0.root0
pci2: <PCI bus> [tentative] on pcib2
pci2: pci_attach() physical bus=2
IOAPIC #0 intpin 21 -> irq 11
Freeing (NOT implemented) redirected PCI irq 9.
	map[10]: type 1, range 32, base 0000b800, size  8
	map[14]: type 1, range 32, base ff5ff400, size  8
found->	vendor=0x10ec, dev=0x8167, revid=0x10
	bus=2, slot=6, func=0
	class=[NETWORK]02-00-00, hdrtype=0x00, mfdev=0
	subordinatebus=0 	secondarybus=0
	intpin=a, irq=11
pcib2: device re0 requested decoded I/O range 0xb800-0xb8ff
re0.pci2.pcib2.pci0.pcib0.legacypci0.nexus0.root0
re0: <RealTek 8169SC/8110SC Single-chip Gigabit Ethernet> [tentative] port 0xb800-0xb8ff mem 0xff5ff400-0xff5ff4ff irq 11 at device 6.0 on pci2
pcib2: device re0 requested decoded I/O range 0xb800-0xb8ff
miibus0.re0.pci2.pcib2.pci0.pcib0.legacypci0.nexus0.root0
miibus0: <MII bus> [tentative] on re0
rgephy0: rev: 2
rgephy0.miibus0.re0.pci2.pcib2.pci0.pcib0.legacypci0.nexus0.root0
rgephy0: <RTL8169S/8110S media interface> [tentative] on miibus0
rgephy0:  10baseT, 10baseT-FDX, 100baseTX, 100baseTX-FDX, 1000baseT, 1000baseT-FDX, auto
rgephy0: <RTL8169S/8110S media interface> [attached!] on miibus0
miibus0: <MII bus> [attached!] on re0
re0: bpf attached
re0: MAC address: 00:19:db:2a:83:04
re0: <RealTek 8169SC/8110SC Single-chip Gigabit Ethernet> [attached!] port 0xb800-0xb8ff mem 0xff5ff400-0xff5ff4ff irq 11 at device 6.0 on pci2
pci2: <PCI bus> [attached!] on pcib2
pcib2: <PCI to PCI bridge (vendor=1002 device=4384)> [attached!] at device 20.4 on pci0
pci0: <PCI bus> [attached!] on pcib0
pcib0: <Host to PCI bridge> [attached!] on legacypci0
legacypci0 [attached!] on motherboard
ex_isa_identify()
ata-: ata0 exists, using next available unit number
ata-: ata1 exists, using next available unit number
Trying Read_Port at 203
Trying Read_Port at 243
Trying Read_Port at 283
Trying Read_Port at 2c3
Trying Read_Port at 303
Trying Read_Port at 343
Trying Read_Port at 383
Trying Read_Port at 3c3
isa_probe_children: disabling PnP devices
isa_probe_children: probing non-PnP devices
orm0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
orm0: <Option ROM> [tentative] at iomem 0xc0000-0xcefff on isa0
orm0: <Option ROM> [attached!] at iomem 0xc0000-0xcefff on isa0
pmtimer0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
pmtimer0 [tentative] on isa0
pmtimer0 [attached!] on isa0
fdc0: ready for input in output
fdc0: cmd 3 failed at out byte 1 of 3
fdc0 [tentative] failed to probe at port 0x3f0-0x3f5,0x3f7 irq 6 drq 2 on isa0
ata4 [tentative] failed to probe at port 0x1f0 irq 14 on isa0
ata5 [tentative] failed to probe at port 0x170 irq 15 on isa0
adv0 [tentative] failed to probe on isa0
bt0: Failed Status Reg Test - ff
bt_isa_probe: Probe failed at 0x330
bt0: Failed Status Reg Test - ff
bt_isa_probe: Probe failed at 0x334
bt0: Failed Status Reg Test - ff
bt_isa_probe: Probe failed at 0x230
bt0: Failed Status Reg Test - ff
bt_isa_probe: Probe failed at 0x234
bt0: Failed Status Reg Test - ff
bt_isa_probe: Probe failed at 0x130
bt0: Failed Status Reg Test - ff
bt_isa_probe: Probe failed at 0x134
bt0 [tentative] failed to probe at port 0x134-0x137 on isa0
aha0: status reg test failed ff
aha0: status reg test failed ff
aha0: status reg test failed ff
aha0: status reg test failed ff
aha0: status reg test failed ff
aha0: status reg test failed ff
aha0 [tentative] failed to probe at port 0x134-0x137 on isa0
aic0 [tentative] failed to probe at port 0x140-0x15f on isa0
atkbdc0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
atkbdc0: <Keyboard controller (i8042)> [tentative] at port 0x60,0x64 on isa0
atkbd0.atkbdc0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
atkbd0: <AT Keyboard> [tentative] flags 0x1 irq 1 on atkbdc0
atkbd: the current kbd controller command byte 0065
atkbd: keyboard ID 0x41ab (2)
kbd0 at atkbd0
kbd0: atkbd0, AT 101/102 (2), config:0x1, flags:0x3d0000
atkbd0: <AT Keyboard> [attached!] flags 0x1 irq 1 on atkbdc0
psm0: current command byte:0065
psm0: failed to reset the aux device.
atkbdc0: <Keyboard controller (i8042)> [attached!] at port 0x60,0x64 on isa0
vga0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
vga0: <Generic ISA VGA> [tentative] at port 0x3c0-0x3df iomem 0xa0000-0xbffff on isa0
fb0: vga0, vga, type:VGA (5), flags:0x7007f
fb0: port:0x3c0-0x3df, crtc:0x3d4, mem:0xa0000 0x20000
fb0: init mode:24, bios mode:3, current mode:24
fb0: window:0xc00b8000 size:32k gran:32k, buf:0 size:32k
VGA parameters upon power-up
50 18 10 00 00 00 03 00 02 67 5f 4f 50 82 55 81 
bf 1f 00 4f 0d 0e 00 00 07 80 9c 8e 8f 28 1f 96 
b9 a3 ff 00 01 02 03 04 05 14 07 38 39 3a 3b 3c 
3d 3e 3f 0c 00 0f 08 00 00 00 00 00 10 0e 00 ff 
VGA parameters in BIOS for mode 24
50 18 10 00 10 00 03 00 02 67 5f 4f 50 82 55 81 
bf 1f 00 4f 0d 0e 00 00 00 00 9c 8e 8f 28 1f 96 
b9 a3 ff 00 01 02 03 04 05 14 07 38 39 3a 3b 3c 
3d 3e 3f 0c 00 0f 08 00 00 00 00 00 10 0e 00 ff 
EGA/VGA parameters to be used for mode 24
50 18 10 00 10 00 03 00 02 67 5f 4f 50 82 55 81 
bf 1f 00 4f 0d 0e 00 00 00 00 9c 8e 8f 28 1f 96 
b9 a3 ff 00 01 02 03 04 05 14 07 38 39 3a 3b 3c 
3d 3e 3f 0c 00 0f 08 00 00 00 00 00 10 0e 00 ff 
vga0: <Generic ISA VGA> [attached!] at port 0x3c0-0x3df iomem 0xa0000-0xbffff on isa0
sc0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
sc0: <System console> [tentative] at flags 0x100 on isa0
sc0: VGA <16 virtual consoles, flags=0x300>
sc0: fb0, kbd0, terminal emulator: sc (syscons terminal)
sc0: <System console> [attached!] at flags 0x100 on isa0
sio0: irq maps: 0x3 0x13 0x3 0x3
sio0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
sio0 [tentative] at port 0x3f8-0x3ff irq 4 flags 0x10 on isa0
sio0: type 16550A
sio0 [attached!] at port 0x3f8-0x3ff irq 4 flags 0x10 on isa0
sio1: can't drain, serial port might not exist, disabling
sio1 [tentative] failed to probe at port 0x2f8-0x2ff irq 3 on isa0
sio2: not probed (disabled)
sio3: not probed (disabled)
ppc0: parallel port found at 0x378
ppc0: using extended I/O port range
ppc0: SPP
ppc0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
ppc0: <Parallel port> [tentative] at port 0x378-0x37f irq 7 on isa0
ppc0: Generic chipset (NIBBLE-only) in COMPATIBLE mode
ppbus0.ppc0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
ppbus0: <Parallel port bus> [tentative] on ppc0
plip0.ppbus0.ppc0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
plip0: <PLIP network interface> [tentative] on ppbus0
lp0: bpf attached
plip0: <PLIP network interface> [attached!] on ppbus0
lpt0.ppbus0.ppc0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
lpt0: <Printer> [tentative] on ppbus0
lpt0: Interrupt-driven port
lpt0: <Printer> [attached!] on ppbus0
ppi0.ppbus0.ppc0.isa0.isab0.pci0.pcib0.legacypci0.nexus0.root0
ppi0: <Parallel I/O> [tentative] on ppbus0
ppi0: <Parallel I/O> [attached!] on ppbus0
ppbus0: <Parallel port bus> [attached!] on ppc0
ppc0: <Parallel port> [attached!] at port 0x378-0x37f irq 7 on isa0
ed0: not probed (disabled)
fe0: not probed (disabled)
ie0: not probed (disabled)
lnc0: not probed (disabled)
cs0: not probed (disabled)
sn0: not probed (disabled)
isa_probe_children: probing PnP devices
SMP: enabled INTs: 1, 2, 4, 5, 7, 9, 11, 14, 15, apic_imen: 0x00ff3549
BIOS Geometries:
 0:03ff0f3f 0..1023=1024 cylinders, 0..15=16 heads, 1..63=63 sectors
 0 accounted for
Device configuration finished.
APIC_IO: Testing 8254 interrupt delivery
APIC_IO: routing 8254 via IOAPIC #0 intpin 2
Finish MP startup
SMP: AP CPU #1 Launched!
SMP: CPU1 apic_initialize():
     lint0: 0x00010000 lint1: 0x00010400 TPR: 0x00000000 SVR: 0x000001ff
Active CPU Mask: 00000003
start scheduler helpers on cpus: 0 1
start dummy scheduler helpers on cpus: 0 1
crypto: assign driver 0, flags 2
crypto: driver 0 registers alg 1 flags 0 maxoplen 0
crypto: driver 0 registers alg 2 flags 0 maxoplen 0
crypto: driver 0 registers alg 3 flags 0 maxoplen 0
crypto: driver 0 registers alg 4 flags 0 maxoplen 0
crypto: driver 0 registers alg 5 flags 0 maxoplen 0
crypto: driver 0 registers alg 17 flags 0 maxoplen 0
crypto: driver 0 registers alg 6 flags 0 maxoplen 0
crypto: driver 0 registers alg 7 flags 0 maxoplen 0
crypto: driver 0 registers alg 15 flags 0 maxoplen 0
crypto: driver 0 registers alg 8 flags 0 maxoplen 0
crypto: driver 0 registers alg 16 flags 0 maxoplen 0
crypto: driver 0 registers alg 9 flags 0 maxoplen 0
crypto: driver 0 registers alg 10 flags 0 maxoplen 0
crypto: driver 0 registers alg 13 flags 0 maxoplen 0
crypto: driver 0 registers alg 14 flags 0 maxoplen 0
crypto: driver 0 registers alg 11 flags 0 maxoplen 0
crypto: driver 0 registers alg 18 flags 0 maxoplen 0
sl0: bpf attached
faith0: bpf attached
lo0: bpf attached
ppp0: bpf attached
Warning: ACPI idle hook not yet supported for SMP
ar: FreeBSD check1 failed
ad0: <WDC WD1600JB-98GVA0/08.02D08> ATA-6 disk at ata0-master
ad0: 152627MB (312581808 sectors), 310101 C, 16 H, 63 S, 512 B
ad0: 16 secs/int, 1 depth queue, BIOSDMA
ad0: piomode=4 dmamode=2 udmamode=5 cblid=1
bootdev: a0200000 type=0 unit=0 slice=2 part=0 major=3
Mounting root from ufs:/dev/ad0s1a
ad0s1: type 0xa5, start 63, end = 312581807, size 312581745 : OK
WARNING:  was not properly dismounted
start_init: trying /sbin/init
intr 3 at 7376 < 20000 hz, livelock removed
